uEFI System Update Package (SUP) Installation and Operation Instructions

Intel highly recommends reading this document in its entirety before performing
the system update. Verifying that your system meets the documented requirments 
will ensure a successful update and provide the most reliable system 
functionalityafter the update has completed.

 
Released - December 16 2020

********************************************************************************
This update package includes the following production level system software 
updates:

   System BIOS  - 02.01.0013
   ME Firmware  - 04.01.04.423
   BMC Firmware - 2.48.ce3e3bd2
   FRUSDR       - 2.01
   Intel® Optane™ DC Persistent Memory Firmware (DCPMM) - 01.02.00.5444  

--- Firmware Update Tools ---

  iFlash32_V14_1_Build15
  FWPIAUPD_v14_1_Build19
  FRUSDR_V14_1_Build17
  
--- Supported Products ---

Intel(R) Server Board S2600WF Family
Intel(R) Server System R1000WF Family
Intel(R) Server System R2000WF Family

*************************************************************************************
				IMPORTANT NOTES
*************************************************************************************

*** Please Check your IPMI through LAN commands ***

Starting from BMC 2.22.59c3b83a, when KCS Policy Control Mode is configured as "Deny ALL" on BMC EWS, BMC and FRUSDR cannot be upgraded/downgraded as expected behavior. Updates can still be performed via Redfish or BMC EWS

This SUP package includes the FW 01.02.00.5417 for Intel® Optane™ DC Persistent Memory (DCPMM), if you received your DCPMM DIMMs with a different FW, please install this one following the general installation procedure below. 

Extra parameter for ipmitool through LAN is required since BMC firmware 1.90 as the Cipher Suite 3 is disabled and only keep Cipher Suite 17 opened by default, the “-C 17” is a must when using ipmitool to access BMC LAN. 
The Cipher Suite 17 was first introduced in ipmitool 1.8.18 on Oct 8th 2016, you have to update ipmitool to this version or newer one, earlier versions of ipmitool don’t have Cipher 17 support.
ipmitool is not working well when running in high load network. We recommend to add extra timeout by using “-N 5”. Default is 1 second for RMCP+, which is not enough. –N 5 will set 5 second as timeout, 
So the command will look like:
ipmitool –I lanplus –H ip –U user –P password –C 17 –N 5 command

Please refer to the included "TA-1143_Extra_parameters_needed_for_ipmitool.pdf" for more information.

Downgrading BMC below 1.43.660a4315 is not supported due to a security revision change.

WARNING: This release has the BMC PCIe bridge disabled. This will cause the 
    majority of operating systems to fail at boot as they stall during video 
    driver initialization
    
    Steps to recover a failing operating system:
    
	Linux variants (one of the below):
        A. Ensure the "modprobe.blacklist=ast" parameter is set in your boot loader (grub)
        B. Ensure you are using a kernel version v4.10 or newer
    For Red Hat* Enterprise Linux* v7.3, please refer to the included "RHEL73_InstallationGuide_Rev1.00.pdf"
	For SUSE* Linux* Enterprise Server v12 SP1 or SP2, please refer to the included "SLES12_InstallationGuide_Rev1.00.pdf"
	
    Windows variants:
        Boot to safe mode, and load aspeed video driver v1.03 or greater and reboot
	For Windows* Server 2016, please refer to the included "WinSrv16_InstallationGuide_Rev1.00.pdf"

*** Advisory Note ***

	Do not modify any of the script files. The scripts as written will provide 
	the most reliable update experience

	To run these updates, you must boot the system to the embedded uEFI shell

	If for any reason the System BIOS, BMC Firmware, or FRUSDR data need to be 
	re-installed after the initial update has been performed, the package does 
	include standalone script files that can be run individually. These files 
	are: UpdBIOS.nsh, UpdMe.nsh, UpdFD.nsh, fwUpdateBMC.nsh, and UpdS2600WFTFRUSDR.nsh

	We recommend to use these files after the system has been updated 
	initially using the Startup.nsh file                                                                           

	When booting the system for the first time after a firmware update is complete,
	it may automatically reboot several times, this is an expected behavior

*************************************************************************************
                       SYSTEM HARDWARE and FIRMWARE REQUIREMENTS
*************************************************************************************
To update the system firmware stack to the versions included in this update package,
the currently loaded system firmware stack on the system must meet the following:
  
  System BIOS  - 02.01.0012 or later
  ME Firmware  - 04.01.04.381 or later
  BMC Firmware - 2.48.89b32e0d or later
  FRUSDR       - 2.00 or later 
    
  
If the system doesn't currently meet the above system firmware requirements,
you must download a previously-posted System Update Package (SUP) and update
the system to the preceding described firmware revisions before updating the
system to the firmware stack included in this package.

********************************************************************************
                            GENERAL INSTALLATION PROCEDURE
********************************************************************************

1. Unzip the contents of the update package and copy all files to the root directory 
of a removable media (USB flash drive)
2. Insert the USB flash drive to any available USB port on the system to be updated
3. Power on the server and load the uEFI shell
4. Access to the USB flash drive insterted and begin the update process running the Startup.nsh
5. Systen will reboot automatically after the update process has successfully completed
6. If DCPMM installed, run Startup.nsh a second time after the first reboot to upgrade DCPMM Firmware and power cycle 
the system to allow DCPMM load the new FW. 

********************************************************************************

Whenever the system BIOS is updated, two BIOS images are installed, a primary 
image and a backup image. The backup image is loaded during the 1st system reboot
after the primary BIOS image is updated. During the 1st system reboot, the
screen will be black for approximately 2 minutes while the backup BIOS image 
is being loaded. DO NOT power off or reboot the system during this time. 
A message will appear on the screen when the backup BIOS image update has 
completed.

Verifying Updates:

01. After the final update has completed successfully, reboot the system
02. During POST, hit the <F2> Key when prompted to access the BIOS Setup Utility
03. From the BIOS Setup Utility main menu, hit the <F9> key to load BIOS defaults
04. Hit the <F10> key to Save Changes and Exit the BIOS defaults
04. At the main menu verify the BIOS revision is correct
05. Move cursor to the SERVER MANAGEMENT menu and hit Enter
06. Move cursor to the SYSTEM INFORMATION Option and hit Enter
07. Verify the BMC Firmware revision is correct
08. Verify the SDR revision is correct
09. Verify the ME Firmware revision is correct
10. Configure desired BIOS Option settings
11. Hit the F10 Key to Save Changes and Exit


The System Software Update is Complete.

***   Warning:  *** 
!! Do NOT interrupt or reboot or remove power from your system during the update process !!
!! Doing so may render your system inoperable !!

!! Do NOT attempt to downgrade the system software once loaded on the system !!

Please refer to the respective "Release Notes" files for complete list of known issues, workarounds and detailed requirements: 

- BIOS: Release Notes BIOS R####.txt
- BMC: Release Notes BMC ####.txt
- FRUSDR: Release Notes FRUSDR ####.txt
