version=2
999989251,0,STATUS,nlog.c,"Some NLOG messages are stored in SPI. Remove these to speed up fatal condition(s) handling"
999666314,0,WARNING,dfx.c,"Module ID specified in input payload ""does not match module ID that was uploaded"
999584907,2,ERROR,sxp_trims.c,"0x63F register read failed. Can't check media type on Rank: %d, Die: %d"
99904649,0,ERROR,commands.c,"Cmd Format Device, failed to flush fw state with life time statistic."
998526148,9,ERROR,media_manager_engine.c,"BlockMoveIndex %d Src.DPA 0x%08X_0x%08X Src.PDA 0x%08X_0x%08X Src.RO %d Dest.PDA 0x%08X_0x%08X Dest.RO %d"
997465026,1,ERROR,short_stroke.c,"Short Stroke Size %d is not a power of 2"
994542473,0,ERROR,command_inject_error.c,"Disabling poison on 4 cache lines"
994421226,0,ERROR,kechika_river_pmic_driver.c,"Failed to set VCCDDRD_DDRT PMIC rail (D) to fused VID code."
99354806,1,DEBUG,checkpoint.c,"Update DIMM Refreshed: %d"
992883149,2,STATUS,fw_activate.c,"Staged FW Api (0x%04x) is lower than the current API Hanshake (0x%04x)."
992360116,0,ERROR,key_management.c,"Security key initialization failed!"
991182921,1,ERROR,adaptive_vdm.c,"AVDM_GetVdmDimmData requested for Invalid VDM : %d"
990913071,8,ERROR,dpa_verify_error_handler.c,"Address Verify Error. DPA 0x%08X_0x%08X PDA 0x%08X_0x%08X FaultData 0x%08X_0x%08X_0x%08X STYPE 0x%02X"
990657921,1,ERROR,update_vsm_resume_sxp_io_traffic.c,"PCSCLR_CFG1: 0x%x"
990097720,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaWrScrambleSeedSel: 0x%x"
98889407,0,STATUS,command_inject_error.c,"Error Injection is enabled"
987025096,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz0: 0x%x"
986644423,1,ERROR,get_media_statistics.c,"Couldn't enable SxpTestMode on Rank: %d"
985124851,0,DEBUG,command_features.c,"Get Admin Features: DDRT IO Init Info"
984919720,0,INFO,dram_patrol_scrub.c,"DRAM patrol scrub started"
983311348,0,ERROR,write_disturb_engine.c,"WriteDisturbEngine_PollStartBit reached time limit"
979841458,2,INFO,task_command_handler.c,"Command Completed on mb[%d] with Status: 0x%08x"
979224458,0,STATUS,thermal_manager.c,"Exiting thermal throttling"
978121527,2,ERROR,log_image_sync_complete.c,"Image sync has been completed at stage: %d, image chunk: %d"
977532808,0,ERROR,fw_img_auth.c,"Computed and derived hash do not match"
974050824,1,ERROR,core_dump.c,"FwDebugData - nlogSpiBackupValid : %d"
969806146,0,ERROR,wear_level_move.c,"Free Block Expansion operation has fatally failed, request has been dropped!"
968860029,0,WARNING,command_inject_error.c,"Mailbox device error, handle was null"
968742982,1,ERROR,task_media_interface.c,"SRAM error at AHB index %d!"
968599101,0,DEBUG,platform_config_data.c,"Set Partition Over DDRT"
967888659,0,ERROR,sxp_rmt_tests.c,"RAS Rx Dqs Min Mask Test Failed"
966846204,2,ERROR,core_wear_level_move.c,"AitPolled_Write Failed on Backup Entry Address 0x%08X_0x%08X: "
966137287,1,ERROR,wear_level_move.c,"WLM BM aborted entered without BM abort status:%x"
965853894,1,ERROR,task_media_interface.c,"DMA command %x failed, PSN or SXP error"
965396199,0,ERROR,fw_upd_halt_at_header_auth.c,"FwUpdate has been halted at header"
964296866,0,WARNING,power_state.c,"Listener already present."
963998151,2,WARNING,chn_no_cmd.c,"AIT read failed; data for DPA 0x%08X_%08X stuck in WDB"
962374793,0,WARNING,task_security.c,"Unable to Erase Unit: Encryption Disabled"
960749958,0,ERROR,task_error_handler.c,"AIT Scrub fails at COPY_LINE state"
958641296,2,ERROR,sxp_trims.c,"Unrecognized S15 media on Rank: %d, Die: %d"
958402751,5,ERROR,ddrt_scheduler.c,"ERROR: DDRT PLL did not lock before timeout MSC_FNVIO_INIT_CONTROL_0=0x%X, DDRT_RESET_STATUS=0x%X, D_DDRT_DCLK_CTRL=0x%X, MSC_FNVIO_VISIBILITY_CSR=0x%X, MSC_PLL_CTRL=0x%X"
957790637,1,DEBUG,wear_level_move.c,"Transition FBE State Machine : %d"
957678542,0,ERROR,core_dump.c,"PowerLossLog:"
952201341,4,ERROR,command_fw_update.c,"Unexpected timestamp from the future. Uptime: 0x%08x_%08x Timestamp saved: 0x%08x_%08x"
948785612,0,DEBUG,buffers.c,"Queue not empty, preparing to dequeue."
948072682,0,WARNING,address_scrub.c,"Address Range Scrub Error Found"
947913700,0,ERROR,mm_free_block_expansion.c,"All reads of AIT line copies failed. Going DIMM fatal."
94527533,3,ERROR,sxp_scheduler.c,"read SXP_REG_ADDR_MSR_11 failed! value = 0x%x, die = %d, rank = %d \n"
944450542,2,ERROR,die_error_emulator.c,"DieErrorEmulator: SxpCmd_SelectId failed on rank : %d, sxpDie : %d"
94252252,2,ERROR,sxp_init.c,"Write DQ-DQS Training failed, Rank: %d Training type: %d"
941964797,0,DEBUG,command_inject_error.c,"Clear poison DPA out of mapped range."
940153312,0,INFO,security_interface.c,"Security_CompleteRequestWithEvent completed...Event generated"
939773689,0,DEBUG,command_features.c,"Get Admin Features: Latch System Shutdown"
938129283,0,WARNING,command_fw_update.c,"Cannot update FW because FW Update already occurred"
937538193,2,ERROR,datastore.c,"Incorrect source datastore. Expected: %x, Found: %x"
934478773,1,ERROR,ltec.c,"LTEC failed to apply VID code updates after %d attempts."
933290999,0,WARNING,command_features.c,"Command not permitted after Config Lockdown"
932900955,1,ERROR,wear_level_move.c,"Free Block Expansion: Relocate Block reported an error %d on move operation"
930260448,0,INFO,ait_dram.c,"DRAM Loading succeeds."
929951974,0,DEBUG,command_features.c,"SS: Disable Security"
929706612,0,ERROR,cpgc.c,"Channel not specified for DDR-T2 ACIOLB"
929561049,1,ERROR,get_ait_info.c,"A_AIT_TOP_BASE_ADDR_H: 0x%x"
927375841,0,ERROR,ltec.c,"LTEC requested to transition from idle mode to normal mode outside of S3 resume path."
925541910,1,ERROR,log_power_event_start.c,"DRDP_WCRD_CONFIG: 0x%x"
924587943,2,ERROR,sxp_init.c,"Sxp_AdvancedTxDqsTraining failed rank: %d Training type: %d"
923627305,0,ERROR,authenticate_spi_region.c,"SPI read Failure during SPI region authentication!"
923428613,1,DEBUG,task_command_handler.c,"Event Flag: 0x%08X"
92194313,0,DEBUG,command_features.c,"Get Features: Package Sparing Policy"
92169212,3,STATUS,command_features.c,"Config Lockdown Executed on DDRT training failure: MSC_PLL_CTRL=0x%X | Current BSR: 0x%08x_%08x"
920592712,1,WARNING,fconfig.c,"Fconfig_SetConfig token cannot be changed Token: 0x%X"
917584305,2,ERROR,core_wear_level_move.c,"AitPolled_WriteReverseMap Failed on Backup Entry Address 0x%08X_0x%08X: "
917064956,1,ERROR,sxp_rcven_training.c,"CoarseRcvenTraining failed rank index[%d]"
916768115,0,WARNING,command_features.c,"Training already has been completed"
913396665,0,DEBUG,command_features.c,"Get Admin Features: FW Load Flag"
912077438,0,INFO,smart.c,"Updating vendor page with Intel details"
911801626,0,ERROR,get_media_statistics.c,"Unknown stat requested"
910925161,0,INFO,ait_dram.c,"DRAM Load already completed! No need to resume!"
907029371,0,WARNING,ait_update.c,"MediaInterface returned Null Handle."
906406608,1,ERROR,nlog_set_ddrt_io_init_info.c,"DA_DDRT_PLL_CTRL: 0x%x"
905478210,0,ERROR,command_software_triggers.c,"Disabled package sparing software trigger"
904144744,0,ERROR,spi_logger.c,"Failed to erase SPI Debug region. Disabling SPI Debug logs"
903487630,4,ERROR,sxp_wr_dqs_training.c,"Adv_TxDqDqs failed margin check R[%d] B[%d]: R[%d] F[%d]"
902284729,0,DEBUG,command_features.c,"PCD Get Partition Size Called"
901033166,0,INFO,zqcal_periodic.c,"Periodic Init"
8966527,1,ERROR,log_ddrt_dll_csr.c,"MSC_FNVIO_DDRTDLL_CSR: 0x%x"
896155660,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr5: 0x%x"
895881881,0,INFO,refresh.c,"Resuming Refresh"
894014943,1,ERROR,hal_pmic_rail.c,"Invalid rail 0x%x requested."
893922849,2,ERROR,ltec.c,"LTEC Mode 0x%X Rail State 0x%08X"
893381250,2,ERROR,write_count_histogram.c,"Received more than expected steps for data retrieval. Number of steps: expected = %d, actual = %d"
892765282,0,WARNING,command_features.c,"Address Range Scrub: Invalid Enable"
88875809,2,ERROR,message_channel.c,"Message channel read data invalid! ctrl = 0x%08X, status = 0x%08X"
887636454,0,WARNING,command_features.c,"SS: Invalid SubOpcode"
886119997,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustIRst at Window. Window : %d"
886088031,0,INFO,fw_img_auth.c,"Calculating hash on fw image"
886072631,3,ERROR,update_firmware.c,"Unexpected FW Update status transition: current_status = %d - last event = %d - next event = %d"
88533214,1,DEBUG,wear_level_move.c,"WLM transition State Machine : %d"
884753734,0,WARNING,task_media_interface.c,"DMA timed out; aborting!"
88441664,1,ERROR,nlog_set_ddrt_io_init_info.c,"D_FW_STATUS_H: 0x%x"
884377546,0,ERROR,thermal_manager.c,"Temperature polling disabled"
884177118,0,ERROR,fw_init.c,"WDB was not flushed on the previous boot cycle (WRITE_DATA_FLUSH_COMPLETE=0)"
883860734,2,ERROR,short_stroke.c,"Short Stroke size %d is invalid. It must be at least %d when Short Stroke FW mode is set"
882827298,0,INFO,ddrt_sense_amp_calibration.c,"Training Complete.  Channel reset"
881633287,1,ERROR,media_manager_engine.c,"WLM Threshold value (%d) is invalid in SetQueuePolicy during MediaManagerInit"
87813280,0,ERROR,vdm.c,"Vdm_AdjustVdm called with unsupported VDM!"
877407022,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD2: 0x%x"
877136979,0,ERROR,write_count_histogram.c,"Start address > DIMM capacity"
876537416,0,ERROR,ait_dram.c,"DRAM Loading timed out."
876071125,2,DEBUG,dpa_for_pda.c,"0x%08X: block DPA is 0x%08X"
875538856,3,INFO,error_logging.c,"Start Address for Log %d : 0x%08X_%08X"
87472397,0,ERROR,kechika_river_pmic_driver.c,"Cap Self test did not complete"
874027919,0,WARNING,debug_log_data.c,"Failed to get handle from Media Interface"
873322763,0,ERROR,sxp_init.c,"ZQCalLongInit failed"
872776566,0,ERROR,command_fw_update.c,"Updated firmware failed a verification test"
872724684,1,WARNING,fconfig.c,"Fconfig_SetConfig unknown token Token: 0x%X"
872720053,0,ERROR,log_zqcal_short.c,"Polled flush of Nlog buffer to media has occurred."
87211441,0,ERROR,media_manager_engine.c,"MediaManagerEngine_PollStartBit has failed. Start Bit has failed to de-assert!"
87076367,0,ERROR,fw_init.c,"Setting media disabled after FwState load - due to FSD failure"
870538048,0,DEBUG,command_features.c,"SS: Disable Security"
870499428,0,WARNING,security_interface.c,"SET_S3_KEY security request timed out"
870343891,0,DEBUG,platform_config_data.c,"DMA transfer complete"
867979267,0,WARNING,sxp_commands.c,"ZQCal Short REQ bit still set after delay!"
867889000,1,ERROR,power_budgeting_engine.c,"Failed to abort EM. EM reset status = 0x%x"
867461530,1,ERROR,nlog_notify_ddrt_normal_mode.c,"PCSCLR_CFG6: 0x%x"
866148490,1,ERROR,power_budgeting_engine.c,"Wrong Coulomb count CSR address offset has been programmed in Energy Meter. em_status = 0x%x"
864681814,1,ERROR,command_fw_update.c,"Error requesting SPI block erase at address 0x%X during FW Update"
864572670,0,ERROR,wear_level_move.c,"Wear Level Move operation has fatally failed, request has been dropped!"
863535383,1,ERROR,sxp_scheduler.c,"Unsupported SXP Device Device ID read error. DeviceId = 0x%X"
862990921,1,ERROR,log_emask_imask_regs.c,"DN_EMASK: 0x%x"
862515713,0,INFO,command_log.c,"Get Memory Info"
862010394,0,DEBUG,wear_level_move.c,"Wear Level Move No Spare Blocks!"
859911725,1,ERROR,sxp_commands.c,"Unexpected FGPK SXP Trim Reg Read Latency value of 0x%X."
859437445,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr4: 0x%x"
85812145,3,ERROR,core_dump.c," - Header -> WriteCounter: %d | Version: %d | isCorrupt: %d"
857532098,0,INFO,task_security.c,"Task_security processed Security_GetSecurityRequest"
855490998,0,INFO,fw_img_auth.c,"Verifying decrypted hash"
853336130,1,ERROR,data_path_error.c,"PC ERR STS FIFO U/O Flow Errors: 0x%08X"
851602737,1,DEBUG,ras.c,"clearing 0x%08X in pw_ras_interrupt_req"
850038082,5,ERROR,core_dump.c,"MbType: %d, CommandReg: 0x%08x_%08x, StatusReg: 0x%08x, Abort: 0x%08x"
849319795,2,DEBUG,refresh.c,"Resuming Migration at Address 0x%08x for failing Die %d "
846541577,1,ERROR,log_power_event_end.c,"DRDP_WCRD_CONFIG: 0x%x"
845696900,4,DEBUG,algo_tx_dq_dqs_training.c,"Advanced_TxDq Rising_Mid_Falling %d: %d_%d_%d"
845377954,1,DEBUG,ait_dram.c,"AIT DRAM Read Error detected: 0x%08X"
84537540,4,DEBUG,command_log.c,"-> version: %d. %d. %d. %d."
845212987,2,ERROR,context_block.c,"Context Block header is detected at offset: 0x%08x for copy %d."
843966412,1,ERROR,io_csr.c,"IO CSR invalid parameter byte = 0x%x"
843812649,0,ERROR,log_prefetch_cache_invalidate.c,"PCHE_INV_ALLSETS bit in D_DDRT_TRAINING_OTHER_EN register was set!"
843487571,0,ERROR,sxp_init.c,"Sxp_RestoreSxpIoRegisters failed"
843005833,0,INFO,core_dump.c,"Using checksum instead of SHA - csrDumpListTable"
842453199,0,STATUS,fw_activate.c,"Viral state detected."
842303897,1,ERROR,context_block.c,"Failed to retrieve any valid CB copy with error opcode: 0x%x - going to partial read."
841111372,0,WARNING,address_scrub.c,"Error limit reached. Aborting Address Range Scrub"
839843177,0,ERROR,chn_no_cmd.c,"channel no command error queue overflow!"
83839594,3,ERROR,update_firmware.c,"Flash write of block %d of image failed. State: %d. Substate: %d"
837791618,0,DEBUG,task_security.c,"SECURITY_FREEZE_LOCK"
837512637,1,ERROR,core_dump.c,"FwDebugData - numAsserts    : %d"
83699859,3,ERROR,sxp_trim_bundle.c,"Could not populate HnlwlSelv RD%d value 0x%02x in register S2X_REG_ADDR_TMR_HNLWLSELV (0x%04x)"
835380536,2,ERROR,sxp_wr_dqs_training.c,"Adv_TxDqDqs failed rank[%d] byte[%d]"
835152349,1,ERROR,partition_manager.c,"Unexpected number of mb %d payload unlock requests."
834329397,1,ERROR,data_path_error.c,"DA FIFO U/O Flow Errors: 0x%08X"
83346157,0,ERROR,kechika_river_pmic_driver.c,"Couldn't read the current rail settings, skipping PMIC Rail Init"
8327795,1,ERROR,sxp_scheduler.c,"Invalid rank count %d. Not assigning the internal address offsets."
832548761,0,ERROR,kechika_river_pmic_driver.c,"Unable to disable power on reset due to null pointer"
832174745,2,ERROR,power.c,"config empty or wdb ddrt empty check timeout - D_DDRT_FUNC_STS = 0x%X, RPQ_WDB_STAT_EMPTY = 0x%X"
829965357,1,ERROR,power_budgeting_engine.c,"Energy meter 12V Coulomb count overflows. em_status = 0x%x"
829153067,4,ERROR,core_dump.c," Log Entry[%d] -> Checkpoint [0x%x] ErrorCode [%d] Timestamp [%d]"
829125042,2,ERROR,spi_flash_driver.c,"Flash operation timed out. Operation: %d, target: 0x%08X"
828956165,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz1: 0x%x"
828229931,2,ERROR,power_budgeting_engine.c,"12V Power sample [%d mW] has exceeded high watermark threshold [%d mW]"
825943307,1,ERROR,host_interrupt.c,"HostInterrupt Abort in flight Host Interrupt of type = %d"
825760757,1,ERROR,power_event_at_image_sync.c,"Picked up random image chunk: %d"
82574135,2,ERROR,reg_flow.c,"PCR update bit is not being cleared (ddrt_update_pcr = %d, i3c_update_pcr = %d"
824909148,1,WARNING,fw_image_sync.c,"Hash of body of block %d failed"
821754296,2,ERROR,mm_wear_level_move.c,"FW is aborting WLM on powerloss. Dest DPA byte address 0x%08X_%08X"
821654256,1,ERROR,ait_dram.c,"AIT DRAM Controller Errors: 0x%08X"
821380737,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD1: 0x%x"
821022729,0,ERROR,hardware_wear_level_move_engine.c,"Line state is invalid."
820643164,1,DEBUG,wear_level_move.c,"Bad Block transition State Machine : %d"
820634837,0,ERROR,security_interface.c,"Couldn't queue Key Management Init security request"
820393757,4,INFO,address_scrub.c,"Validate Address Failed. Start Address: 0x08%X_%08X End Address: 0x%08X_%08X"
819626445,0,WARNING,fw_img_auth.c,"Invalid image block size"
819045026,0,ERROR,key_management.c,"Failed to unwrap PM-RK with security disabled wrapping key"
81865647,0,ERROR,i2c_bus_manager.c,"Energy meter failed to resume after queued I2C bus requests were processed."
818082314,2,ERROR,sxp_trims.c,"0x60F register read failed. Can't check media type on Rank: %d, Die: %d"
816893576,0,ERROR,fw_image_sync.c,"SPI write error during copying one section of SPI to another!"
815984756,0,ERROR,ddrt_restore.c,"S3 Resume Failed- Unable to restore DDRT training registers"
814783727,0,INFO,power_budgeting_engine.c,"Energy Meter is in pause state"
814315911,15,ERROR,dma_polled.c,"Address Verify Error! FaultData Rank: 0x%01X; Stype: 0x%01X; RetryIndex: 0x%01X; Vdm: 0x%01X; FwErrComp: 0x%01X; FwErrAddrComp: 0x%01X; Length: 0x%01X; Rdir: 0x%01X; WdbAddr: 0x%02X; Rid: 0x%02X; Rtype: 0x%02X; WriteCount: 0x%01X; InitialVdm: 0x%01X; AitSecondCopyPoison: 0x%02X; PoisonStatus: 0x%06X;"
813859751,0,ERROR,log_msc_spare_ctrl.c,"Normal mode."
812366672,0,ERROR,fw_image_sync.c,"SPI read error during SPI block authentication!"
811828724,0,DEBUG,task_security.c,"SECURITY_UNLOCK_UNIT"
811275692,0,DEBUG,ait.c,"AIT lookup is disabled!"
810035558,0,ERROR,sxp_init.c,"Sxp_SenseAmpCalibration failed"
805742069,0,DEBUG,ddrt_scheduler.c,"lockFailCounter is about to wrap"
805509294,0,DEBUG,command_features.c,"Get Admin Features: Latch System Shutdown"
805198056,2,ERROR,message_channel.c,"Message channel read data invalid! ctrl = 0x%08X, status = 0x%08X"
804228703,0,ERROR,fw_activate.c,"Current Dynamic VDM window saved during FW activate is greater than VDM window to apply."
804094493,0,ERROR,key_management.c,"Failed to generate the key encryption key from passphrase and salt"
8037070,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr6: 0x%x"
801760379,0,ERROR,core_wear_level_move.c,"FBE AIT DMA Line Callback DMA Failure"
800770492,0,ERROR,command_effect_log.c,"More modifiable entries than expected."
800429739,0,DEBUG,platform_config_data.c,"MediaInterface returned NULL handler, exiting with error"
798963307,0,WARNING,ait_dram.c,"AIT DRAM Correctable Read Error threshold reached"
794845530,0,ERROR,partition_manager.c,"Unexpected mailbox may not remain locked throughout operation."
794004718,0,ERROR,spi_logger.c,"Couldn't check SPI debug region. Disabling SPI Debug logs"
793858081,0,DEBUG,power_state.c,"Surprise Reset Exit Clock Enable"
793124356,2,DEBUG,task_command_handler.c,"MB Nonce: 0x%08X:0x%08X"
790870177,0,DEBUG,command_features.c,"Set Admin Features: Set Protected Register Access"
788458522,0,ERROR,nlog_region_lock.c,"VDM tracking after DRAM load has finished."
787912404,0,ERROR,ddrt_scheduler.c,"Ddrt Mrc Programming Error: No Table Date Found"
786866547,1,ERROR,ras.c,"RAS Log: Valid bit not set - PW_LOG_WDB_UE = 0x%x"
784961583,3,ERROR,sxp_scheduler.c,"read SXP_REG_ADDR_MSR_12 failed! value = 0x%x, die = %d, rank = %d \n"
784105608,0,ERROR,dpa_verify_error_handler.c,"This error happens again after the transaction fatal, complete the transaction and go DIMM fatal!"
783383579,0,INFO,write_count_histogram.c,"Stop address > DIMM capacity"
782120395,0,ERROR,cpgc.c,"Valid mode not specified for DDR-T2 ACIOLB"
779371350,1,ERROR,update_firmware.c,"Invalid state %d"
777744289,2,WARNING,set_fconfig.c,"DFX Set Fconfig incorrect version Expected: 0x%X, Actual: 0x%X"
77606704,0,INFO,wear_level_move.c,"Block Move: Address is within spare block region"
775802949,0,INFO,refresh.c,"Resuming Migration"
774962586,0,WARNING,debug_log_data.c,"Dma transfer not completed!"
774311345,0,DEBUG,refresh.c,"first refresh is not in progress"
773986273,0,DEBUG,task_error_handler.c,"Retrieving settings for Package Sparing"
77180823,0,WARNING,debug_log_data.c,"DMA transfer not completed!"
769776342,0,INFO,wear_level_move.c,"Block Move: Cannot move CB or SMD or FSD"
766165137,2,ERROR,sxp_decode_media.c,"0x63F register read failed. Can't check media type on Rank: %d, Die: %d"
765501612,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaWrScrambleSeedSel: 0x%x"
764713683,0,ERROR,infoturn_error_log.c,"InitorRetrieveInfoturnErrorLog: Buffer address is 0x0"
760932766,1,DEBUG,host_interrupt.c,"Current blocks: 0x%x"
759824811,0,STATUS,fill_nlog_sram_buffer.c,"Starting FillNlogSRAMBuffer IMF"
758509092,0,DEBUG,command_features.c,"Get Features: Address Range Scrub"
755659150,0,WARNING,fw_img_auth.c,"Header length invalid"
755417426,0,ERROR,fw_image_sync.c,"Image Sync failed with loaded image header is not valid\n"
754939659,3,WARNING,wear_level_move.c,"FBL head pointer not in valid range. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
753845200,0,WARNING,debug_log_data.c,"DMA write to large payload region Error"
752707257,1,ERROR,data_path_error.c,"CSR Error, valid bit AND valid_unimpl_bit not set in log registers! FnvError %d."
75196581,0,ERROR,security_interface.c,"Couldn't queue EAU security request"
750520066,0,INFO,error_logging.c,"Creating new thermal entry"
747941909,0,ERROR,kechika_river_pmic_driver.c,"Cap self test start failed."
746697473,0,ERROR,die_error_emulator.c,"DieErrorEmulator: Error map due to earlier request exists."
746506743,2,ERROR,assert.c,"*** ASSERT *** module: (decimal) %d Line: %d"
746281987,0,STATUS,refresh.c,"Package Migration Completed"
743123522,1,ERROR,command_inject_error.c,"Wrong event notification: %d"
741735123,0,WARNING,command_features.c,"Not Bios Mailbox"
741635530,0,ERROR,block_move_error_handler.c,"Hardware wear level move: Illegal DPA error!"
741489486,1,ERROR,core_dump.c,"Package Sparing Policy - Enable: 0x%02x"
740942031,3,ERROR,sticky_die.c,"Partition unsticking SxpCmd_SendCommandWriteRegister failed on rank: %d, address: 0x%08X, value: 0x%08X"
739126684,1,ERROR,spd.c,"Invalid 3DXP DeviceID Fconfig token value: 0x%x"
738122295,0,INFO,ait_update.c,"Ait Update Main Line State: Poison Error!"
736842518,1,ERROR,partition_error.c,"Partition Error Log: Valid bit not set! DN_LOG_ADDR_REGION_ERR_1_VLD = 0x%x"
7342824,0,ERROR,power_budgeting_engine.c,"Failed to resume energy meter - energy meter is in unknown state."
732783198,1,ERROR,format_device.c,"Cmd Format Device, security MD rebuild failed. %d"
732035808,0,ERROR,dma_polled.c,"First copy of AIT was poison.  FW prepare read of AIT copy!"
726171581,0,ERROR,log_refresh_engine_start.c,"Refresh engine started!"
726151237,0,WARNING,command_inject_error.c,"Mailbox device error, handle was null"
724243208,0,ERROR,vdm.c,"Vdm_AdjustVdm, trying to adjust VDM0 on S15 media!"
723647355,3,ERROR,task_media_interface.c,"Unknown handle. 0x%08X. Free(%d) WIP(%d)."
723333897,0,WARNING,power_loss_log.c,"Did not read from power loss log because sxp training, context block init, or ait init failures"
719001031,0,ERROR,algo_training.c,"Saving SXP and DRAM registers unsuccessful - SPI writes failing."
71879241,0,ERROR,format_device.c,"Cmd Format Device, creating fw state failed."
718174110,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustIRst at Window. Window : %d"
716641766,3,ERROR,partition_error.c,"read address region error %u at DPA 0x%08X_%08X"
716271502,0,STATUS,pause_ait_dram_refresh_rate_updates.c,"AIT DRAM Refresh Rate Updates have been paused."
716167459,1,ERROR,partition_manager.c,"Unexpected number of mb %d payload unlock requests while media disabled."
715666859,1,ERROR,kernel.c,"APIC_TPR:0x%08X"
714246009,5,ERROR,scheduler_ddrt.c,"ERROR: DDRT PLL did not lock before timeout DDRT_PLL_REF_CTRL=0x%X, DDRT_RESET_STATUS=0x%X, D_DDRT_DCLK_CTRL=0x%X, MSC_FNVIO_VISIBILITY_CSR=0x%X, IO_INIT_CTRL=0x%X"
712128937,2,INFO,ras.c,"0x%08X: fault data: type 0x%02X"
708871995,0,ERROR,log_ait_move_complete.c,"AIT NM2 table move completed!"
70884491,0,DEBUG,buffers.c,"Queue not empty, preparing to dequeue."
708673484,1,WARNING,dfx.c,"ModuleSize was either NOT 256B aligned, less than 256B, or greater than 0x%08X"
708535468,1,ERROR,power_budgeting_engine.c,"Resuming energy meter failed with reset status 0x%X. Entering open loop power throttling"
706748048,1,ERROR,hal_pmic_vendor.c,"UNKNOWN RTK PMIC Stepping - Product Stepping: [0x%X]"
705964683,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz2: 0x%x"
704486389,0,WARNING,sxp_commands.c,"ZQCal Short REQ bit still set after delay!"
703878727,1,ERROR,log_emask_imask_regs.c,"DN_IMASK: 0x%x"
701671887,1,ERROR,log_vdm_for_wlm.c,"FreeBlockExpansionState: %d"
70104796,1,INFO,ait_read_line.c,"Transition Ait Readline State Machine : %d"
700230646,0,ERROR,format_device.c,"Cmd Format Device, context block rebuild failed."
698705293,2,ERROR,commands.c,"BIOS Api version set to 0x%X, FW API: 0x%X"
698403345,1,ERROR,nlog_region_lock.c,"D_TWO_LM_BASE_ADDR_H: 0x%08x"
697700217,0,ERROR,key_management.c,"Failed to unwrap PM-RK with KEK"
69665117,2,ERROR,short_stroke.c,"Short Stroke offset %d is invalid. It must be a multiple of Short Stroke Size %d when HW Short Stroke is enabled"
696564616,1,ERROR,core_dump.c,"SKU ID  -  0x%08x"
694197297,2,ERROR,wear_level_move.c,"WearLevelMove_Transition Could not refresh all source lines of pda 0x%08X_%08X"
693509916,0,WARNING,command_features.c,"Invalid parameter for Address Range Scrub"
69323143,0,ERROR,key_management.c,"Failed to unwrap PM-RK using security disabled wrapping key"
68878366,0,ERROR,ltec.c,"ERROR: Disabling LTEC due to update failure. LTEC rails are currently at BOOT VID"
684779696,0,ERROR,dfx.c,"Large payload upload logical read failed!"
683742367,0,WARNING,command_features.c,"Clear History can only be executed when no Poison Errors have been injected."
676063385,0,WARNING,security_interface.c,"HMAC security queue request timed out"
675099758,0,ERROR,sxp_training.c,"SXP timing tables are unversioned!"
674568170,0,ERROR,reg_flow.c,"SPI table authentication failed!"
673693500,1,ERROR,log_vdm_for_wlm.c,"WearLevelMoveState: %d"
673683856,1,ERROR,sxp_scheduler_init.c,"Unsupported SXP Device Device ID read error. DeviceId = 0x%X"
673328722,1,DEBUG,host_interrupt.c,"Event[%d] DT is Ready, clearing block"
673184999,0,ERROR,power_loss_log.c,"At least one PLI log was corrupt from last PLI."
672133723,0,DEBUG,task_security.c,"SECURITY_GET_INFO"
671790448,0,ERROR,ltec.c,"LTEC received multiple requests to enter normal mode. DDRT IO Init. sequence may be invalid"
671481062,0,ERROR,task_command_handler.c,"Format was completed. Power cycle is required after a device format."
670622231,0,ERROR,example_pimf_command.c,"Congrats! You made it inside a pIMF module!"
670180285,0,WARNING,power_state.c,"Listener already present."
669959559,2,ERROR,security_md.c,"Security md checksum failed on copy: %d, checksum = 0x%08x"
667561700,1,ERROR,sxp_commands.c,"ZQCal Long REQ bit still set after delay for rank %d!"
666435400,1,ERROR,die_error_emulator.c,"Invalid VDM level %d"
662659228,0,ERROR,ltec.c,"LTEC DDRT training mode update failed due to I2C bus error"
661721967,4,ERROR,sxp_scheduler.c,"SXP Mixed Stepping ID detected [%d] != [%d] at rank=%d die=%d"
661706542,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustS26IRst at Window. Window : %d"
659017194,0,ERROR,write_delay_read.c,"Buffer address is 0x0"
657915379,0,ERROR,command_software_triggers.c,"Fatal error software trigger is disabled"
656519100,1,ERROR,pli_host_throttling_check.c,"DRDP_WCRD_TIMER: 0x%x"
655842185,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaRdScrLfsr: 0x%x"
655320832,0,ERROR,infoturn_error_log.c,"QueueInfoturnErrorLog: Buffer address is 0x0"
653653641,0,ERROR,fw_img_auth.c,"EAU signature padding verification (padding 1, 3 and 4) failed"
650267572,1,ERROR,error_logging.c,"Wrong power event notification: %d"
650187472,0,ERROR,ddrt_training.c,"Ddrt_RxDqDqsTraining failed"
64953126,1,ERROR,power_event_at_image_auth.c,"Stopping image sync in state: %d"
649284436,0,ERROR,command_inject_error.c,"Error Injection is disabled"
647612524,0,ERROR,log_ait_move_start.c,"AIT NM2 table move started!"
64758110,0,ERROR,address_scrub.c,"Failed to get handle for DMA. Stopping Address Range Scrub"
647396872,1,ERROR,log_pli_io_trig.c,"MSC_SPARE_CTRL: 0x%x"
643561745,0,WARNING,command_features.c,"Invalid PCD Retrieve Option"
642624003,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr1: 0x%x"
641798086,1,ERROR,short_stroke.c,"Short Stroke offset %d is invalid"
639585996,1,ERROR,short_stroke.c,"Short Stroke Size %d is invalid"
639295238,0,ERROR,overwrite_dimm.c,"AIT Read failed"
637871166,1,ERROR,fw_init.c,"Previous boot PowerStateEvents is 0x%x"
637784915,1,ERROR,fw_activate.c,"DDRT Write Transactions during FW Activate: 0x%08x"
63657748,0,ERROR,ddrt_training.c,"DdrtTraining_StartTraining- Failure while Programming DDRT IO registers from MMRC"
634662707,2,ERROR,mm_free_block_expansion.c,"Initial AIT Copy: %d, Current Copy: %d"
634051287,2,ERROR,datastore.c,"Entry Size Mismatch on token %d in datastore %d. This is bad, Make sure you updated the datastore correctly"
632259093,0,WARNING,task_security.c,"Unable to Unlock Unit: Encryption Disabled"
631732977,0,ERROR,dfx.c,"Injection module upload failed!"
631376755,0,ERROR,task_media_interface.c,"DMA retry failed with SRAM parity error again!"
631180036,1,ERROR,log_emask_imask_regs.c,"DN_FIFO_EMASK: 0x%x"
630787440,0,WARNING,fw_img_auth.c,"Either Key, Modulus, or Exponent size is invalid"
630692829,0,ERROR,algo_training.c,"Restoring SXP and DRAM registers unsuccessful - SPI reads failing."
630688912,1,INFO,sxp_init.c,"Writing Training Report CRC: 0x%08x"
630256938,0,ERROR,ddrt_training.c,"DdrtTraining_StartTraining- Failure while Programming DDRT IO registers from MMRC"
626433991,1,ERROR,cpgc.c,"Invalid ACIOLB mode requested (%d)"
62455580,1,ERROR,write_disturb_engine.c,"WD Threshold value (%d) is invalid in SetQueuePolicy during MediaManagerInit"
621867782,3,ERROR,partition_error.c,"write address region error %u at DPA 0x%08X_%08X"
620787980,2,DEBUG,nlog.c,"wr 0x%08X = 0x%08X"
618845618,0,ERROR,command_features.c,"S3 Restore has not completed, and PLL's haven't locked"
61865499,0,WARNING,command_fw_update.c,"Uploaded binary is not 256B aligned"
615935416,0,ERROR,task_media_interface.c,"DMA command failed with AHB error twice in a row!"
61572666,0,ERROR,fw_upd_halt_at_spi_write.c,"Stopping update timer"
615206071,1,WARNING,spi.c,"Invalid Read Size %d"
614897296,0,DEBUG,task_security.c,"SECURITY_ERASE_UNIT"
614168269,0,ERROR,block_move_error_handler.c,"Hardware wear level move: Illegal PDA error!"
614087275,15,STATUS,hal_pmic_rail_cwv.c,"Current Rail Values: A[%d][%x] B0[%x] B1[%x] C[%x] D[%d][%x] E[%x] F[%x] G[%x] H0[%x] H1[%x] J[%x] K[%x] L[%x]"
613660783,0,ERROR,ait_read_line.c,"AitReadLineRead Complete with Failure Status!"
609215373,0,DEBUG,command_features.c,"Get Admin Features: Platform Config Data"
607022232,0,ERROR,sxp_rmt_tests.c,"RAS Tx Vref Max Mask Test Failed"
606916560,1,ERROR,log_emask_imask_regs.c,"CHN_IMASK_1: 0x%x"
605974024,1,ERROR,sxp_trims.c,"PCL reg access not supported for DIMMs with ranks %d"
60442795,0,ERROR,ddrt_scheduler.c,"SPI read error during reading DDRT IO MMRC end table!"
60355344,0,ERROR,power_budgeting_engine.c,"I2C Host in bad state"
601481001,0,WARNING,command_features.c,"Config Lockdown not supported"
600067245,0,ERROR,adaptive_vdm.c,"AVDM pull flow AIT read failed"
599494689,0,ERROR,short_stroke.c,"Short Stroke Fconfig values are invalid, Going DIMM Fatal"
598404248,2,ERROR,core_dump.c,"HW CSR Address: 0x%08x Value: 0x%08x"
594123342,0,WARNING,command_fw_update.c,"Small Payload: New image is larger than the max image size in SPI"
593260970,0,INFO,ddrt_scheduler.c,"DDRT Ungate Pll!"
592122228,3,ERROR,dynamic_vdm.c,"Populate Near AdwlVdm rank %d die %d deck %d is invalid"
591851255,0,WARNING,wear_level_move.c,"Source PDA doesn't match WDPQ PDA - Block has moved already"
591711949,0,ERROR,sxp_init.c,"Sxp_SenseAmpCalibration failed"
591466616,0,ERROR,ait_dram.c,"DRAM loading stall detected!"
589748085,1,ERROR,assert.c,"ESP +  0: 0x%X [    Instruction Pointer (EIP)   ]"
589411494,1,ERROR,nlog_region_lock.c,"D_FW_MB_LOCK: 0x%08x"
586291298,0,ERROR,power_loss_log.c,"Error translating PLI log buffer A's dpa address to pda"
586093292,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaWrScrLfsrL: 0x%x"
585982027,1,DEBUG,memory_info.c,"DFX Memory Info Page Requested - Allowed [%x]"
585589119,0,ERROR,core_wear_level_move.c,"Free Block Expansion operation has fatally failed, request has been dropped!"
584514983,1,ERROR,core_dump.c,"  - CurrentMbTracker: %d"
583230042,4,ERROR,task_error_handler.c,"AIT Scrub Start! FaultData DPA 0x%08X_%08X; PDA 0x%08X_%08X"
582453175,3,WARNING,task_error_handler.c,"Error found for domain %u ferr_%u bit %u, no handling other than clearing the bit"
580963782,0,ERROR,dfx.c,"DMA did NOT complete!"
579910123,0,DEBUG,command_reset_policies.c,"ResetPolicy : Data Dump"
579207786,1,WARNING,set_fconfig.c,"DFX Set Fconfig length too big: 0x%X"
578595464,0,ERROR,dynamic_vdm.c,"DynamicVdm_Adjustment_TimerCallback called with VDM_WINDOW_NONE!"
577116268,0,WARNING,command_features.c,"Alarm Threshold: Invalid spare block parameter"
576031070,2,ERROR,task_high_priority_message_handler.c,"HPMH Message queued when queue was full. Message ID: %d, events 0x%08X"
573835598,1,ERROR,sxp_init.c,"after trim change ZQCalLong command failed for rank: %d"
572874746,0,ERROR,write_count_histogram.c,"Write Count Status results have some overflowed steps"
5722307,1,ERROR,wear_level_move.c,"FW is aborting WLM on powerloss. A_WLV_MV_DEST 0x%08X"
571702531,1,ERROR,core_dump.c,"Stack address not found in stack regions! Failed to get call trace. addr: 0x%X"
570080119,2,ERROR,sxp_trims.c,"0x50D register read failed. Can't check media type on Rank: %d, Die: %d"
56972515,1,INFO,power_budgeting_engine.c,"Energy Meter has missed %d I2C sequences in the current accumulation window, initiating safe mode"
568352036,0,ERROR,key_management.c,"Forward expansion of PM-RK failed"
568147231,0,ERROR,platform_config_data.c,"Invalid DMA direction"
567293909,0,INFO,wear_level_move.c,"Block Move: Cannot move CB or SMD"
567095745,0,WARNING,command_features.c,"Not able to complete command - either not unlocked or not skuable"
566777726,1,ERROR,thermal_engine.c,"Forced temperature calibration workaround, set: %08X"
565111536,0,ERROR,data_path_error.c,"2 WECC's detected within WECC_WINDOW"
56461553,1,ERROR,log_emask_imask_regs.c,"DA_IMASK: 0x%x"
564047915,1,ERROR,ras.c,"RAS Log: Valid bit not set - DN_LOG_RDATA_E2E_CRC_ERR_1 = 0x%x"
562356851,1,ERROR,fw_upd_halt_at_img_auth.c,"FwUpdate will halt at block: %d"
56227732,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaWrScrLfsrH: 0x%x"
560618204,0,WARNING,command_features.c,"Unknown Command"
560412016,4,ERROR,vdm.c,"Vdm_AdjustVdm failed to adjust vdm %d by value %d on rank %d die %d."
557876568,1,ERROR,nlog_region_lock.c,"D_PM_BASE_ADDR_H: 0x%08x"
555665409,2,ERROR,sxp_trims.c,"0x60F register read failed. Can't check media type on Rank: %d, Die: %d"
555640658,0,DEBUG,command_features.c,"Get Admin Features: Platform Config Data"
554845618,3,ERROR,core_dump.c," - Header -> WriteCounter: %d | Version: %d | isCorrupt: %d"
548019077,4,ERROR,aclk_periodic.c,"ACLK Calibration : SxpCmd_SendCommandWriteRegister failed on rank : %d, die : %d, address : 0x%08X, value : 0x%08X"
547958696,0,DEBUG,command_inject_error.c,"Inject poison DPA to memory type mismatch"
547595076,1,ERROR,log_msc_spare_ctrl.c,"MSC_SPARE_CTRL: 0x%x"
547567651,0,ERROR,ltec.c,"LTEC failed to apply BOOT_VIDs during reset event."
547086209,0,INFO,security_interface.c,"Security_GetSecurityRequest: No work waiting in RequestQueue"
546696432,1,ERROR,core.c,"Core Message queued before handler was provided. Message: 0x%X."
544186057,0,STATUS,power.c,"PLI is detected."
543693514,1,ERROR,ras.c,"RAS Log: Valid bit not set - DN_LOG_RDATA_POSION_1 = 0x%x"
542388935,4,ERROR,die_error_emulator.c,"DieErrorEmulator SxpCmd_SendCommandWriteRegister failed on rank : %d, sxpDie : %d, address : 0x%08X, value : 0x%08X"
539945176,0,ERROR,write_disturb_engine.c,"Called with no entries in the HW queue pending."
536896231,4,INFO,ras.c,"0x%08X: fault data: info0 0x%08X, info1 0x%08X, info2 0x%08X"
535941459,0,DEBUG,pmic.c,"PMIC Set Bits Error"
533453043,0,WARNING,command_features.c,"Command not permitted after Config Lockdown"
530160937,0,ERROR,task_error_handler.c,"AIT scrub failed, queue the BBM!"
528992081,0,ERROR,power_budgeting_engine.c,"Energy meter unresponsive (missed 3 accumulation windows), disabling closed loop power throttling."
527803552,3,WARNING,wear_level_move.c,"FBL tail pointer not in valid range. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
527407999,6,ERROR,fw_img_auth.c,"Image with incompatible HW Architecture detected. Running DIMM Info: Vendor ID (0x%x), Device Id: (0x%x), Revision Id (0x%x). ""Image header under authentication Info: Vendor ID (0x%x), Device Id: (0x%x), Revision Id (0x%x)"
522085303,3,DEBUG,task_command_handler.c,"Recd. Mailbox Cmd. 0x%08x:%08x , %x"
52158704,3,ERROR,power_state.c,"PowerState_AddListener: Max Power Listeners Reached - %d, add New Listener 0x%x failed with Transition Event = %d"
520304268,0,INFO,platform_config_data.c,"Allocate Buffer Callback Made DDRT"
519723911,1,ERROR,hal_pmic_cap_test.c,"PLI Cap Value is Critically Low. Self Test Time : %d"
518920795,1,ERROR,log_power_event_end.c,"PowerStateEvents: 0x%x"
518713661,1,ERROR,ras.c,"RAS Log: Valid bit not set - DS_LOG_WDATA_POSION_1 = 0x%x"
516847966,0,DEBUG,address_scrub.c,"DMA Callback"
515128071,0,ERROR,thermal_engine.c,"DTS Calibration still running, cannot poll controller"
514425955,2,ERROR,ltec.c,"ERROR: Unsupported rail ID %d passed to Ltec_GetSlopeOffset. Using default slope offset of %d uv/C."
513615253,0,ERROR,fw_img_auth.c,"EAU signature hash algo id verification failed"
513531783,0,WARNING,fw_img_auth.c,"Invalid image block size"
513237343,0,WARNING,task_security.c,"Unable to Freeze Lock: Encryption Disabled"
512499462,0,ERROR,adaptive_vdm.c,"AVDM pull flow AIT read failed"
511390785,0,DEBUG,task_security.c,"SECURITY_SHA_DMA"
509104521,0,ERROR,fw_img_auth.c,"EAU signature padding verification (padding 2) failed"
508621224,0,ERROR,die_error_emulator.c,"DieErrorEmulator: Spare die is not part of the common id group. DQ failure is not supported on this die."
508316016,0,ERROR,host_throttle.c,"HostThrottle_EnableFeature called"
507385744,1,DEBUG,data_path_error.c,"AHB Address translated to DPA 0x%x"
506472558,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD1: 0x%x"
506376150,0,ERROR,format_device.c,"Cmd Format Device, building AIT failed."
504136657,0,ERROR,command_fw_update.c,"Cannot update FW because image sync has not completed"
503817300,0,DEBUG,command_features.c,"Set Admin Features: System Time"
50320106,1,ERROR,pli_log_entries.c,"Requested PLI Log page is out of bounds 0x%x"
502423771,0,DEBUG,life_span.c,"Percent Remaining alarm tripped"
501569278,0,INFO,fw_img_auth.c,"Decrypting image signature"
501543743,1,ERROR,pli_host_throttling_check.c,"DN_SPARE_CTRL: 0x%x"
50136954,10,ERROR,sxp_commands.c,"SXP Reg Read Error D[%d]MSR[%x]:%x,%x,%x,%x,%x,%x,%x,%x"
50065735,1,INFO,kechika_river_pmic_driver.c,"PMIC Detected PRODUCT: 0x%x\n"
500564767,1,ERROR,wear_level_move.c,"Default case in FBE state machine hit! STATE = %d"
496416111,0,ERROR,sxp_training.c,"Sxp Mrc Programming Error: No Table Found"
49637989,0,DEBUG,task_command_handler.c,"Mailbox Success"
495300776,0,DEBUG,task_error_handler.c,"Ait Scrub Allocate Buffer Callback"
494596053,1,ERROR,fw_image_sync.c,"Image_Sync_Completed called with an unexpected status: %d"
494560807,0,ERROR,dma_polled.c,"GLB_NERR_1 RACQ Parity error in dma polled"
494262675,0,ERROR,power_budgeting_engine.c,"EM reset operation failed due to I2C operations timing out"
492050011,1,ERROR,power_budgeting_engine.c,"Detected invalid reporting time constant: %dms"
49075992,0,STATUS,ddrt_restore.c,"S3 Resume Restore has completed"
490548138,0,ERROR,format_device.c,"Cmd Format Device, context block rebuild failed."
489137472,0,WARNING,command_features.c,"Invalid parameter for Address Range Scrub"
487743316,1,ERROR,task_media_interface.c,"We received a DMA completion event, but there is a DMA active adma_status: 0x%X"
487036899,0,WARNING,dfx.c,"Injection module framework is in DEBUG mode. Be careful!"
486832990,0,ERROR,ait_dram_scheduler.c,"AIT DRAM refresh rate changed to 2x"
483300151,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustToWindow does not have a window type for vdmWindow %d"
482807227,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD0: 0x%x"
48243579,0,WARNING,task_media_interface.c,"DMA timed out; aborting!"
482214124,0,ERROR,fw_img_auth.c,"EAU engine failed"
480855854,1,ERROR,sxp_init.c,"Sxp_CoarseWriteLeveling failed rank: %d"
48079406,1,ERROR,log_zqcal_short.c,"APB_TIMER2: 0x%08X"
478788975,0,DEBUG,command_features.c,"PCD Get Data SMBus"
47718859,1,ERROR,wear_level_move.c,"FreeBlockExpansion_Dispatch unexpected relocate block msg:%x"
475478519,1,DEBUG,hal_pmic_rail.c,"Waiting %d microseconds for PMIC voltage ramp to complete"
474941692,2,ERROR,ait.c,"AIT Log: Valid bit not set! base = 0x%x, hi = 0x%x"
474783342,0,DEBUG,key_management.c,"Wrapping S3 Stored Persistent Memory Keys"
473855689,0,DEBUG,command_features.c,"Get Admin Features: System Time"
473537158,2,DEBUG,platform_config_data.c,"Subtracted Address: 0x%08X_%08X"
472109737,0,DEBUG,task_command_handler.c,"Task_CommandHandler: Media Disabled Command Not Allowed"
471570006,0,ERROR,crypto_selftests.c,"PKCS #5 v2.0 PBKDF2 [PRF=HMAC-SHA-384] Test FAIL: Result does not match expected KAT output."
471228626,0,DEBUG,command_features.c,"SS: Security Secure Erase Policy"
470065140,4,ERROR,sxp_wr_dqs_training.c,"Adv_TxDqDqs failed margin check R[%d] B[%d]: R[%d] F[%d]"
466808639,1,ERROR,task_media_interface.c,"AitRead. Invalid level provided. 0x%X."
465919494,3,ERROR,algo_write_leveling.c,"DRAM External Coarse WrLvl failed. Rank[%d] BytePassMask[%x] BytePassFlag[%x]"
464342236,1,ERROR,ait_dram.c,"Fatal Error: DRAM loading stall detected at the index 0x%x!"
463879688,0,STATUS,update_firmware.c,"Previous FW Update completed successfully"
463354348,0,WARNING,command_features.c,"Invalid SKU"
463307908,0,ERROR,enqueue_media_request.c,"Media request is not allowed."
462798704,0,INFO,security_interface.c,"Security_CompleteRequestWithResponse completed...Response queued...Event generated"
462671803,0,WARNING,command_features.c,"Invalid Mailbox SubOpcode"
462078570,2,ERROR,power_event_at_image_sync.c,"Stopping image sync at chunk: %d, in state: %d"
461434814,2,ERROR,kechika_river_pmic_driver.c,"PMIC Manufacture ID: 0x%X    Product Stepping: 0x%X"
460273654,0,ERROR,ddrt_scheduler.c,"Ddrt Mrc authentication failed!"
459990748,1,INFO,task_command_handler.c,"Current Mailbox: %d"
459826403,1,ERROR,datastore.c,"Dropped token %d"
459573075,0,ERROR,ait_read_line.c,"AitReadLineRead SRAM buffer is too small!"
458478479,5,ERROR,ddrt_scheduler.c,"ERROR: DDRT PLL did not lock before timeout MSC_FNVIO_INIT_CONTROL_0=0x%X, DDRT_RESET_STATUS=0x%X, D_DDRT_DCLK_CTRL=0x%X, MSC_FNVIO_VISIBILITY_CSR=0x%X, IO_INIT_CTRL=0x%X"
458104853,1,ERROR,log_bsr.c,"D_FW_STATUS: 0x%x"
457203263,0,WARNING,fw_img_auth.c,"Key Size field is invalid"
456497920,3,STATUS,ait_dram.c,"Platform API set -- DRAM Able to load: %d, Drift tracking ready: %d, load status: %d"
455740160,0,DEBUG,command_features.c,"SS: Overwrite DIMM"
45523417,0,ERROR,fw_init.c,"VCAP self-test failure detected"
454938051,0,INFO,overwrite_dimm.c,"Initialize Overwrite DIMM"
45471304,0,INFO,security_interface.c,"Security State: Locked"
454045308,1,ERROR,nlog_region_lock.c,"D_FW_MB_LOCK: 0x%08x"
447332779,3,ERROR,sxp_trim_bundle.c,"Could not populate AdwlVdm %d from S2X_REG_ADDR_TMR_ADWLVDM_NEAR_DECK_%d. Register Data: 0x%04x"
447272206,0,ERROR,sxp_device_access.c,"SXP Devices do not have Persistent ID fused. Cannot apply desired device mode."
446966442,0,ERROR,key_management.c,"Forward expansion of VM keys failed"
446694719,1,ERROR,ait_nm3_csr.c,"AIT N-3 entry has single bit correctable error. Index: %d"
446572519,0,ERROR,ait.c,"Ait_LookupAitEntryDpaLevel was called for a level of N-3, should never happen!"
445252694,1,ERROR,core_dump.c,"FwDebugData - pmicInitReason: %x"
443956059,0,ERROR,platform_config_data.c,"Invalid Small Payload Part during set operation"
442282519,2,ERROR,short_stroke.c,"Short Stroke size %d is invalid. It must be at least %d when Short Stroke FW mode is set"
441515797,0,ERROR,task_error_handler.c,"Both AIT UECC, don't complete the transaction!"
441364512,0,ERROR,fw_init.c,"Failed to load soft fuses"
440386986,0,ERROR,fw_init.c,"Unsupported Device ID, regflow table is not loaded"
440240544,0,ERROR,fw_upd_halt_at_img_auth.c,"Stopping update timer"
440083156,1,ERROR,core_dump.c,"***** CoreDump End: %x   *****"
439264194,2,ERROR,log_image_sync_complete.c,"Image sync has been completed at stage: %d, image chunk: %d"
435137326,0,ERROR,ait_dram_scheduler.c,"Ait Dram Scheduler Init failed"
43473006,2,ERROR,sxp_init.c,"Sxp_AdvancedRxDqsTraining failed rank: %d Training type: %d"
432404181,0,ERROR,command_fw_update.c,"DMA Submission entry failed to queue."
431001291,0,INFO,ait_update.c,"AIT Update Backup Line State: Success Status!"
4293223980,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD4: 0x%x"
4293057648,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD3: 0x%x"
429176518,1,INFO,command_log.c,"Number of entries set to %d"
4290714463,0,ERROR,command_software_triggers.c,"Injected package sparing software trigger error"
4288909854,1,DEBUG,host_interrupt.c,"Event[%d] -> set device blocking"
428853814,0,ERROR,health_manager.c,"Spare Blocks = 0"
4285925692,0,DEBUG,task_error_handler.c,"Ait Scrub Allocate Buffer Callback"
4285790109,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz0: 0x%x"
4284294744,1,INFO,fw_image_sync.c,"Sync Completed Successfully with %d authentication failures"
4283329772,1,ERROR,update_vsm_block_sxp_io_traffic.c,"PCSCLR_CFG1: 0x%x"
4282864397,0,WARNING,command_features.c,"Attempted to set a invalid System Time"
4282738969,0,INFO,command_log.c,"Get FW Image Info"
4279029300,0,ERROR,feature_state_data.c,"Feature State Data Initialization Failed"
4278821751,3,DEBUG,spi.c,"Write sramAddress: 0x%08X, spiAddress: 0x%08X, size: 0x%08X"
4278310544,0,ERROR,ait_dram_scheduler.c,"Incorrect raw DIMM capacity detected"
4275989786,2,ERROR,datastore.c,"Invalid datastore header version. Dest Id: %x Version: %x"
4273012855,3,ERROR,task_error_handler.c,"Dclk is not enabled when handling DA_FERR. DdrtPllLocked = %d, DdrtCkDet = %d, DdrtCkIdle = %d"
4268705039,0,ERROR,command_fw_update.c,"Cannot update FW because image sync failed"
4267858853,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr7: 0x%x"
4267589260,10,ERROR,kechika_river_pmic_driver.c,"Current Rail Values: A[%d][%x] B[%x] C[%x] D[%d][%x] E[%x] F[%x] G[%x] H[%x]"
4265826439,15,ERROR,dma_polled.c,"Address Verify Error! FaultData Rank: 0x%01X; Stype: 0x%01X; RetryIndex: 0x%01X; Vdm: 0x%01X; FwErrComp: 0x%01X; FwErrAddrComp: 0x%01X; Length: 0x%01X; Rdir: 0x%01X; WdbAddr: 0x%02X; Rid: 0x%02X; Rtype: 0x%02X; WriteCount: 0x%01X; InitialVdm: 0x%01X; AitSecondCopyPoison: 0x%02X; PoisonStatus: 0x%06X;"
4263941367,0,ERROR,ltec.c,"Setting Health Status Critical. HSR is set to performance degraded"
4263880059,0,INFO,security_interface.c,"Security free pool is unavailable!"
4263680776,0,DEBUG,command_features.c,"SS: Get Security OptIn Payload"
4263603252,0,DEBUG,command_features.c,"Set Admin Features: Clear History"
4262694919,0,DEBUG,task_error_handler.c,"New AIT Scrub Event"
4260388724,1,ERROR,kernel.c,"APIC_TPR:0x%08X"
4259551757,0,DEBUG,command_features.c,"Get Features: DDRT Alerts"
4259454622,0,ERROR,dma_polled.c,"GLB_FERR_1 RACQ Parity error in dma polled"
4259101081,1,ERROR,update_vsm_resume_sxp_io_traffic.c,"PCSCLR_CFG1: 0x%x"
4258624893,1,ERROR,pmic.c,"PMIC Read Error : %d"
4257957013,1,ERROR,power_budgeting_engine.c,"Fail to disable EM. EmResetStatus = 0x%x"
4256637592,0,ERROR,security_interface.c,"Couldn't queue SHA RESET security request"
4254859135,2,ERROR,sxp_write_leveling.c,"SXP Coarse WrLvl failed rank[%d] nibble[%d]"
4254423850,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaRdScrLfsr: 0x%x"
4254095597,0,ERROR,kechika_river_pmic_driver.c,"Null pointer passed to KechikaRiverPMIC_ApplyDynamicVidRailSettings, not updating rails"
4253589147,1,ERROR,die_error_emulator.c,"Invalid relative VDM level %d"
4252117560,1,STATUS,command_software_triggers.c,"Percentage remaining software trigger is injected with a value of %d"
4251250452,0,ERROR,command_features.c,"Clear History has been executed."
4250888221,1,ERROR,block_move_error_handler.c,"WLM CSR access timeout: opcode = %d"
424893847,0,DEBUG,task_command_handler.c,"Task_CommandHandler: Media Disabled DFx Command Not Allowed"
4247354160,0,ERROR,task_high_priority_message_handler.c,"HPMH Message queued when queue was full."
4246728065,0,DEBUG,task_security.c,"SECURITY_SET_S3_RESUME_PASSPHRASE"
4245261493,0,WARNING,command_features.c,"Invalid value for Package Sparing Policy Enable"
4244366506,0,WARNING,sxp_commands.c,"SXP WriteReg REQ bit still set after delay!"
4243978897,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz3: 0x%x"
4242881498,0,ERROR,ltec.c,"PMIC rails are not at Boot VIDs at the time of LTEC failure. Going to Transaction fatal"
4242822447,2,ERROR,power_budgeting_engine.c,"DIMM Average Power [%d mW] has exceeded high watermark threshold [%d mW]"
4242413901,0,INFO,security_interface.c,"Security_GetSecurityRequest: RequestQueue has work ready to process"
4241964732,0,DEBUG,aes_bulk_encryption_selftest.c,"Verify AES Bulk Encryption successfully encrypted the first cacheline."
4240373053,0,WARNING,breakpoint.c,"Invalid Breakpoint"
4239754995,0,ERROR,sxp_init.c,"Sxp_SaveSxpIoRegisters failed"
4237487862,0,INFO,wear_level_move.c,"Block Move:  Address is within AIT[n-1] and AIT[n-2] table move in progress"
4237050748,0,WARNING,command_features.c,"Not able to complete command - either not unlocked or not skuable"
4236423577,0,INFO,wear_level_move.c,"FBE: AIT line of address contains Security Metadata and CB"
4235655141,3,ERROR,sxp_trim_bundle.c,"Could not populate AdwlVdm value %d to S2X_REG_ADDR_TMR_ADWLVDM_NEAR_DECK_%d (0x%04x)"
4235595009,0,ERROR,write_count_histogram.c,"Write Count Status: WD pending counter overflowed"
423271166,0,ERROR,season_device.c,"Season failed. Invalid Media Type."
4232537206,3,ERROR,sxp_trim_bundle.c,"irefSenseEnb SxpReg_PopulateIRefSenseEnbRead/Write returned %d on rank = %d die = %d. Iref Sense Enb Trim not set."
4232069919,1,ERROR,log_emask_imask_regs.c,"AITDR_RAS_IMASK: 0x%x"
4231972137,0,ERROR,algo_training.c,"Restoring SXP and DRAM registers unsuccessful - DRAM mode register write failed."
4231606159,10,ERROR,task_error_handler.c,"Uncorrectable error! Source Transaction Type 0x%02X; Initial VDM 0x%02X; Final VDM 0x%02X; FaultData 0x%08X_0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
4227756814,0,DEBUG,command_features.c,"SS: Set BIOS Security Nonce"
4225493847,0,WARNING,buffers.c,"Not a valid buffer range"
4224725706,3,ERROR,sxp_trims.c,"Unrecognized S26 media on Rank: %d, Die: %d, MediaMilestone 0x%X"
4223970668,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtLatency: 0x%x"
4223758133,1,ERROR,pli_host_throttling_check.c,"DN_SPARE_CTRL: 0x%x"
4222439263,1,DEBUG,ait_dram.c,"AIT DRAM Controller Error detected: 0x%08X"
422185061,0,ERROR,dpa_verify_error_handler.c,"This AVF error is on a RMW, do NOT complete transaction and go DIMM fatal!"
422007788,0,ERROR,aes_bulk_encryption_selftest.c,"*** FAIL *** encryption test"
4219907646,1,INFO,error_logging.c,"Saving log %d"
4216960716,6,DEBUG,dpa_for_pda.c,"0x%08X: DPA 0x%08X_%08X has AIT level N-%d DPA 0x%08X_%08X"
4216125145,3,ERROR,core_dump.c,"OutputPayload QWORD[%d]: 0x%08x_%08x"
4215824663,0,DEBUG,command_reset_policies.c,"ResetPolicy : Data Dump"
4213856657,1,ERROR,assert.c,"ESP +  8: 0x%X [      Stack Pointer (ESP)       ]"
421149543,0,ERROR,dma_polled.c,"Dma polled timed out during operation"
4211162721,9,ERROR,task_error_handler.c,"Uncorrectable error! Source Transaction Type 0x%02X; Initial VDM 0x%02X; Final VDM 0x%02X; FaultData 0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
4210769408,6,ERROR,spi_debug_structures.c,"Found In SPI Debug Region: CPU Exception -> Vec: 0x%08X, EIP: 0x%08X, ESP: 0x%08X, Info1: 0x%08X, Info2: 0x%08X, eflags: 0x%08X"
421012812,0,ERROR,kechika_river_pmic_driver.c,"Null pointer passed to KechikaRiverPMIC_ApplyDynamicVidRailSettings, not updating rails"
4209291200,2,ERROR,sxp_scheduler.c,"SXP Mixed DeviceIds detected [%d] != [%d]\n"
4209033759,0,WARNING,format_device.c,"REBUILD_MD security request timed out"
4204479995,0,ERROR,core_dump.c,"***** CoreDump End   *****"
4204168881,0,ERROR,ddrt_sense_amp_calibration.c,"Sense Amp Calibration Data Training- Failure did not find an SA Offset"
4201404406,0,WARNING,fw_img_auth.c,"Date field is invalid"
4201056430,0,INFO,address_scrub.c,"Abort Requested"
4200675776,2,ERROR,fw_image_sync.c,"Image Sync failed with error requesting SPI WriteWithErase at 0x%x in state: %d."
4199849533,0,INFO,security_interface.c,"Security_CompleteRequestWithNoEvent completed"
4198637744,0,ERROR,task_media_interface.c,"Unable to submit dma request. Requeuing back into the free queue."
4197814634,0,ERROR,sxp_scheduler.c,"PHY Initialization completion timed out"
4197729448,0,DEBUG,core_wear_level_move.c,"Wear Level Move No Spare Blocks!"
4196799994,0,ERROR,sxp_training.c,"Sxp Mrc Programming Error: No Table Found"
4195905468,0,ERROR,feature_state_data.c,"Feature State Data Needs Initialization - Creating Default"
4195905230,4,ERROR,vdm.c,"Vdm_AdjustVdm failed to adjust vdm %d by value %d on rank %d die %d."
4195809190,1,DEBUG,spi.c,"Sending %d write commands to SPI Flash"
4195443104,0,ERROR,ltec.c,"I2C Bus request queue full at time of LTEC DDRT training update request."
4194287081,0,INFO,commands.c,"Obtaining DIMM device characteristics"
4194251847,1,ERROR,ait_nm3_csr.c,"AIT N-3 entry has single bit uncorrectable error. Index: %d"
4193526912,1,ERROR,power_budgeting_engine.c,"Energy meter missed an accumulation window, miss count = %d"
4193095910,0,ERROR,dma_polled.c,"RACQ Parity failure in dma polled"
4192030434,1,ERROR,read_write_pmic.c,"After sending I2C request EM_STATUS: 0x%08x"
4190795472,1,ERROR,host_throttle.c,"HostThrottle_DecreaseThrottleLevelState called, current state %d"
4190189150,0,ERROR,command_effect_log.c,"Invalid access value for command"
4189385869,1,ERROR,sxp_init.c,"Fine Write Leveling Training failed, Rank: %d"
4187737076,0,DEBUG,key_management.c,"Initializing Key Values"
4187196254,0,INFO,ddrt_scheduler.c,"DDRT Gate Pll!"
4186774154,0,STATUS,spi_debug_structures.c,"Found In SPI Debug Region: PLI Checkpoint"
4186591919,0,ERROR,fw_img_auth.c,"EAU engine failed"
4185244670,2,ERROR,sxp_rcven_training.c,"Sxp_CoarseRcven failed rank[%d] status[%x]"
4184535842,0,ERROR,barlow_creek_pmic_init_reason.c,"Unknown PMIC Init reason - Unknown PMIC vendor."
4181728599,0,WARNING,fw_img_auth.c,"Either Key, Modulus, or Exponent size is invalid"
4180750142,0,WARNING,security_interface.c,"SHA-256 SDMA security request timed out"
4176945583,2,ERROR,address_verify_error.c,"AddrVerifyRepairDram: 0x%08x_%08x"
4173670224,1,ERROR,core.c,"Core Message queued before handler was provided. Message: 0x%X."
417237294,2,INFO,format_device.c,"Cmd Format Device, Capacity: %d in %d-byte chunks."
4171758866,0,WARNING,command_features.c,"Unable to set 4K partition sizes"
4171420250,3,WARNING,wear_level_move.c,"FBL tail pointer not in valid range. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
417131785,0,INFO,security_interface.c,"Security_GetSecurityResponse: ResponseQueue has response ready to process"
4168623977,1,ERROR,kechika_river_pmic_driver.c,"UNKNOWN RTK PMIC Stepping - Product Stepping: [0x%X]"
4167555387,0,ERROR,sxp_init.c,"Rank interleave configuration failed during FW activate reset."
4166244116,1,ERROR,power_budgeting_engine.c,"Firmware samples energy meter slower than every %dus."
4165918663,2,ERROR,dpa_verify_error_handler.c,"PDA read from DRAM ait copy is 0x%08X_0x%08X"
4164627073,1,ERROR,log_power_event_start.c,"CHN_WCTL: 0x%x"
4164531188,1,ERROR,core_dump.c,"DDRT MMRC Version: %d"
4163936891,0,ERROR,log_ddrt_io_init.c,"DDRT IO Initialization started!"
4163144591,0,ERROR,die_error_emulator.c,"DieErrorEmulator: Not supported on DIMMs that do not have common ID applied."
4160891805,1,ERROR,read_write_pmic.c,"Before sending I2C request PCSCLR_PWR_CFG7: 0x%08x"
4158847876,0,INFO,commands.c,"Obtaining DIMM information"
4156938722,0,DEBUG,command_features.c,"Set Admin Features: Viral Policy"
4156520987,0,ERROR,ait_read_line.c,"DMA read failed after attempt on ait backup line."
4155806246,1,DEBUG,task_command_handler.c,"Task Command Handler (0x%08X)"
4154231383,0,ERROR,wear_level_move.c,"Free Block Expansion operation has fatally failed, request has been dropped!"
4153440196,1,ERROR,data_path_error.c,"A FIFO U/O Flow Error 1 : 0x%08X"
4151482116,4,INFO,address_scrub.c,"Validate Address Failed. Start Address: 0x08%X_%08X End Address: 0x%08X_%08X"
4151235689,0,DEBUG,command_features.c,"Get Features: Power Management Policy"
4149893980,0,ERROR,key_management.c,"Failed to unwrap PM-RK with KEK"
4148254561,2,ERROR,core_wear_level_move.c,"FW is aborting WLM on powerloss. A_WLV_MV_DEST byte address 0x%08X_%08X"
4147506005,1,ERROR,fw_image_sync.c,"Image Sync completed with a null buffer in state: %d."
4146514140,0,ERROR,key_management.c,"Failed to generate the key encryption key from passphrase based derived key"
4145715103,0,DEBUG,memory_info.c,"Output Payload was NULL"
4144587509,0,DEBUG,key_management.c,"Wrapping S3 Stored Volatile Memory Keys"
4144071725,1,ERROR,ait_nm3_csr.c,"AIT N-3 entry has single bit uncorrectable error. Index: %d"
4143451044,1,ERROR,wear_level_move.c,"Wear Level Move: Relocate Block reported an error %d on move operation"
4143027809,2,STATUS,scheduler_ddrt.c,"DDRT locked at %d us after %d tries"
4142413271,1,ERROR,power_budgeting_engine.c,"Energy meter missed an accumulation window, miss count = %d"
4141883597,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr2: 0x%x"
4141233160,1,ERROR,fw_state.c,"Failed to retrieve valid FwState with error opcode: 0x%x"
4140475427,2,ERROR,sxp_init.c,"Coarse Write Leveling Training failed, Rank: %d Training type: %d"
4140204985,4,ERROR,core_dump.c," Log Entry[%d] -> Checkpoint [0x%x] ErrorCode [%d] Timestamp [%d]"
4139130920,0,ERROR,security_md.c,"Security Metadata Initialization Failed"
4138894346,1,WARNING,data_path_error.c,"data path error %u"
4137302869,1,ERROR,sxp_scheduler.c,"Unsupported Device 0x%08x. Not assigning the internal address offsets."
4135617362,0,ERROR,power_loss_log.c,"Could not load a PLI log (B) due to polled DMA error"
4134319420,1,ERROR,get_spi_manifest.c,"Spi read failed when reading MMRC table version at address x%08x"
413245358,0,WARNING,task_security.c,"Unable to disable passphrase: Encryption Disabled"
4131020373,0,ERROR,core_dump.c,"Mailbox Tracking Info:"
4129886878,2,DEBUG,platform_config_data.c,"PCD_GetPartitionDataSmbus: Partition - 0x%08X, Offset - 0x%08X"
4129409714,4,DEBUG,sxp_wr_dqs_training.c,"Advanced_TxDq Rising_Mid_Falling%d: %d_%d_%d"
412882674,2,STATUS,fw_init_profiler.c,"FW reached Mailbox Ready @ 0x%08X after %d us."
4128313512,0,ERROR,ddrt_training.c,"Ddrt_RxDqDqsTraining failed"
4125112060,0,INFO,zqcal_periodic.c,"Periodic Init"
412302095,0,ERROR,ait_dram_scheduler.c,"Invalid AIT DRAM size from fconfig."
4121381,0,ERROR,sxp_scheduler.c,"IoTrainReset: Bit never flipped to 1"
4117879439,1,ERROR,kechika_river_pmic_driver.c,"Invalid state message queued for processing: %d"
4117857928,1,ERROR,ddrt_training.c,"DdrtTraining_StartTraining- Failure at DDRT Sense Amp Calibration CNT=%d - ABORTING RETRY"
4116861182,0,WARNING,command_features.c,"Knob Value is not valid"
4116384833,1,ERROR,core_dump.c,"OtherStateInfo - IsShutdownTimeSet   : 0x%02x"
4113241761,0,ERROR,write_disturb_refresh.c,"WriteDisturbEngine_PollStartBit has failed. Start Bit has failed to de-assert!"
4112410447,3,ERROR,sxp_scheduler.c,"read SXP_REG_ADDR_MSR_12 failed! value = 0x%x, die = %d, rank = %d \n"
4112250965,0,INFO,ddrt_sense_amp_calibration.c,"Starting Sense Amp Calibration Training"
4112111319,3,WARNING,write_disturb_refresh.c,"Write Disturb Refresh failed with %d on PDA 0x%08x_%08x"
4109785729,2,ERROR,algo_training.c,"Restoring SXP and DRAM registers unsuccessful - Invalid checksum value [Actual - 0x%X, Expected - 0x%X]"
4107378192,0,DEBUG,key_management.c,"Wrapping S3 Stored Persistent Memory Keys"
4106786511,0,WARNING,task_security.c,"Unable to Erase Unit: Encryption Disabled"
4106700831,0,ERROR,thermal_manager.c,"Media temperature error injection is disabled to avoid the actual device overheating"
4105491207,0,ERROR,wear_level_move.c,"Bad Block Move operation has fatally failed, request has been dropped!"
4104997744,1,INFO,backside_training.c,"Writing Training Report CRC: 0x%08x"
4104393238,1,ERROR,data_path_error.c,"PW ERR STS FIFO U/O Flow Errors: 0x%08X"
4103147759,1,ERROR,read_write_pmic.c,"Before sending I2C request EM_CTRL: 0x%08x"
4102357408,0,DEBUG,command_features.c,"SS: Unlock Unit"
4098736187,0,STATUS,refresh.c,"Package Migration Started"
4096597409,0,ERROR,sxp_training.c,"Writing Training Report to SPI failed"
4096584201,1,ERROR,reg_flow.c,"SPI Table Error: Bad CSR Entry [%x]"
409521972,0,ERROR,enqueue_media_request.c,"Media request cannot be enqueued as its queue is full."
4093526215,1,ERROR,core.c,"Core General Message Handler called with invalid message id: 0x%X. Going transaction fatal."
4092044842,0,WARNING,sxp_commands.c,"ZQCal Long REQ bit still set after delay!"
40915492,0,DEBUG,platform_config_data.c,"Allocate Buffer Callback Made SMBus"
4091421619,2,ERROR,sxp_trim_bundle.c,"Could not determine TcHnlwlSelvWrtStep%d from 0x%04x"
4088337295,2,ERROR,chn_no_cmd.c,"Chn no cmd with no WLM for DPA 0x%08x_%08x deallocating WDB entry"
4088102032,1,ERROR,health_manager.c,"Die on package %d met failure criteria with no spare package available."
4088088299,2,ERROR,datastore.c,"Invalid datastore header version. Dest Id: %x Version: %x"
4085847447,1,ERROR,get_media_statistics.c,"GetMediaStatistics_GetAvdmData requested for Invalid VDM : %d"
4085803361,0,ERROR,command_features.c,"Setting FW Load Flag failed"
4085778200,0,INFO,smart.c,"Retrieving SMART data"
4085194807,1,ERROR,commands.c,"Cmd Format Device, security MD rebuild failed. %d"
4084896989,0,ERROR,format_device.c,"Cmd Format Device, failed to flush fw state with life time statistic."
4082455351,0,ERROR,ahb_unified_engine.c,"DMA Abort!"
4082078889,0,ERROR,vdm.c,"Vdm_AdjustVdm, trying to adjust VDM3 on S26 media!"
4081926654,0,DEBUG,command_inject_error.c,"Disabling poison on 4 cache lines"
4080986068,0,ERROR,power_budgeting_engine_imf.c,"Memory Bandwidth Boost feature is already initialized and started."
4080312536,1,ERROR,partition_manager.c,"Unlock Payload called when mb %d was already unlocked."
4079050591,0,ERROR,fw_init.c,"Failed to program boot vid to Rail D."
4078617586,1,ERROR,sxp_trims.c,"%d ranks not supported"
4078188718,0,WARNING,dfx.c,"No module uploaded - unable to execute"
4075728908,2,ERROR,algo_write_leveling.c,"SXP Coarse WrLvl failed due to incorrect fine write leveling result. Rank[%d] ByteFailArray[0x%X]"
4075627413,3,ERROR,aes_bulk_encryption_selftest.c,"*** FAIL *** read data (0x%x), expected data (0x%x), at dword offset %d"
4071988745,0,ERROR,wear_level_move.c,"Bad Block Check operation has fatally failed, request has been dropped!"
4071125951,0,ERROR,sxp_rank_interleave.c,"Unknown SXP devices, cannot set rank interleaving."
4070940641,2,ERROR,sxp_init.c,"Fine RcvEn Training failed, Rank: %d Training type: %d"
4069204515,1,ERROR,nlog_set_ddrt_io_init_info.c,"DDRT_RESET_STATUS: 0x%x"
4067268671,0,ERROR,ltec.c,"ERROR: Failed to update LTEC supported rails."
40656710,0,ERROR,leaky_bucket.c,"Unknown stat total requested"
4064614676,1,ERROR,long_op.c,"Wrong power event notification: %d"
406343928,9,STATUS,fw_init.c,"Current FW version - %02x.%02x.%02x.%04x, DIMM Unique ID - %04x-%02x-%04x-%08x, Power Cycle count - %d"
406186950,0,ERROR,fw_img_auth.c,"Hashing image block failed"
4060809670,0,DEBUG,ait_dram.c,"Unknown AIT DRAM Error -> should never see this"
4058049690,0,INFO,core_wear_level_move.c,"Block Move: Cannot move CB or SMD or FSD"
4057252202,1,ERROR,error_logging.c,"Failed to load Error Log %d"
405646844,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz3: 0x%x"
4053303973,0,DEBUG,task_security.c,"SECURITY_SET_S3_RESUME_AUTHENTICATE"
405322382,0,ERROR,media_statistics.c,"RMW Uncorrectable encountered but max write count CSR contains a value of 0. Could not decrement MWC."
4052025371,1,ERROR,log_power_event_start.c,"D_PWM_STS: 0x%x"
40519949,0,INFO,power_budgeting_engine.c,"Energy Meter hasn't been started yet."
4051945963,1,INFO,read_disturb.c,"Read Disturb Random Interval too big, set to max.  Too big: 0x%X"
4050546305,0,ERROR,buffers.c,"Core Buffer requested when queue was full. Going transaction fatal."
4049902169,0,ERROR,kechika_river_pmic_driver.c,"Failed to enter power good state"
4048829077,1,ERROR,ait_dram.c,"Wrong power event notification: %d"
4047979082,0,ERROR,hal_pmic_cap_test.c,"CAP test error - communication problem - rescheduling test"
4047415024,2,ERROR,datastore.c,"Entry Size Mismatch on token %d in datastore %d. This is bad, Make sure you updated the datastore correctly"
4047290963,2,ERROR,kechika_river_pmic_driver.c,"PLI Cap Value is Low. Self Test Time : %d, Voltage: %d"
4045483297,0,ERROR,dpa_verify_error_handler.c,"Retrying the command to channel failed!"
4045426375,1,ERROR,power.c,"PMIC Rail A set to [%d] as W/A since svid fuse returns 0x0"
4045308697,0,ERROR,fw_upd_halt_at_header_auth.c,"Stopping update timer"
4043079208,1,ERROR,log_power_event_start.c,"D_FW_STATUS: 0x%x"
4041645454,1,ERROR,sxp_reg.c,"Unsupported 3DXP media device type: 0x%08x"
4041059833,1,ERROR,fw_init.c,"Training Retry Failed at Count: %d"
4041044894,1,ERROR,core_dump.c,"ViralPolicy - Enable: 0x%02x"
4038740388,1,ERROR,vdm.c,"No Vdm Retry Path values to program for DeviceId = 0x%X."
4035936212,0,WARNING,command_features.c,"Security state is frozen or locked"
4033984038,1,ERROR,command_inject_error.c,"Injected a media temperature of %d C"
4032871351,0,ERROR,refresh.c,"Package Migration Completed"
4030882027,1,ERROR,die_error_emulator.c,"Die error emulator not supported on 3DXP device: 0x%08x"
402880033,1,INFO,sxp_init.c,"Writing Training Report CRC: 0x%08x"
4027440062,0,INFO,task_command_handler.c,"Part is UNLOCKED, executing dfx command"
4023141625,0,ERROR,security_error.c,"Security Key Error Log: Valid bit not set!"
4022365823,0,ERROR,fw_img_auth.c,"EAU signature hash algo id verification failed"
402225849,0,INFO,fw_image_sync.c,"Starting Sync"
4021979408,0,INFO,commands.c,"Obtaining DIMM device characteristics"
4021283623,0,ERROR,sxp_scheduler_init.c,"Failed to firewall RESET pins. Stop proceeding Rail D Floor Reduction."
4020826612,2,ERROR,core_dump.c,"RefreshState - Current Refresh Pointer  : 0x%08x_%08x"
4020561403,1,ERROR,log_power_event_end.c,"MSC_PLL_CTRL: 0x%x"
4018906515,0,ERROR,task_media_interface.c,"DMA command failed with SRAM parity error twice in a row!"
4018048008,0,ERROR,ltec.c,"I2C Bus request queue full at time of LTEC DDRT training update request."
4017733651,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz1: 0x%x"
4016926629,2,ERROR,package_spare_monitor.c,"Package sparing criteria met for package %d, error type %d"
4015430656,0,ERROR,ddrt_sense_amp_calibration.c,"Sense Amp Calibration Training- Failure did not find an SA Offset"
401541129,7,STATUS,update_firmware.c,"FW Update has successfully staged FW %02x.%02x.%02x.%04x, activation version: 0x%02x,""API version: 0x%04x. Current BIOS API version: 0x%04x"
401513414,1,ERROR,ras.c,"RAS Log: Valid bit not set - PC_LOG_RRAW_P0_PE = 0x%x"
4015115604,0,DEBUG,wear_level_move.c,"WLM state machine calling complete!"
40137574,1,ERROR,get_ait_info.c,"A_AIT_DEFEATURE: 0x%x"
401264204,0,DEBUG,command_inject_error.c,"Poison: DPA is undergoing relocation!"
4010998282,0,WARNING,spi.c,"Write Address Not Sector Boundary"
4010525208,2,STATUS,fw_activate.c,"Staged FW Api (0x%04x) is lower than the current API Handshake (0x%04x)."
4010214352,0,STATUS,high_priority_message_handlers.c,"S3 flow was aborted"
4009827459,2,ERROR,spi_flash_driver.c,"HW Failed to accept SPI request. cmd: %d, target: 0x%08X"
4009539145,4,ERROR,sxp_scheduler.c,"Error (%d) writing to register addr: 0x%04x rank: %d die %d"
400951202,1,ERROR,read_write_pmic.c,"After sending I2C request PCSCLR_PWR_CFG7: 0x%08x"
4008817572,5,ERROR,wdt.c,"Watchdog Timeout: Instruction Pointer(eip) = 0x%x, Stack Pointer(esp) = 0x%x, Fault Permission = 0x%x, Fault Address = 0x%x, eflags = 0x%x"
4006537263,0,ERROR,command_features.c,"Host Side DDRT Link Training Failure detected- Link unstable!"
4005642679,1,ERROR,log_power_event_end.c,"RPQ_WDB_STAT_EMPTY: 0x%x"
4004646551,3,INFO,format_device.c,"Cmd Format Device, Capacity: 0x%08X_%08X in %d-byte chunks."
4004604773,1,ERROR,partition_error.c,"Partition Error Log: Valid bit not set! Log_register_1 = 0x%x"
40037179,1,ERROR,hal_pmic_cap_test.c,"Message Handler incorrectly called with message: %x"
4003219943,0,DEBUG,task_command_handler.c,"Calling Security Interface Initialization"
4000864888,1,ERROR,kechika_river_pmic_driver.c,"Failed reading PMIC power good register with PMIC return code 0x%X"
4000629048,2,ERROR,sxp_trims.c,"0x63F register read failed. Can't check media type on Rank: %d, Die: %d"
4000193254,0,WARNING,update_firmware.c,"Supplied image is incorrect."
3996684178,2,DEBUG,platform_config_data.c,"PCD_GetPartitionDataSmbus: Partition - 0x%08X, Offset - 0x%08X"
3996680083,0,ERROR,overwrite_dimm.c,"Media interface DMA Queue Full"
3996070552,1,ERROR,kechika_river_pmic_driver.c,"PLI Cap Value is Critically Low. Self Test Time : %d"
3995732342,1,ERROR,command_software_triggers.c,"Percentage remaining software trigger is injected with a value of %d"
3994760349,0,ERROR,block_move_error_handler.c,"Hardware wear level move: WLM FSM CSR access timeout!"
3993965567,0,INFO,power_state.c,"Warm Reset Flow Retrain DDRT"
3992139714,0,ERROR,thermal_manager.c,"Media temperature error injection is disabled to avoid the actual device overheating"
3985557427,4,WARNING,sxp_write_leveling.c,"WARNING: WL Rank[%d] Byte[%d]: Rising[%d] Falling[%d]"
3983685135,3,WARNING,ras.c,"0x%08X: no fault data for type 0x%02X (pw_ras_interrupt_req was 0x%08X)"
3983357714,1,ERROR,log_emask_imask_regs.c,"A_EMASK: 0x%x"
3983331055,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustVdm at Window. Window : %d"
3980623908,6,ERROR,fw_img_auth.c,"Image with incompatible HW Architecture detected. Running DIMM Info: Vendor ID (0x%x), Device Id: (0x%x), Revision Id (0x%x). ""Image header under authentication Info: Vendor ID (0x%x), Device Id: (0x%x), Revision Id (0x%x)"
3979997991,0,ERROR,dpa_verify_error_handler.c,"Retrying the command to channel failed!"
3979310286,3,ERROR,algo_write_leveling.c,"SXP Coarse WrLvl failed. Rank[%d] BytePassMask[%x] BytePassFlag[%x]"
3978805447,2,ERROR,sxp_trims.c,"0x50D register read failed. Can't check media type on Rank: %d, Die: %d"
3978612269,0,INFO,core_dump.c,"Sha Hash failed for coreDumpInfo"
3976992071,0,ERROR,log_refresh_engine_start.c,"Refresh engine started!"
3973845776,1,ERROR,nlog_set_ddrt_io_init_info.c,"D_FW_STATUS: 0x%x"
3972808341,0,ERROR,dpa_verify_error_handler.c,"PDA read from DRAM matches the original error PDA, go transaction fatal!"
3971981630,1,DEBUG,commands.c,"Size of device characteristics - %d"
3970121823,0,ERROR,power_event_at_image_auth.c,"Image sync timer was not initialized"
3969544209,2,DEBUG,hal_pmic_rail.c,"Waiting %d microseconds for PMIC rail 0x%x voltage ramp to complete"
3968715528,0,ERROR,power_event_at_image_sync.c,"Image sync timer was not initialized"
3966709385,0,WARNING,dfx.c,"Uploaded header was invalid"
3965958830,1,ERROR,spd.c,"Invalid 3DXP DeviceID Fconfig token value: 0x%x"
3965071251,0,DEBUG,task_security.c,"SECURITY_SHA256DMA"
396392962,1,ERROR,core_dump.c,"PowerStateEvents Raw: 0x%x"
3963087159,0,STATUS,command_software_triggers.c,"Disabled package sparing software trigger"
396158455,1,ERROR,command_features.c,"Bad CEL entry - can't determine restrictions: %d"
3960621371,0,STATUS,feature_state_data.c,"Feature State Data Needs Initialization - Creating Default"
3959583163,0,ERROR,mm_free_block_expansion.c,"MediaInterface handle returned NULL. AIT Read for cold block selection failed."
3958911692,2,ERROR,hal_pmic_rail.c,"Failed to apply value 0x%x to power rail register 0x%x"
395728170,12,INFO,sxp_scheduler.c,"SXP Stepping ID R[%d]:%x,%x,%x,%x,%x,%x,%x,%x,%x,%x,%x"
3956778875,2,ERROR,core_dump.c,"OtherStateInfo - Shutdown Time       : 0x%08x_%08x"
3956311405,1,INFO,reg_flow.c,"RF Table Version[0x%x]"
3956064900,1,ERROR,spi.c,"Erase failed on 0x%08X"
3955312871,2,ERROR,fw_image_sync.c,"Image_Sync_Completed called in state (%d) with an unexpected status: %d"
3954529882,0,ERROR,key_management.c,"Failed to generate the passphrase based derived key"
3952795587,0,WARNING,task_command_handler.c,"Error: Media Not Ready"
3951613236,0,STATUS,command_software_triggers.c,"Unsafe shutdown software trigger is disabled"
3949551666,0,WARNING,task_command_handler.c,"NULL Command"
3949521431,0,ERROR,i2c_bus_manager.c,"I2C bus manager invoked with unknown bus request status"
394751012,0,INFO,command_log.c,"DMA Transfer Complete"
394625250,1,ERROR,kechika_river_pmic_driver.c,"PMIC did not assert power good on all rails. Power Good Status 0x%X"
3945234440,2,DEBUG,platform_config_data.c,"Subtracted Address: 0x%08X_%08X"
3944666165,1,DEBUG,kechika_river_pmic_driver.c,"Waiting %d microseconds for PMIC voltage ramp and settling time to complete"
3943686886,0,ERROR,power_budgeting_engine.c,"Energy meter missed one accumulation window"
3943100192,1,ERROR,feature_state_data.c,"Wrong power event notification: %d"
3942827844,2,ERROR,ddrt_scheduler.c,"ERROR: DDRT PLL did not lock before timeout MSC_FNVIO_INIT_CONTROL_1.DDRTPLLLOCKED=0x%X, DDRT_CKDET=0x%X"
3941091361,1,ERROR,wear_level_move.c,"WearLevelMove_Dispatch unexpected AIT read msg:%x"
3937700377,0,ERROR,format_device.c,"Cmd Format Device, failed to erase PMIC init reason."
3936888309,1,ERROR,chn_no_cmd.c,"Channel no command flow started but there's no fault data, pw_ras_interrupt_req: 0x%X"
3935043203,0,ERROR,core_dump.c,"Cpu Registers:"
3934791314,1,DEBUG,spare_block.c,"Calculating remaining spare blocks: %d"
3934421124,0,DEBUG,command_features.c,"Set Features: Address Range Scrub"
3933238180,4,ERROR,kernel.c,"D_PWM_STS:0x%08X  D_PWM_MASK:0x%08X  NC_APIC_ISR:0x%08X  NC_APIC_IRR: 0x%08X"
3931606769,2,ERROR,thermal_manager.c,"Rank %d had all failedDies for Temp reading 0x%x"
3931180761,0,DEBUG,aes_bulk_encryption_selftest.c,"Read the decrypted 256 Byte AES Bulk encryption test buffer from SXP executed"
3929871317,28,STATUS,hal_pmic_rail_cwv.c,"Requested Update Values: A[%d][%d][%x] B0[%d][%x] B1[%d][%x] C[%d][%x] D[%d][%d][%x] E[%d][%x] F[%d][%x] G[%d][%x] H0[%d][%x] H1[%d][%x] J[%d][%x] K[%d][%x] L[%d][%x]"
3929858428,2,WARNING,get_fconfig.c,"DFX Get Fconfig incorrect transfer type: 0x%X expecting: 0x%X"
3928697901,0,INFO,refresh.c,"Starting Refresh Engine"
3928413624,0,STATUS,thermal_manager.c,"Entering thermal throttling"
3927669156,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr7: 0x%x"
3926433564,0,INFO,power_state.c,"Surprise Reset Exit Clock Enable"
3926048994,3,ERROR,power_state.c,"PowerState_AddListener: Max Power Listeners Reached - %d, add New Listener 0x%x failed with Transition Event = %d"
3925703504,0,ERROR,error_logging.c,"Max Entries == 0, would result in division by 0, don't complete request"
3925293893,7,ERROR,cmd_timer_end.c,"CMDCC: %d %02x %02x %08x %u %u %u"
3925022501,0,ERROR,host_throttle.c,"HostThrottle_Initialize called"
3923817183,0,ERROR,log_vsm_state.c,"Dynamic VDM Stop Media Access state: success."
392136529,0,WARNING,command_features.c,"Unable to set 4K partition sizes"
3919917613,2,ERROR,power_budgeting_engine.c,"DIMM Average Power [%d mW] has exceeded high watermark threshold [%d mW]"
3919688156,0,ERROR,ait.c,"Ait_LookupAitEntryDpaLevel was called for a level of N-3, should never happen!"
3918425412,0,ERROR,fw_init.c,"Insecure SPI FW Header was not erased!"
3918131670,0,ERROR,write_count_histogram.c,"Write Count Status: WLM pending counter overflowed"
3914048929,0,DEBUG,wear_level_move.c,"FBE AIT DMA Line Callback"
3913081875,1,INFO,read_disturb.c,"Read Disturb Random Interval is not 1 less than power of 2: 0x%X"
3911087513,2,INFO,task_command_handler.c,"Duplicate Cmd Detected: 0x%x -> Completing with Status [0x%x]"
3910482169,0,ERROR,kechika_river_pmic_driver.c,"Cap self test setup failed."
3908124589,1,DEBUG,power_state.c,"Signal Power Event: %d"
3907679136,0,ERROR,ait_dram.c,"DRAM load NOT started due to media is not trained or disabled!"
3907225476,0,WARNING,command_inject_error.c,"Media temperature error is cleared because error injection is disabled"
390671506,0,ERROR,ait_dram.c,"DRAM loading completes!"
3906000715,3,ERROR,security_error.c,"Security Key Error Log: Valid bit not set! base = 0x%x, lo = 0x%x, hi = 0x%x"
39056926,1,ERROR,nlog_region_lock.c,"D_DBUF_REG_LOCK: 0x%08x"
3905423608,0,INFO,ddrt_training.c,"DdrtTraining_StartTraining!"
3905359074,0,ERROR,infoturn_error_log.c,"QueueInfoturnErrorLog: Buffer address is 0x0"
3902782307,0,WARNING,task_command_handler.c,"Unsupported command"
3902673049,0,ERROR,command_fw_update.c,"Small Payload: DMA read of block of image failed"
390242884,1,ERROR,log_ddrt_dll_csr.c,"MSC_FNVIO_DDRTDLL_CSR: 0x%x"
3901353817,1,ERROR,ait_nm3_csr.c,"AIT N-3 entry has error but no valid bit set, going DIMM FATAL! Header: 0x%x"
3901346387,0,ERROR,key_management.c,"Wrapping PM-RK with S3 wrapping key failed"
3899845555,1,ERROR,kernel.c,"CFI Exception occured at address: 0x%08X"
3899517042,0,STATUS,command_inject_error.c,"Disabling poison on 4 cache lines"
3899037383,2,INFO,mmrc_parser.c,"MMRC Bus %d Revision %d"
3898816554,1,ERROR,feature_state_data.c,"DMA_STATUS_ERROR encountered while flushing feature state data ID: %d."
3897358201,0,DEBUG,task_security.c,"SECURITY_GENERATE_RANDOM_256BIT_VALUE"
3896099215,1,ERROR,wear_level_move.c,"Wear Level Move: Relocate Block reported an error %d on move operation"
3895119624,1,ERROR,wear_level_move.c,"AIT Read Callback DMA Failure %d"
3892041627,2,STATUS,commands.c,"BIOS Api version set to 0x%X, FW API: 0x%X"
3891492019,2,ERROR,dpa_verify_error_handler.c,"PDA read from DRAM ait copy is 0x%08X_0x%08X"
3890408695,2,ERROR,algo_write_leveling.c,"SXP Coarse WrLvl failed rank[%d] byteFailArray[0x%X]"
3890238510,1,ERROR,nlog_set_ddrt_io_init_info.c,"MSC_FNVIO_INIT_CONTROL_1: 0x%x"
3883762007,5,ERROR,update_firmware.c,"FW Update found that the Staging FW Info got corrupted leaving FW Update initialization in a bad state Staged FW Version %02X.%02X.%02X.%04X FW Type %d"
3883403378,1,ERROR,thermal_engine.c,"Forced temperature calibration workaround, set: %08X"
3883208737,0,ERROR,power_budgeting_engine.c,"Energy meter 1.2V Coulomb count overflows."
3881239682,0,ERROR,key_management.c,"Wrapping PM-RK with S3 wrapping key failed"
387962448,2,ERROR,pmic.c,"PMIC Read Failure: Address 0x%X, Error Code %d"
3878861381,0,ERROR,format_device.c,"Invalid FW State. Failed to preserve lifetime stats"
3876824341,2,ERROR,sxp_rcven_training.c,"Fine Rcven failed rank[%d] byte[%d]"
3876157535,1,ERROR,core_wear_level_move.c,"Wear Level Move: Relocate Block reported an error %d on move operation"
3873650827,1,DEBUG,commands.c,"Size of IdentifyData - %d"
3867068142,0,STATUS,update_firmware.c,"Clearing the previous FW stage information."
3867029823,0,ERROR,fconfig.c,"FconfigSpiLayout->header.dwordLen beyond size of SRAM structure."
3866043478,0,ERROR,command_log.c,"DMA Submission entry failed to queue."
3863455096,0,INFO,ait_dram.c,"Initialize the DRAM Load"
3861722552,0,ERROR,cpgc.c,"CPGC failed to complete"
3858451625,1,ERROR,i2c_bus_manager.c,"Invalid core message 0x%X passed to I2C bus manager"
3858351206,1,ERROR,core_dump.c,"Stack address not found in stack regions! Failed to get call trace. addr: 0x%08x"
3857554875,1,ERROR,data_path_error.c,"DS FIFO U/O Flow Errors: 0x%08X"
3857516980,0,ERROR,fw_activate.c,"FW activate failed to read runtime data"
3853462810,0,ERROR,die_error_emulator.c,"DieErrorEmulator: Not supported on DIMMs that do not have common ID applied."
3852985798,1,ERROR,hardware_wear_level_move_engine.c,"WLM Threshold value (%d) is invalid."
3852915803,1,ERROR,hardware_wear_level_move_engine.c,"FBLE Opportunistic Threshold value (%d) is invalid."
3852452190,0,DEBUG,task_command_handler.c,"Task_CommandHandler: Background Operation Running"
3852178102,0,ERROR,security_interface.c,"Couldn't queue HMAC security request"
385073273,0,ERROR,fw_init.c,"Going DIMM fatal because the criteria for an unfinished shutdown flow has been met"
3850555486,2,ERROR,core_dump.c,"OtherStateInfo - Shutdown Time       : 0x%08x_%08x"
3849558335,1,ERROR,nlog_set_ddrt_io_init_info.c,"DA_DDRT_PLL_CTRL: 0x%x"
384777339,1,ERROR,get_ait_info.c,"A_AIT_TOP_BASE_ADDR_L: 0x%x"
3845570964,1,ERROR,write_count_histogram.c,"Error: Invalid stats mode: %d"
3844075839,0,ERROR,task_error_handler.c,"AIT Scrub fails at COPY_LINE state"
3842380675,0,DEBUG,command_pmon.c,"Set Features: PMON Registers"
3842284070,0,WARNING,command_features.c,"Invalid payload configuration"
3840852578,0,ERROR,hal_pmic_rail.c,"Couldn't read the current rail settings, skipping PMIC Rail Init"
3839387987,1,ERROR,sxp_device_access.c,"Could not properly set the SXP Device Select IDs for rank[%d]"
3838942565,0,DEBUG,aes_bulk_encryption_selftest.c,"Write Bulk_Encryption source data to SXP"
383892619,1,ERROR,task_media_interface.c,"We received a DMA completion event, but there is a DMA active afwe_status: 0x%X"
3838281912,4,STATUS,mm_block_move.c,"HW WLM Pause timeout detected. Source DPA: 0x%08X_0x%08X Destination DPA: 0x%08X_0x%08X"
3837576240,2,ERROR,dynamic_vdm.c,"Dynamic_VDM Trim Error rank : %d, die : %d"
3837319287,1,ERROR,nlog_region_lock.c,"D_PM_SIZE_H: 0x%08x"
3836457667,0,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustIRst one or more refreshes were unsuccessful"
3835428009,0,WARNING,dfx.c,"No module uploaded - unable to execute"
3835387922,1,ERROR,ltec.c,"LTEC failed to apply VID code updates after %d attempts."
3834461124,2,ERROR,datastore.c,"Detected invalid datastore size: %d for datastore id: %d"
3833872745,1,ERROR,nlog_set_ddrt_io_init_info.c,"MSC_FNVIO_INIT_CONTROL_1: 0x%x"
3833658845,0,INFO,core_dump.c,"Sha Hash failed for csrDumpListTable"
3832467888,0,ERROR,sxp_scheduler.c,"IoTrainReset: Bit never flipped to 1"
3832147595,0,ERROR,fw_init.c,"Dynamic and Adaptive VDM features have both been disabled!"
3831445938,1,ERROR,log_emask_imask_regs.c,"AITDR_RAS_EMASK: 0x%x"
3831391242,0,ERROR,sxp_training.c,"Writing Training Report to SPI failed"
383029833,0,ERROR,reg_flow.c,"SPI table authentication failed!"
3829255544,0,WARNING,fw_image_sync.c,"Non loaded slot signature invalid"
3824805715,1,ERROR,core_wear_level_move.c,"Free Block Expansion: Relocate Block reported an error %d on move operation"
382161413,2,ERROR,security_error.c,"Security Key Error, unexpected error bit set: ferr num %d, error bit %d!"
3819431674,0,WARNING,command_features.c,"Address Range Scrub: Invalid Enable"
3817573517,1,ERROR,kechika_river_pmic_driver.c,"PLI Cap Value is Low. Self Test Time : %d"
3817564782,0,ERROR,sxp_training.c,"Sxp Mrc Programming Error: No Table Date Found"
3816699816,2,ERROR,sticky_die.c,"Partition unsticking SxpCmd_SelectId failed on rank: %d, die: %d"
3816182506,3,ERROR,sxp_scheduler.c,"read SXP_REG_TRNPATTERN failed! value = 0x%x, die = %d, rank = %d \n"
3815141909,0,WARNING,command_fw_update.c,"Invalid packet number"
3814988286,6,ERROR,nc_bus_isr.c,"Nanocore SRAM RMW error. Error Count 0x%08X SRAM Rank 0x%08X Error Address 0x%08X Error Data 0x%08X Parity 0x%08X IRQ status 0x%08X"
3814505750,0,ERROR,write_count_histogram.c,"Start address > DIMM capacity"
3810742972,1,ERROR,nlog_region_lock.c,"D_PM_REG_LOCK: 0x%08x"
3809860792,1,ERROR,sxp_init.c,"Sxp_FineWriteLeveling failed rank: %d"
3808999802,2,ERROR,command_features.c,"System Time Set at boot. Time: 0x%x_%x"
3807556481,1,INFO,fw_image_sync.c,"Sync Completed Successfully with %d authentication failures"
3806029822,0,WARNING,command_features.c,"Unable to enable Address Range Scrub - Currently in progress"
3804647470,1,INFO,kechika_river_pmic_driver.c,"PLI Cap value is good. Self Test time: %d"
3801569635,0,ERROR,crypto_selftests.c,"3DXP XTS-AES-256 Decryption self-test failed!"
3800787229,0,ERROR,aes_bulk_encryption_selftest.c,"*** FAIL *** decryption test"
3799827832,0,INFO,refresh.c,"Getting Refresh Interval"
3795223597,0,ERROR,power.c,"PMIC Rail D got svid fuse value 0x0"
379419071,1,ERROR,core_wear_level_move.c,"FW is aborting WLM on powerloss. WLM Dest DPA 0x%08X"
3791043944,0,DEBUG,platform_config_data.c,"PCD_DmaDataSmallPayload: Enter"
3790547346,2,ERROR,wear_level_move.c,"WearLevelMove_Transition Could not refresh all source lines of pda 0x%08X_%08X"
3789526814,1,ERROR,core_dump.c,"SKU ID  -  0x%08x"
3789474503,0,ERROR,sxp_commands.c,"RDWR_BUF_CTRL REQ did not return to idle"
3788470302,1,ERROR,task_media_interface.c,"DMA command failed with AHB error twice in a row! statusBitField: 0x%x"
3786522372,0,ERROR,command_inject_error.c,"Media temperature error injection is disabled"
378556549,0,INFO,ddrt_scheduler.c,"DDRT_RestoreRegisters!"
3785462825,1,ERROR,log_ddrt_io_init.c,"MSC_SPARE_CTRL: 0x%x"
3784625847,1,ERROR,nlog_notify_ddrt_normal_mode.c,"DA_IO_PCR_PERMISSIONS0: 0x%x"
3782650075,0,INFO,smart.c,"Updating vendor page with Intel details"
3782535772,2,ERROR,io_csr.c,"IO CSR invalid parameter rank = 0x%x, byte = 0x%x"
3782197060,0,ERROR,dfx.c,"Large payload upload logical read failed!"
3781787377,0,ERROR,fw_init.c,"Injection module from SPI was not loaded"
3781630592,2,ERROR,sxp_init.c,"Fine Write Leveling Training failed, Rank: %d Training type: %d"
3780560267,1,ERROR,log_emask_imask_regs.c,"MSC_IMASK: 0x%x"
3779372641,1,ERROR,ddrt_training.c,"DdrtTraining_StartTraining- Failure at DDRT Sense Amp Calibration CNT=%d"
3777396339,0,DEBUG,warm_reset.c,"Warm Reset Flow Retrain DDRT"
37768261,9,ERROR,task_error_handler.c,"Uncorrectable error! Source Transaction Type 0x%02X; Initial VDM 0x%02X; Final VDM 0x%02X; Fault data 0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
377673659,1,ERROR,kechika_river_pmic_driver.c,"Invalid pmic rail passed to UpdateRailValue. rail: %d"
3775935833,0,DEBUG,task_security.c,"SECURITY_KEY_MANAGEMENT_INIT"
3775232677,0,INFO,fw_image_sync.c,"Initialize the image sync"
3774852479,0,DEBUG,key_management.c,"Initializing Key Values"
3773570742,0,ERROR,ait_dram.c,"DRAM load NOT started due to unsuccessful dram training!"
377267262,0,ERROR,command_log.c,"CEL entries did not fit in the buffer."
3771982823,2,ERROR,thermal_engine.c,"Rank read of SXP_SR1 failed on rank:%d fail die map:0x%04x"
37711939,0,WARNING,command_features.c,"Both PM and 2LM disabled SKU"
3770714573,0,DEBUG,command_features.c,"Set Features: Optional Configuration"
3766575662,0,ERROR,dpa_verify_error_handler.c,"PDA read from DRAM matches the original error PDA, go transaction fatal!"
3762840126,0,ERROR,leaky_bucket.c,"Unknown stat requested"
3760803007,1,ERROR,task_high_priority_message_handler.c,"Message Id is out of range. HPMH Message Id: 0x%X."
3760084419,0,ERROR,fw_activate.c,"FW activate failed to suspend the power budgeting engine"
3759972031,0,WARNING,update_firmware.c,"Staged Major, Minor, or Security version is older than running FW. FW downgrades are not allowed."
3759532628,5,ERROR,ddrt_scheduler.c,"ERROR: DDRT PLL did not lock before timeout MSC_FNVIO_INIT_CONTROL_0=0x%X, MSC_FNVIO_INIT_CONTROL_1=0x%X, D_DDRT_DCLK_CTRL=0x%X, MSC_FNVIO_VISIBILITY_CSR=0x%X, MSC_PLL_CTRL=0x%X"
3758703480,0,DEBUG,command_features.c,"PCD Get Partition Size Called"
3756443592,1,ERROR,dma_polled.c,"Completed in-flight DMA inside polled DMA! Inside PLI: %d"
3756332230,0,ERROR,platform_config_data.c,"Invalid DMA direction"
3756243980,5,INFO,task_error_handler.c,"0x%08X: channel command: 0x%08X, 0x%08X, 0x%08X, 0x%08X"
3754867881,0,WARNING,command_features.c,"Invalid DDRT payload"
3754249999,1,ERROR,core_dump.c,"CallStack Logging started: 0x%X"
3752424199,1,ERROR,kechika_river_pmic_driver.c,"UNKNOWN RTK PMIC Stepping - Product Stepping: [0x%X]"
3752331104,0,ERROR,sxp_init.c,"Sxp_SenseAmpcalibration failed"
3751573825,1,ERROR,log_emask_imask_regs.c,"A_IMASK: 0x%x"
3749345685,1,ERROR,fw_init.c,"Previous boot PowerStateEvents is 0x%x"
374768961,0,ERROR,feature_state_data.c,"Feature State Data Needs Initialization - Creating Default"
3747658022,0,WARNING,fw_img_auth.c,"Image type is invalid"
3747265365,2,ERROR,command_features.c,"Performance Knob %d is updated with value %d"
3744991523,1,ERROR,power_state.c,"PowerState_SignalPowerEvent: Unexpected Power State event [0x%x] detected."
3744737471,0,ERROR,sxp_scheduler_init.c,"Aep Scheduler Init failed"
3740641328,1,ERROR,power_budgeting_engine.c,"Invalid time constant %dms requested. Power budgeting engine applies the value but does not store in FW state."
3740080186,1,ERROR,ras.c,"RAS Log: Valid bit not set - DN_LOG_RDATA_E2E_CRC_ERR_1 = 0x%x"
3739776205,2,STATUS,hal_pmic_cfg.c,"PMIC Manufacture ID: 0x%X    Product Stepping: 0x%X"
3737453531,1,ERROR,log_power_event_start.c,"RPQ_WDB_STAT_EMPTY: 0x%x"
3736525103,3,ERROR,sxp_commands.c,"Error writing to register addr: 0x%04x rank: %d die %d"
3735220044,0,ERROR,die_error_emulator.c,"DieErrorEmulator: DQ failure not supported due to package migration is in progress/already complete."
3734622490,1,ERROR,hal_pmic_cap_test.c,"PLI Cap Value is Low. Self Test Time : %d"
373384324,0,INFO,wear_level_move.c,"Invalid address value"
3732915078,1,WARNING,ras.c,"WdbUe on Banks[0x%x]"
3730791046,0,WARNING,platform_config_data.c,"DMA transfer failed to complete"
3730314007,3,STATUS,thermal_manager.c,"Controller: %d C; Highest Die Temp: %d C; DRAM Sensor Status: %d (0 = 1x refresh, 1 = 2x refresh, 2 = Shutdown)"
3729996894,0,DEBUG,warm_reset.c,"Warm Reset Exit Clock Enable"
3727120300,0,ERROR,wear_level_move.c,"Invalid Firmware State Data, Wear Level Resume State Machine could not complete!"
372583539,1,ERROR,ras.c,"RAS Log: Valid bit not set - DS_LOG_WDATA_POISON_1 = 0x%x"
3724768229,1,ERROR,hardware_wear_level_move_engine.c,"FBLE Demand Threshold value (%d) is invalid."
372470948,2,ERROR,sxp_decode_media.c,"Unrecognized media on Rank: %d, Die: %d"
3724623681,1,ERROR,log_power_event_start.c,"DRDP_WCRD_CONFIG: 0x%x"
3723297419,1,ERROR,hal_pmic_cap_test.c,"CAP test error - communication problem - promoting state from: %d - no further cap tests for this boot"
3723035500,0,INFO,power_state.c,"Warm Reset Flow PM Idle"
3721472766,3,ERROR,thermal_manager.c,"Controller: %d C; Highest Die Temp: %d C; DRAM Sensor Status: %d (0 = 1x refresh, 1 = 2x refresh, 2 = Shutdown)"
3717643479,0,ERROR,task_error_handler.c,"Completing AIT Scrub"
3716732899,0,STATUS,feature_state_data.c,"FSD Access Fconfig is set to SRAM, skipping FSD load!"
3715173705,9,ERROR,dma_polled.c,"DMA Polled STYPE AIT UECC. Source Transaction Type 0x%02X; Initial VDM 0x%02X; Retry Index 0x%02X; Fault data 0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
3713286080,0,ERROR,security_interface.c,"Couldn't queue EAU security request"
3712620794,0,WARNING,command_features.c,"Address Range Scrub: Invalid Address"
3712223287,0,WARNING,debug_log_data.c,"Dma transfer not completed!"
3709864068,0,WARNING,command_features.c,"The DDRT Alert Policy data is not valid - non-zero reserved bits!"
3707856130,1,DEBUG,core_wear_level_move.c,"Transition FBE State Machine : %d"
3707300116,0,DEBUG,command_features.c,"Get Admin Features: System Time"
3704938247,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz4: 0x%x"
3703030370,0,ERROR,example_pimf_command.c,"Congrats! You made it inside a pIMF module!"
3702723644,0,WARNING,power_loss_log.c,"Did not read from power loss log because sxp training, context block init, or ait init failures"
37014553,0,WARNING,security_interface.c,"SHA RESET security request timed out"
3700915535,0,DEBUG,pmic.c,"PMIC Write Error"
370029833,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingRc0E: 0x%x"
3699238528,2,INFO,task_command_handler.c,"Command Completed on mb[%d] with Status: 0x%08x"
3698185018,2,ERROR,assert.c,"*** ASSERT *** module: (decimal) %d Line: %d"
3696971528,1,ERROR,core_dump.c,"DDRT MMRC Version: %d"
3695875813,1,ERROR,power.c,"PMIC Rail D set to [%d] as W/A since svid fuse returns 0x0"
3694889298,0,INFO,refresh.c,"Resuming Refresh"
3693589861,0,ERROR,sxp_scheduler_init.c,"Unsupported SXP Device Type or Device ID read error"
3690529588,0,WARNING,dfx.c,"Mismatching module build platform and firmware build platform"
3690465689,0,ERROR,power_budgeting_engine.c,"FW was unable to process energy meter data in a timely manner"
3690344702,0,WARNING,core_dump.c,"DMA transfer failed to complete"
3690178860,0,WARNING,key_management.c,"Security Metadata Interface pointer is NULL"
3688432822,1,DEBUG,breakpoint.c,"Breakpoint: %d"
3687938442,0,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustLegacyVdm one or more refreshes were unsuccessful"
3687831304,0,DEBUG,command_features.c,"Get Admin Features: Viral Policy"
3686605326,0,ERROR,task_media_interface.c,"Unable to submit dma request. Requeuing back into the free queue."
3685752053,0,ERROR,wear_level_move.c,"BBM AIT Read Callback DMA Failure"
3684804835,1,ERROR,wear_level_move.c,"BBC AIT Callback DMA Failure, state = %d"
3682803841,0,DEBUG,command_features.c,"SS: Set BIOS Security Nonce"
3681969716,0,DEBUG,task_security.c,"SECURITY_EXPONENTIATE"
368136174,1,ERROR,kechika_river_pmic_driver.c,"PMIC Error returned while updating Rail[%d]"
3680976816,1,ERROR,update_firmware.c,"SPI request failed on address 0x%08X"
3678962489,1,DEBUG,task_command_handler.c,"Setting opcode as: 0x%08X"
3678566716,0,WARNING,format_device.c,"REBUILD_MD security request timed out"
3678317818,3,ERROR,task_media_interface.c,"More requests exist then should be possible. Free(%d) WIP(%d) Pending(%d)."
3675857084,0,WARNING,command_features.c,"Operating frequency is invalid"
3675693513,5,ERROR,thermal_manager.c,"Stuck Refresh pointer observed! RP : 0x%08X PC_LOG_RFRSH_UNEXP_0 0x%08X PC_LOG_RFRSH_UNEXP_1 0x%08X;  PC_LOG_RFRSH_UNEXP_2 0x%08X PC_LOG_RFRSH_UNEXP_3 0x%08X"
3674425788,1,ERROR,sxp_trims.c,"PCL reg access not supported for DIMMs with ranks %d"
3672741502,0,ERROR,fw_init.c,"Setting media disabled after FwState load"
3670560126,0,ERROR,sxp_rmt_tests.c,"RAS Tx Vref Min Mask Test Failed"
3669256060,1,ERROR,wear_level_move.c,"FreeBlockExpansion_Dispatch unexpected AIT get line msg:%x"
3668121906,2,ERROR,datastore.c,"Incorrect source datastore. Expected: %x, Found: %x"
3667444307,4,ERROR,dynamic_vdm.c,"Max window adjustment %d for Far AdwlVdm rank %d die %d deck %d is invalid"
3665546434,0,DEBUG,crypto_selftests.c,"Size of data for the 3DXP XTS-AES-256 Decryption Test exceeds size of buffer."
366438423,0,DEBUG,kechika_river_pmic_driver.c,"Cap test Timer Callback"
3663804958,1,ERROR,update_firmware.c,"Handler could not handle this event. Event type: %d"
3661371359,0,WARNING,fw_img_auth.c,"Header version field is invalid"
3660726262,1,WARNING,task_error_handler.c,"unexpected fault type 0x%02X"
3660151020,0,WARNING,core_wear_level_move.c,"Source PDA doesn't match WDPQ PDA - Block has moved already"
3659724794,1,ERROR,core_dump.c,"FwDebugData - version       : %d"
3658189930,1,ERROR,data_path_error.c,"SRAM read parity error is found at SRAM address 0x%x, retry the request!"
3658010557,0,ERROR,format_device.c,"Cmd Format Device, failed to set initial write count to non-zero from DRNG."
3656191888,2,ERROR,format_device.c,"Cmd Format Device, DMA returns a failure status. ""sxp address:  0x%08X_%08X"
3654738532,2,ERROR,wear_level_move.c,"AitPolled_Write Failed on Entry Address 0x%08X_0x%08X: "
3653438746,1,ERROR,core_dump.c,"FwDebugData - nlogSpiBackupValid : %d"
3652731044,1,ERROR,media_manager_engine.c,"WLM Threshold value (%d) is invalid in SetQueuePolicy during MediaManagerInit"
3652536044,2,ERROR,commands.c,"Cmd Format Device, DMA returns a failure status. sxp address:  0x%08X_%08X"
3651921043,0,WARNING,command_features.c,"Security state is frozen or locked"
365118261,0,ERROR,key_management.c,"Forward expansion of VM keys failed"
3650505340,1,ERROR,data_path_error.c,"A FIFO U/O Flow Error 1 : 0x%08X"
3650373498,0,DEBUG,power.c,"Caller used incorrect Power Type to set Power Threshold"
3649856616,3,ERROR,algo_write_leveling.c,"DRAM External Coarse WrLvl failed rank[%d] bytePassMask[%x] bytePassFlag[%x]"
3647632902,2,WARNING,fconfig.c,"Set Fconfig failed Token: 0x%X, Status: 0x%X"
3643211148,1,ERROR,task_media_interface.c,"DMA command %x failed, PSN error"
3642550350,0,INFO,refresh.c,"Suspending Refresh and Saving Pointers"
3642425822,1,ERROR,power_event_at_image_auth.c,"Stopping image sync in state: %d"
3641184298,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustS26Vdm called with invalid vdmWindow : %d"
3638993528,0,ERROR,write_disturb_engine.c,"WriteDisturbEngine_PollStartBit reached time limit"
3638795264,0,DEBUG,task_security.c,"SECURITY_SET_PASSPHRASE"
363876228,1,DEBUG,host_interrupt.c,"Current blocks: 0x%x"
3637220793,0,ERROR,thermal_manager.c,"AIT DRAM temperature sensor read failure"
3636340655,0,ERROR,ltec.c,"LTEC normal mode update missed due to I2C bus error."
3636045643,2,STATUS,command_features.c,"System Time Set at boot. Time: 0x%x_%x"
363407423,1,ERROR,sxp_init.c,"Coarse RcvEn Training failed, Rank: %d"
3633359450,1,ERROR,data_path_error.c,"A FIFO U/O Flow Error 0: 0x%08X"
3633069585,0,ERROR,infoturn_error_log.c,"InitorRetrieveInfoturnErrorLog: Buffer address is 0x0"
3632285732,2,ERROR,sxp_init.c,"Fine Write Leveling Training failed, Rank: %d Training type: %d"
3630591950,0,DEBUG,fw_image_sync.c,"Timer Callback"
3630062004,0,ERROR,fw_init.c,"Setting media disabled after FwState load"
3629193578,0,WARNING,command_features.c,"Not a Package Sparing capable SKU"
3628871061,1,ERROR,power_state.c,"PC6: Unexpected Power State event [0x%x] detected."
3627305254,1,INFO,power_budgeting_engine.c,"Energy Meter has missed %d I2C sequences in the current accumulation window, initiating safe mode"
3626644871,1,ERROR,log_power_event_end.c,"D_PWM_MASK: 0x%x"
362645667,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz4: 0x%x"
3625133004,0,ERROR,sxp_training.c,"Sxp Mrc authentication failed!"
3622329505,0,DEBUG,task_security.c,"SECURITY_REBUILD_MD"
3618428192,2,INFO,command_features.c,"System Time set, boot up occured at %d %d"
3616529778,0,STATUS,kechika_river_pmic_driver.c,"CAP Test result already Critical, not initiating any more testing\n"
3614448869,0,DEBUG,command_features.c,"PCD Get Data DDRT"
3608808088,2,DEBUG,core_dump.c," Data[0x%08x]: 0x%08x"
3607449354,0,WARNING,command_features.c,"Invalid PCD Retrieve Option"
360725785,1,DEBUG,core_dump.c,"Address provided was not found in searched regions: 0x%X"
3606698576,10,ERROR,sxp_commands.c,"SXP Reg Read Error D[%d]MSR[%x]:%x,%x,%x,%x,%x,%x,%x,%x"
3606475483,1,ERROR,sxp_init.c,"Unable to initialize media latencies. Invalid media device ID %d"
360412339,0,ERROR,skip_img_sync_at_ddrt_training.c,"Ddrt is not trained"
3601330892,0,WARNING,task_command_handler.c,"Mailbox Failure"
359859706,4,ERROR,host_interrupt.c,"Packet ACK for DDR-T interrupt timed out- erid = 0x%02X | type=%d | D_DDRT_INTR_CTRL= 0x%X | D_DDRT_INTR_STS=0x%X"
3598284538,0,ERROR,power_loss_log.c,"Error translating PLI log buffer B's dpa address to pda"
3597186892,0,DEBUG,overwrite_dimm.c,"Overwrite DIMM ait write Callback"
3594602861,0,WARNING,command_features.c,"Unable to enable Address Range Scrub - Currently in progress"
3594377492,0,DEBUG,task_command_handler.c,"Task_CommandHandler: Host is trying to call a disabled command."
3592533400,0,INFO,overwrite_dimm.c,"Starting Overwrite DIMM"
3592245563,1,ERROR,fconfig.c,"ParseAndUpdateTokens failed zero length Token: 0x%X"
3592242185,1,ERROR,data_path_error.c,"Data path Error: This error %d causes DIMM Fatal!"
3592050108,1,ERROR,log_emask_imask_regs.c,"DS_IMASK: 0x%x"
3588782652,0,ERROR,pll_gating_failure_trigger.c,"PLL gating was desynchronized."
3588148018,0,ERROR,ddrt_training.c,"Ddrt_FineRcvenTraining failed"
3588107945,2,ERROR,thermal_manager.c,"ThermalComp Thermal Shutdown Comp[%d] Temp[%d]"
3587697473,0,ERROR,core_dump.c,"Mailbox Tracking Info:"
3586045100,2,INFO,ras.c,"0x%08X: fault data: type 0x%02X"
3585948543,0,WARNING,smart.c,"No supported vendor found"
3585765447,4,ERROR,algo_write_leveling.c,"WARNING: WL Rank[%d] Byte[%d]: Rising[%d] Falling[%d]"
3585247450,2,ERROR,hal_pmic_rail_cwv.c,"PMIC did not assert power good on all rails. Power Good Status0: 0x%X, Status1: 0x%X"
3582869151,1,ERROR,ait_nm3_csr.c,"AIT N-3 entry has error but no valid bit set, going DIMM FATAL! Header: 0x%x"
3582347527,2,ERROR,write_count_histogram.c,"Received more than maximum supported steps. Number of steps: supported = %d, requested = %d"
3582288898,0,DEBUG,command_features.c,"Get Features: DDRT Alerts"
3581669736,2,DEBUG,platform_config_data.c,"dstAddress: 0x%08X_%08X"
3580701267,2,ERROR,algo_write_leveling.c,"Fine WrLvl failed Rank[%d] Byte[%d]"
3580340828,1,ERROR,pmic.c,"PMIC Read Error : %d"
3580290500,0,WARNING,command_features.c,"The DDRT Alert Policy data is not valid - low and high priority both set!"
3579148535,0,WARNING,wear_level_move.c,"Source PDA doesn't match WDPQ PDA - Block has moved already"
3579066527,3,ERROR,core_dump.c,"LatchedShutdownStatus - Latch: 0x%02x | Latch Dirty Shutdown Count: 0x%08x | Power State Events (raw): 0x%08x"
3578380128,0,INFO,platform_config_data.c,"Allocate Buffer Callback Made DDRT"
3577358859,0,WARNING,ait_dram.c,"AIT DRAM Correctable Read Error threshold reached"
3574636869,2,ERROR,debug.c,"*** ASSERT *** module: %x Line: %d"
3573922503,0,ERROR,hal_pmic_rail_cwv.c,"Rail D VID is not fused."
357247256,1,ERROR,log_power_event_end.c,"PowerEvent: 0x%x"
3571444054,3,STATUS,fw_init_profiler.c,"ROM init completed @ 0x%08X. FW init completed @ 0x%08X after %d us."
3570286416,0,ERROR,error_logging.c,"Error log initialization failed. Not returning error logs."
3568751667,5,STATUS,fw_activate_profiler.c,"FW Activate completed @ 0x%08X taking a total of %d us: Shutdown %d us, ROM %d us, init %d us."
3566632604,3,ERROR,ddrt_training.c,"ERROR: Clock Alignment Failed-  DA_DDRT_TRAINING_STS0.DONE_DCKADJ_TRN= 0x%X, DDRT_CKDET=0x%X, MSC_FNVIO_INIT_CONTROL_1.DDRTPLLLOCKED=0x%X"
3564792536,3,ERROR,core_dump.c,"SxpTimingTableVersion 1D: 0x%x | 2D: 0x%x | 4D: 0x%x"
3562894893,2,ERROR,core_wear_level_move.c,"FreeBlockExpansion_Transition Could not refresh all source lines of pda 0x%08X_%08X"
3562568096,3,ERROR,sxp_trim_bundle.c,"Could not populate AdwlVdm value %d to S2X_REG_ADDR_TMR_ADWLVDM_NEAR_FAR_DECK_%d (0x%04x)"
3562350041,2,ERROR,core_dump.c," Call[%d]: 0x%08x (guess based on code region)"
3562021033,0,INFO,refresh.c,"Suspending Refresh and Saving Pointers"
3558783716,0,ERROR,ltec.c,"PMIC rails are not at Boot VIDs at the time of LTEC failure. Going to Transaction fatal"
355753038,0,INFO,core_wear_level_move.c,"Block Move: Address is within spare block region"
3557221934,0,WARNING,command_inject_error.c,"Dma transfer not completed"
3555961706,2,ERROR,sxp_trim_bundle.c,"Could not determine HnlwlSelv RD%d from S2X_REG_ADDR_TMR_HNLWLSELV registerdata: 0x%04x"
3555022985,3,DEBUG,task_command_handler.c,"checking sequence: mb[%d] sequence[0x%x] command[0x%x]"
3553955558,1,ERROR,fw_upd_halt_at_img_auth.c,"FwUpdate has been halted at block: %d"
3553699647,0,DEBUG,buffers.c,"Queue not empty, someone is waiting for a buffer"
3552812575,1,DEBUG,core_dump.c,"Data: 0x%X"
3551649929,3,ERROR,update_firmware.c,"State machine attempted to transition to unknown state %d. Current state/substate is %d/%d"
3549201325,0,ERROR,commands.c,"Invalid FW State. Failed to preserve lifetime stats"
3548578742,1,ERROR,log_power_event_start.c,"P_PWM_STS: 0x%x"
3547776670,0,ERROR,power_loss_log.c,"Could not erase a PLI log due to polled DMA error"
3547546391,5,ERROR,core_dump.c," - Log Entry[%d] -> Checkpoint [%d] ErrorCode [%d] MiscData[0x%x] Timestamp [%d]"
3545738239,0,ERROR,security_md.c,"Wrap the AES part of PM-RK error"
3545002928,4,DEBUG,sxp_rx_dqs_training.c,"Advanced_RxDqs Rising_Mid_Falling%d: %d_%d_%d"
3544576542,1,INFO,read_disturb.c,"Read Disturb Random Interval too big, set to max.  Too big: 0x%X"
3543998170,0,ERROR,wear_level_move.c,"FBE AIT DMA Line Callback DMA Failure"
354312535,0,ERROR,adaptive_vdm.c,"AVDM_GetVdmDimmData requested VDM3 with S2X media."
3542575399,1,ERROR,nlog_notify_ddrt_normal_mode.c,"D_FW_STATUS_H: 0x%x"
3541046495,2,INFO,ras.c,"pw_ras_interrupt_req is 0x%08X, fault data mask is 0x%08X"
3540958188,8,ERROR,adma.c,"Cmd = 0x%X, sram = 0x%X, dpa = 0x%08X_%08X, pda = 0x%08X_%08X, size = 0x%08X, flags = 0x%08X"
3540093887,0,STATUS,fill_nlog_sram_buffer.c,"Filling up the NLOG SRAM buffer..."
353972255,0,DEBUG,command_features.c,"Get Admin Features: DIMM Partition Info"
3534702288,1,DEBUG,ddrt_scheduler.c,"DDRT Divider Ratio is: 0x%08x"
3530985493,1,ERROR,ait_dram.c,"AIT DRAM Uncorrectable read error detected at index 0x%x"
3530533140,2,ERROR,kernel.c,"Unclearable: %d | Event %x"
3530449322,1,ERROR,ait_nm3_csr.c,"Second uncorrectable in an AIT N-3 entry, going DIMM FATAL! Index: %d"
3530054905,3,ERROR,hal_pmic_rail.c,"Dynamic PMIC Rail 0x%x did not ramp to target value 0x%x. Current value is 0x%x."
3528828647,0,ERROR,hal_pmic_cap_test.c,"Cap self test getting voltage failed."
3526472054,0,ERROR,kechika_river_pmic_driver.c,"Cap self test start failed."
3525728683,4,ERROR,dma_polled.c,"Address Verify Error! DPA 0x%08X_%08X; PDA 0x%08X_%08X"
3525184819,5,ERROR,block_move_error_handler.c,"WLM CSR resp error opcode: 0x%X blockmovetype: 0x%X filterFsm: 0x%X AidUpdateFsm: 0x%X MasterFsm: 0x%X"
3519984277,1,ERROR,algo_sense_amp_calibration.c,"No transition found for Sense Amp Calibration DQ bit: %d"
3519673109,0,ERROR,ltec.c,"LTEC DDRT training mode update failed due to I2C bus error"
3519593312,1,ERROR,fw_image_sync.c,"Image Sync Abort called while Image Sync was in state: %d."
3518686965,0,DEBUG,platform_config_data.c,"Allocate Buffer Callback Made SMBus"
3517850029,0,WARNING,command_log.c,"DMA Transfer Failure"
3517153162,2,ERROR,power_budgeting_engine.c,"12V Power sample [%d mW] has exceeded high watermark threshold [%d mW]"
3516933014,2,ERROR,power_budgeting_engine.c,"1.2V Power sample [%d mW] has exceeded high watermark threshold [%d mW]"
3514258845,2,ERROR,kechika_river_pmic_driver.c,"Failed to apply IDT silicon workaround while updating rail %d to vid %d"
3513728743,0,ERROR,sxp_init.c,"Writing Training report to SPI failed"
3511683020,4,INFO,address_scrub.c,"Start ARS: Start Address: 0x%08X_%08X End Address: 0x%08X_%08X"
3509575640,2,ERROR,sxp_trim_bundle.c,"Could not determine TcSetCurrentStep%d from 0x%04x"
3509503738,1,DEBUG,checkpoint.c,"FW status: Update Media Ready - %d"
3508996958,1,WARNING,ras.c,"WdbUe on Banks[0x%x]"
3508795009,2,ERROR,sxp_trim_bundle.c,"Could not determine TcIrefGenStep%d from 0x%04x"
3508724962,2,ERROR,chn_no_cmd.c,"failed to poison DPA 0x%08X_%08X"
3506215587,0,DEBUG,cpgc.c,"Provide data pattern or set the zeroPattern flag to true"
3506199962,3,WARNING,task_error_handler.c,"Error found for domain %u nerr_%u bit %u, no handling other than clearing the bit"
3501186390,1,ERROR,write_count_histogram.c,"Invalid Transfer Type %d"
3498448765,0,WARNING,fw_img_auth.c,"Key Size field is invalid"
349765868,0,ERROR,power.c,"PMIC Rail A got svid fuse value 0x0"
3497207446,0,INFO,command_log.c,"Get Memory Info"
3495868004,2,ERROR,core_dump.c,"Call[%d]: 0x%X"
3495512558,0,WARNING,command_features.c,"Invalid Value for Vendor Specific Additional Settings"
3494995271,0,DEBUG,task_error_handler.c,"Changing settings for Package Sparing"
3491991870,1,ERROR,task_media_interface.c,"AitRead. Invalid level provided. 0x%X."
3491611251,3,WARNING,wear_level_move.c,"BB pointer not in valid range. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
3491448344,1,ERROR,log_emask_imask_regs.c,"A_EMASK_2: 0x%x"
3491163864,12,INFO,sxp_scheduler.c,"SXP Addr Offset R[%d]:%x,%x,%x,%x,%x,%x,%x,%x,%x,%x,%x"
3490801899,0,WARNING,command_features.c,"GetSecurityInfo: Invalid SubOpcode"
3489172607,1,DEBUG,ras.c,"clearing 0x%08X in pw_ras_interrupt_req"
3489109234,0,WARNING,dfx.c,"Module ID specified in input payload ""does not match module ID that was uploaded"
3488693905,0,ERROR,fw_activate.c,"Current Dynamic VDM window saved during FW activate is greater than max VDM window."
3488077349,0,ERROR,format_device.c,"Cmd Format Device, creating fw state failed."
3485741546,1,ERROR,nlog_region_lock.c,"D_PM_SIZE_L: 0x%08x"
3485379412,0,ERROR,core_dump.c,"PowerLossLog Checkpoints:"
3484715167,1,WARNING,core.c,"Unknown subId for Core General Message Handler [%d]"
3484272056,1,STATUS,dynamic_vdm.c,"DynamicVdm_AdjustVdm at Window. Window : %d"
3482434137,0,ERROR,task_command_handler.c,"Format was completed. Power cycle is required after a device format."
3482372100,0,ERROR,format_device.c,"Cmd Format Device, building AIT failed."
3481776267,0,ERROR,error_logging.c,"Could not add an error entry to media error log because it is not Initialized yet"
3481538604,1,DEBUG,host_interrupt.c,"HostInterrupt PowerStateNotify Event[%d]"
3479660945,0,WARNING,task_security.c,"Unable to Freeze Lock: Encryption Disabled"
3478984100,0,ERROR,spi.c,"Program of data chunks failed"
347896670,1,ERROR,data_path_error.c,"Data path Error: %d"
347801122,0,ERROR,task_media_interface.c,"got DMA completion while engine was hung!"
3474941726,1,ERROR,adaptive_vdm.c,"AVDM_GetVdmDimmData requested for Invalid VDM : %d"
3473629459,2,ERROR,kechika_river_pmic_driver.c,"Failed to apply IDT silicon workaround while updating rail %d to vid %d"
3473496729,0,DEBUG,command_features.c,"Get Features: Address Range Scrub"
3473432757,0,INFO,command_errorlog.c,"Retrieving Error Logs"
3468609230,0,WARNING,buffers.c,"Not a valid buffer range"
3467864389,1,ERROR,nlog_config_lockdown.c,"D_FW_STATUS: 0x%x"
3467742944,1,ERROR,nlog_notify_ddrt_normal_mode.c,"IO_INIT_CTRL: 0x%x"
3467537274,1,WARNING,health_manager.c,"Complete Package Sparing has occurred. Failing Die: %d."
346700515,0,ERROR,fw_activate.c,"FW activate failed to suspend LTEC."
346494225,1,ERROR,command_features.c,"NOT Going to Normal Mode - Host Side Training Incomplete: hostTrainingStatus=%d"
3461790387,0,ERROR,media_manager_engine.c,"MediaManagerEngine_PollStartBit has failed. Start Bit has failed to de-assert!"
346115036,4,ERROR,algo_tx_dq_dqs_training.c,"Adv_TxDqDqs failed margin check R[%d] B[%d]: R[%d] F[%d]"
3458728905,3,ERROR,ddrt_training.c,"ERROR: Clock Alignment Failed-  DA_DDRT_TRAINING_STS0.DONE_DCKADJ_TRN= 0x%X, DDRT_CKDET=0x%X, MSC_FNVIO_INIT_CONTROL_1.DDRTPLLLOCKED=0x%X"
3458643806,0,DEBUG,core_wear_level_move.c,"AIT Update Callback"
3457675908,2,ERROR,command_features.c,"Performance Knob %d is updated with value %d"
3456705503,1,ERROR,core_dump.c,"Package Sparing Policy - Enable: 0x%02x"
3454501252,0,ERROR,commands.c,"Cmd Format Device, building AIT failed."
3452465453,1,ERROR,core_dump.c,"RefreshState - Fast First Refresh Enable: 0x%02x"
3452149772,0,INFO,power_state.c,"Warm Reset Start"
3448978154,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz2: 0x%x"
3448970214,0,WARNING,command_features.c,"Only PM enabled SKU"
3445486020,0,INFO,ait_update.c,"Updating Main Line State"
3444651188,1,ERROR,log_msc_spare_ctrl.c,"MSC_SPARE_CTRL: 0x%x"
3444434809,0,WARNING,command_features.c,"Invalid DDRT payload"
3444185450,0,ERROR,feature_state_data.c,"Hashing 0's failed"
3443891549,0,ERROR,ddrt_training.c,"Ddrt_XoverCalibration failed"
3443623458,1,ERROR,kechika_river_pmic_driver.c,"Vcap failed to ramp for self test after %dms"
3443420675,0,INFO,address_scrub.c,"Initialize Address Range Scrub"
3442600462,2,ERROR,format_device.c,"Cmd Format Device, DMA returns a failure status. ""sxp address:  0x%08X_%08X"
3442436457,1,ERROR,platform_config_data.c,"Invalid Small Payload Part during get operation. pcd_spPart = 0x%08X"
3441229966,0,INFO,smart.c,"Retrieving SMART data"
3438224124,0,WARNING,fw_img_auth.c,"Tried to do a customer debug FW update with a perPartID that did not match this DIMM"
3437001295,0,ERROR,key_management.c,"Failed to unwrap PM-RK with security disabled wrapping key"
3436635842,0,ERROR,sxp_init.c,"Sxp_XoverCalibration failed"
3436621052,8,ERROR,fw_init.c,"Current FW version - %x.%x.%x.%04x, DIMM Unique ID - 0x%02x%08x%08x, Power Cycle count - %d"
3435542425,2,DEBUG,dpa_for_pda.c,"0x%08X: skipping line %d"
3432962642,0,ERROR,fconfig.c,"FconfigSpiLayout->header.dwordLen beyond size of SRAM structure."
3430872182,0,WARNING,command_fw_update.c,"Invalid SVN Downgrade Opt-in input Payload value"
3429738261,0,ERROR,kechika_river_pmic_driver.c,"Failed to disable power on reset"
3427538084,2,ERROR,core_dump.c,"HW CSR Address: 0x%x Value: 0x%x"
3425935741,1,ERROR,power_state.c,"Surprise Reset: Unexpected Power State event [0x%x] detected."
3423929964,1,ERROR,log_emask_imask_regs.c,"PW_EMASK_0: 0x%x"
3423334270,0,ERROR,ddrt_training.c,"Ddrt_SenseAmpCalibration failed"
3422184131,0,ERROR,ltec.c,"LTEC requested to transition from idle mode to normal mode outside of S3 resume path."
342043210,4,WARNING,command_features.c,"Invalid set power management params. Values are not within minimum and maximum limits"" AveragePowerLimit = %d; mBBAveragePowerTimeConstant = %d; mBBEnable = %d; mBBMaxPowerLimit = %d"
34197468,0,INFO,sxp_scheduler.c,"Sxp_GetDieInventory()!\n"
3419605228,0,ERROR,hal_pmic_cap_test.c,"Erroneous Cap test tick value"
3415103555,4,DEBUG,sxp_wr_dqs_training.c,"Advanced_TxDq Rising_Mid_Falling%d: %d_%d_%d"
3414511382,0,ERROR,format_device.c,"HW WLM engine did not Pause."
3414427753,1,ERROR,task_high_priority_message_handler.c,"Message handler is null. HPMH Message Id: 0x%X."
3414202904,1,ERROR,core_wear_level_move.c,"Default case in FBE state machine hit! STATE = %d"
3414142167,0,DEBUG,command_features.c,"Set Features: Address Range Scrub"
3412993871,3,ERROR,hal_ait.c,"Size %d is not a multiple of %d bytes (AIT LEVEL %d)"
3411656498,0,DEBUG,command_features.c,"PCD Get Data SMBus"
3411082501,0,INFO,key_management.c,"Build new KEK"
3409972603,1,ERROR,hal_pmic_rail_cwv.c,"Failed reading PMIC power good register with PMIC return code 0x%X"
3409873987,1,WARNING,error_logging.c,"Failed to load Error Log %d"
3408415764,2,ERROR,fw_image_sync.c,"Image Sync failed with error SPI Write at 0x%x in state: %d."
3407326482,1,INFO,power_budgeting_engine.c,"Energy meter was paused for %d msec."
3406607009,2,ERROR,kernel.c,"Unclearable: %d | Event %x"
3404201856,0,ERROR,pll_gating_failure_trigger.c,"PLL gating was desynchronized."
3403469630,2,ERROR,core_wear_level_move.c,"WearLevelMove_Transition Could not refresh all source lines of pda 0x%08X_%08X"
3403382840,0,DEBUG,task_error_handler.c,"Changing settings for Package Sparing"
3401619930,0,ERROR,ddrt_scheduler.c,"Ddrt Mrc Programming Error: No Table Found"
3400551524,0,ERROR,dynamic_vdm.c,"Dynamic VDM cannot apply media policy to this DIMM!"
3397914703,0,DEBUG,key_management.c,"Unwrapping S3 Saved Volatile Memory Keys"
3396267756,6,ERROR,barlow_creek_pmic_init_reason.c,"Fault Code 0 = 0x%x, Fault Code 1 = 0x%x, Fault Code 2 = 0x%x, Fault Code 3 = 0x%x, Fault Code 4 = 0x%x, Fault Code 5 = 0x%x"
3395046878,1,ERROR,sxp_commands.c,"Unexpected FGPK SXP Reg Read Offset value of 0x%X."
3393805622,1,ERROR,log_power_event_end.c,"CHN_WCTL: 0x%x"
3390751672,0,STATUS,log_ddrt_training_start.c,"DDRT training started."
3389532038,1,ERROR,log_power_event_end.c,"D_FUNC_DEFEATURE1: 0x%x"
3389041242,0,INFO,power_state.c,"PC6 Enter: Clock Stopped"
338775283,1,ERROR,log_power_event_start.c,"D_PWM_MASK: 0x%x"
3387683729,0,INFO,ait_update.c,"Updating Complete State"
338717244,3,INFO,task_error_handler.c,"domain %u nerr_%u bit %u was set"
3384007594,0,DEBUG,power_state.c,"PC6 Enter: Power down."
3381163033,0,ERROR,command_fw_update.c,"FW Update locked for an unknown reason"
3381001846,0,DEBUG,fw_image_sync.c,"Timer Callback"
33782020,2,ERROR,sxp_trims.c,"Unrecognized media on Rank: %d, Die: %d"
3377135673,0,ERROR,sxp_init.c,"Writing Training RMT Report to SPI failed"
337676954,2,ERROR,thermal_engine.c,"ThermalEngine_LoadSxpTemperatureCalibrationValues failed to Read SxpRegister Rank: %d FailMap: 0x%04x"
3374461225,2,ERROR,sxp_trims.c,"Unrecognized S15 media on Rank: %d, Die: %d"
3371874122,1,ERROR,command_software_triggers.c,"Wrong event notification: %d"
3368509055,4,STATUS,update_firmware.c,"FW Update has successfully staged FW %02x.%02x.%02x.%04x."
3364363768,0,INFO,security_interface.c,"Security_CompleteRequestWithEvent completed...Event generated"
3355855053,2,ERROR,message_channel.c,"Window Access READ Fail  Address = 0x%X, ReadData = 0x%X"
3355504405,2,STATUS,kechika_river_pmic_driver.c,"PMIC Manufacture ID: 0x%X    Product Stepping: 0x%X"
3353871339,0,ERROR,update_firmware.c,"Could not retrieve SPI Image Address"
3353162954,0,ERROR,write_count_histogram.c,"Write Count Status: WLM pending counter overflowed"
335285287,1,ERROR,ait_nm3_csr.c,"AIT N-3 entry has double bit uncorrectable error. Index: %d"
335259044,1,ERROR,ltec.c,"PMIC driver failed to apply LTEC update after %d attempts."
3352464449,4,STATUS,fw_activate.c,"FW Activate Timing [us]: shutdown %d, ROM %d, init %d, total %d"
3352225618,1,DEBUG,task_error_handler.c,"AIT Scrub State Machine : %d"
3349598407,4,ERROR,core_dump.c,"FwS Datastore Id | Header Version | Entries Size : 0x%x | 0x%x | 0x%x [%d]"
3349344742,0,INFO,security_interface.c,"SecurityInterface_Initialize completed."
3348769973,1,ERROR,log_emask_imask_regs.c,"CHN_IMASK_0: 0x%x"
3344797308,0,WARNING,dfx.c,"Mismatching module COMMIT ID with firmware COMMIT ID"
3344439111,0,STATUS,command_fw_update.c,"Cannot update FW because image sync has not completed"
3343989517,0,DEBUG,pmic.c,"PMIC Read Error"
3343632524,0,ERROR,key_management.c,"Forward expansion of PM-RK failed"
3342554354,4,ERROR,dynamic_vdm.c,"Dynamic VDM SxpCmd_SendCommandWriteRegister failed on rank : %d, die : %d, address : 0x%08X, value : 0x%08X"
3341873094,2,ERROR,message_channel.c,"Message channel error! ctrl = 0x%08X, status = 0x%08X"
3340944979,2,ERROR,sxp_init.c,"Write DQ-DQS Training failed, Rank: %d Training type: %d"
3339584837,1,ERROR,wear_level_move.c,"FBE Block Move aborted entered without BM abort status:%x"
3339571421,0,INFO,power_state.c,"Warm Reset Exit Clock Enable"
3338123745,0,DEBUG,fw_image_sync.c,"Image Sync Allocate Callback"
3333509975,1,ERROR,ras.c,"RAS Log: Valid bit not set - PC_LOG_RPDA_P0_PE = 0x%x"
3333191073,1,STATUS,command_features.c,"Going to Normal Mode -> Current BSR: 0x%08x"
3332950078,1,ERROR,data_path_error.c,"DN FIFO U/O Flow Errors: 0x%08X"
3332572499,1,ERROR,ltec.c,"LTEC DDRT training VID update did not complete within timeout of %d microseconds."
3332119802,0,INFO,fw_image_sync.c,"Image sync completed. Start Cap test "
3331440782,2,ERROR,aclk_periodic.c,"ACLK Calibration : SxpCmd_SelectId failed on rank : %d, die : %d"
3330111516,1,DEBUG,spare_block.c,"Calculating remaining spare block percent: %d%%"
3328968948,0,ERROR,sxp_rmt_tests.c,"RAS Tx Dq Min Mask Test Failed"
3327806577,4,ERROR,dma_polled.c,"Uncorrectable error! DPA 0x%08X_%08X; PDA 0x%08X_%08X"
3327720057,1,ERROR,high_priority_message_handlers.c,"Surprise clockstop received and current PowerStateEvents is 0x%x"
3326763939,1,ERROR,power_wake_isr.c,"Surprise clockstop received and current PowerStateEvents is 0x%x"
3325444490,18,ERROR,kechika_river_pmic_driver.c,"Requested Update Values: A[%d][%d][%x] B[%d][%x] C[%d][%x] D[%d][%d][%x] E[%d][%x] F[%d][%x] G[%d][%x] H[%d][%x]"
3325144483,1,ERROR,power_budgeting_engine.c,"Energy meter is in unknown state(%d)."
3323932083,1,ERROR,power_budgeting_engine.c,"Firmware samples energy meter slower than every %dus."
3318448609,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz2: 0x%x"
3318255629,1,ERROR,log_emask_imask_regs.c,"A_IMASK: 0x%x"
3317797329,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrioCmdEn: 0x%x"
3317344679,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz2: 0x%x"
3314862889,2,ERROR,dpa_verify_error_handler.c,"DRAM read at DPA LvL N address Lo: %x Hi: %x  failed"
3313085391,0,ERROR,dfx.c,"DMA did NOT complete!"
3312841587,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustToWindow does not have a window type for vdmWindow %d"
3310462343,0,ERROR,ait_dram.c,"Abort DRAM Load"
3308912536,3,ERROR,sxp_scheduler.c,"read SXP_REG_IDREG failed! value = 0x%x, die = %d, rank = %d \n"
3308825734,2,ERROR,sxp_trim_bundle.c,"Could not determine TcHnmirrorSelect%d from 0x%04x"
3307570553,1,ERROR,sxp_init.c,"Sxp_WrDqsTraining failed rank: %d"
3305136635,2,WARNING,data_path_error.c,"data path error PDA 0x%08X_%08X"
33049783,0,ERROR,sxp_training.c,"SPI read failure during crc pull!"
3304696785,0,ERROR,memory_info.c,"Unknown stat total requested"
3303068881,0,ERROR,command_features.c,"Bad CEL entry - can't determine restrictions"
3301996193,1,ERROR,write_disturb_engine.c,"Write Disturb Threshold in PW_WCCTRL had an unexpected value: %d. Re-initializing WD threshold"
3301064181,2,ERROR,ddrt_sense_amp_calibration.c,"lines that can be trained: %d, failed lines in fub: %d"
3300440658,0,ERROR,task_media_interface.c,"Media Interface Dma Timed Out"
3296246557,2,ERROR,core_dump.c,"LP InputPayload Addr : 0x%08x_%08x"
3296221385,2,DEBUG,wear_level_move.c,"Invalid Block: 0x%08X_0x%08X"
3295382658,0,WARNING,dfx.c,"Uploaded header was invalid"
3295233107,0,ERROR,ait_dram_scheduler.c,"Ait Dram Scheduler Init failed"
3292224809,0,WARNING,command_features.c,"Unable to update the SKU"
3292117139,0,ERROR,sxp_training.c,"Sxp timing table authentication failed!"
3291024762,2,ERROR,barlow_creek_pmic_init_reason.c,"Retrieved invalid code from Fault Code %d: 0x%x."
3290668360,1,ERROR,spi_debug_structures.c,"Found In SPI Debug Region: Unknown debugId %d"
3290024352,1,ERROR,data_path_error.c,"A FIFO U/O Flow Error 0: 0x%08X"
3289769807,0,INFO,error_logging.c,"Initializing Logging"
3288878426,0,ERROR,feature_state_data.c,"Feature State Data Initialization Failed"
3288347909,0,INFO,core_dump.c,"Using checksum instead of SHA - coreDumpPart 1"
3287429008,0,DEBUG,command_features.c,"Get Features: Alarm Threshold"
3286435201,2,DEBUG,error_logging.c,"Error Log size is 0x%08X and available size is 0x%08X"
3283472636,0,INFO,address_scrub.c,"Address Range Scrub Complete"
3281447126,0,ERROR,task_error_handler.c,"Both AIT UECC, don't complete the transaction!"
3278639911,0,ERROR,command_features.c,"S3 Restore has not completed, and PLL's haven't locked"
3277971792,1,ERROR,host_interrupt.c,"HostInterrupt Abort in flight Host Interrupt of type = %d"
3275759284,2,DEBUG,algo_tx_dq_dqs_training.c,"tx dqs delay for byte %d is %d"
3275489977,3,ERROR,algo_xover_calibration.c,"Xover calibration failed due to invalid strobe duty cycle. CmdFub[%d] Rising Edge[%d] Falling Edge[%d]"
3272748845,2,ERROR,sxp_init.c,"Coarse Write Leveling Training failed, Rank: %d Training type: %d"
327166611,0,ERROR,fw_state.c,"DMA failure when loading FW State"
3270891840,1,ERROR,log_zqcal_short.c,"APB_TIMER2: 0x%08X"
3270093292,1,INFO,command_log.c,"Number of entries set to %d"
3269648857,1,ERROR,overwrite_dimm.c,"Spi Erase failed on address 0x%X"
3269290440,0,INFO,ait_update.c,"Updating Backup Line State"
326839236,0,ERROR,dma_polled.c,"Started polled DMA when a DMA hadn't completed, not in PLI. Shouldn't be possible."
3268174494,3,ERROR,core_dump.c,"InputPayload QWORD[%d]: 0x%08x_%08x"
3267898631,0,DEBUG,command_features.c,"SS: Overwrite DIMM"
3267681649,0,ERROR,key_management.c,"Failed to unwrap PM-RK using security disabled wrapping key"
3265658051,1,ERROR,core_dump.c,"***** CoreDump Start: %x *****"
3265629355,3,ERROR,ras.c,"RAS PC_WPDA Log: Valid bit not set! base = 0x%x, lo = 0x%x, hi = 0x%x"
3265423756,0,WARNING,task_security.c,"WARNING: Request not recognized in task_security"
3263244103,0,ERROR,dfx.c,"Krnl Event Timer Expired"
3263043170,0,ERROR,sxp_device_access.c,"S26 Devices detected. Forcing 11 Device mode due to current issue"
3262204460,0,ERROR,commands.c,"Cmd Format Device, creating fw state failed."
3261981221,0,ERROR,log_power_event_end.c,"LogPowerEventEnd"
3260957058,4,ERROR,core_dump.c,"FwS Datastore Id | Header Version | Entries Size : 0x%x | 0x%x | 0x%x [%d]"
3259413242,1,ERROR,sxp_init.c,"Coarse Write Leveling Training failed, Rank: %d"
3259211955,0,ERROR,vdm.c,"Vdm_AdjustVdm called with unsupported VDM!"
3256831966,1,ERROR,update_firmware.c,"Supplied image is signed with wrong key. Debug signed images work only on PRE_PRQ part and release signed images work only on PRQ part. This part type: 0x%x"
3255570045,1,ERROR,log_emask_imask_regs.c,"DS_EMASK: 0x%x"
3254385282,7,ERROR,spi_debug_structures.c,"Found In SPI Debug Region: DMA Timeout -> Cmd: 0x%08X, Status: 0x%08X, DPA: 0x%08X_0x%08X, PDA: 0x%08X_0x%08X, PWM Status: 0x%08X"
3251794179,0,INFO,key_management.c,"Build new KEK"
3251698145,2,WARNING,refresh.c,"shutdown time 0x%08X_%08X is not less than the boot time"
3251696861,1,ERROR,nlog_region_lock.c,"D_TWO_LM_SIZE_H: 0x%08x"
3251645981,3,ERROR,sxp_trim_bundle.c,"irefSenseEnb SxpReg_PopulateIRefSenseEnbRead/Write returned %d on rank = %d die = %d. Iref Sense Enb Trim not set."
324681682,0,ERROR,security_md.c,"Security Metadata Initialization Failed"
3246567352,1,ERROR,get_spi_manifest.c,"Spi read failed when reading pIMF Header at address 0x%08x"
3245484018,7,STATUS,update_firmware.c,"FW Update has successfully staged FW %02x.%02x.%02x.%04x, activation version: 0x%02x,""API version: 0x%04x. Current handshake API version: 0x%04x"
3243506106,0,INFO,address_scrub.c,"Starting Address Range Scrub"
3240601552,3,ERROR,core_dump.c,"FwState Data: Top[0x%x] | Bot[0x%x] | Valid[%d]"
3237821726,0,ERROR,update_firmware.c,"Cannot reset SHA engine"
323703001,2,ERROR,thermal_manager.c,"ThermalComp Thermal Shutdown Comp[%d] Temp[%d]"
3236893640,1,ERROR,update_firmware.c,"Handler could not handle this event. Event type: %d"
3234920806,0,ERROR,power_budgeting_engine.c,"Setting average power budget to default value as FW is unable to process EM data in a timely manner for two consecutive accumulation windows"
3234210394,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtLatency: 0x%x"
3233014679,5,INFO,task_error_handler.c,"0x%08X: channel command: 0x%08X, 0x%08X, 0x%08X, 0x%08X"
3232618447,1,ERROR,sxp_init.c,"This board 0x%08x does not support 10 Die Mode without rework"
323160299,1,ERROR,nlog_notify_ddrt_normal_mode.c,"D_FW_STATUS_H: 0x%x"
3226763315,4,DEBUG,ahb_unified_engine.c,"Doing PDA Write. PDA: 0x%x_%x DPA: 0x%x_%x"
322536835,8,STATUS,fw_init.c,"Current FW version - %02x.%02x.%02x.%04x, DIMM Unique ID - 0x%02x%08x%08x, Power Cycle count - %d"
3224545735,1,ERROR,ait_nm3_csr.c,"Second uncorrectable in an AIT N-3 entry, going DIMM FATAL! Index: %d"
3223712991,3,ERROR,task_error_handler.c,"Unexpected FERR: domain %d, ferrNum %d, ferrBit %d"
3223349990,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustS26IRst called with invalid vdmWindow : %d"
3221672788,0,ERROR,barlow_creek_pmic_init_reason.c,"Unknown PMIC Init reason - Unknown PMIC vendor."
3221531703,0,WARNING,task_command_handler.c,"DDRT Training In Progress - Command Not Valid"
3221397378,1,ERROR,read_write_pmic.c,"Before sending I2C request EM_STATUS: 0x%08x"
3220844409,1,ERROR,partition_manager.c,"Unexpected mailbox %d may not remain locked throughout operation."
3219575617,0,DEBUG,dfx.c,"Upload via small payload complete"
3217844399,5,ERROR,sxp_training.c,"Register 0x%08X at offset 0x%08X with maskValue 0x%08X wrote 0x%08X read 0x%08X"
3216920955,1,ERROR,sxp_training.c,"PMIC cumulative reboot count [%d]"
3215518423,0,ERROR,sxp_init.c,"Sxp_RestoreSxpIoRegisters failed"
3210596807,5,ERROR,core_dump.c," - Log Entry[%d] -> Checkpoint [%d] ErrorCode [%d] MiscData[0x%x] Timestamp [%d]"
3210432691,1,ERROR,ait_dram.c,"Abort DRAM Load at Index %x"
3210047405,1,ERROR,update_firmware.c,"Invalid state %d"
3207823068,2,ERROR,pmic.c,"PMIC Set Bits Failure: Address 0x%X, Error Code %d"
3206377002,1,ERROR,get_ait_info.c,"A_AIT_TOP_BASE_ADDR_L: 0x%x"
3204485791,2,ERROR,dynamic_vdm.c,"Dynamic_IRST Trim Error rank : %d, die : %d"
3204085982,0,WARNING,overwrite_dimm.c,"Overwrite DIMM Error Found"
3203500595,1,ERROR,get_media_statistics.c,"GetMediaStatistics_GetAvdmData requested for Invalid VDM : %d"
320230413,0,ERROR,kechika_river_pmic_driver.c,"CAP test error - communication problem - rescheduling test"
3201935043,0,ERROR,spi_debug.c,"Debug region not initialized, skipping SaveData call"
3201846644,1,ERROR,short_stroke.c,"Short Stroke Mode %d is invalid"
3200927688,1,ERROR,fw_upd_halt_at_spi_write.c,"FwUpdate will halt at block: %d"
3197296858,0,WARNING,task_media_interface.c,"DMA abort failed!"
3196636779,1,DEBUG,platform_config_data.c,"PCD Part: 0x%08X"
3196485623,4,ERROR,dynamic_vdm.c,"Max window adjustment %d for Near AdwlVdm rank %d die %d deck %d is invalid"
319623009,0,DEBUG,power_state.c,"PC6 Enter: Clock Stopped"
3193690401,0,ERROR,pcsclr_engine.c,"RDWR_BUF_CTRL LINE_AVAIL did not return to idle"
3192954076,0,ERROR,enqueue_media_request.c,"Media request is being enqueued."
3192884137,1,ERROR,core_wear_level_move.c,"WearLevelMove_Dispatch unexpected AIT read msg:%x"
3192726540,1,ERROR,log_power_event_end.c,"IO_INIT_CTRL: 0x%x"
3191964061,1,ERROR,buffers.c,"Invalid Buffer released. Buffer address = 0x%08X. Going transaction fatal."
3190626798,1,ERROR,pli_host_throttling_check.c,"DRDP_WCRD_TIMER: 0x%x"
3189850496,0,WARNING,platform_config_data.c,"DMA transfer failed to complete"
3189060317,4,ERROR,task_media_interface.c,"MI 0x%X request made when no free requests were available. Free(%d) WIP(%d) Pending(%d)."
3188087785,1,ERROR,nlog_notify_ddrt_normal_mode.c,"DA_IO_PCR_PERMISSIONS0: 0x%x"
3187745752,2,ERROR,pmic.c,"PMIC Clear Bits Failure: Address 0x%X, Error Code %d"
3187471728,1,STATUS,fw_init.c,"Recovery FW used %d times"
3186493778,0,ERROR,task_media_interface.c,"Media Interface Dma Timed Out"
3183936557,1,ERROR,buffers.c,"Invalid Buffer. Buffer address = 0x%08X. Going transaction fatal."
318392443,2,ERROR,algo_rx_dqs_training.c,"Basic Sxp_RxDqDqs failed rank[%d] byte[%d]\n"
3181403268,1,ERROR,log_power_event_end.c,"D_RST_STS: 0x%x"
3180189062,3,ERROR,algo_write_leveling.c,"DRAM Internal Fine WrLvl failed. Rank[%d] BytePassMask[%x] BytePassFlag[%x]"
3178657213,0,DEBUG,overwrite_dimm.c,"Overwrite DIMM DMA Callback"
3177804576,0,ERROR,enqueue_media_request.c,"Media request is not allowed."
3177784934,1,ERROR,feature_state_data.c,"Wrong power event notification: %d"
3176987081,1,ERROR,core.c,"MessageId is out of range. MessageId: 0x%X."
3176111958,3,INFO,task_error_handler.c,"domain %u nerr_%u bit %u was set"
3175047601,0,DEBUG,overwrite_dimm.c,"Overwrite DIMM ait read Callback"
3174726844,1,ERROR,log_emask_imask_regs.c,"MCU_EMASK: 0x%x"
3173594552,1,INFO,hal_pmic_cap_test.c,"PLI Cap value is good. Self Test time: %d"
3173403564,0,ERROR,i2c_bus_manager.c,"I2C bus is in error state. Executing error handlers of queued requests."
3172428101,2,ERROR,sxp_trims.c,"Unrecognized S26 media on Rank: %d, Die: %d"
3172357393,0,DEBUG,warm_reset.c,"Warm Reset Flow PM Idle"
3172080582,0,ERROR,season_device.c,"Season failed. Media not ready."
3171591720,1,ERROR,get_ait_info.c,"A_LVLN_BASE_DPA: 0x%x"
3169751369,1,ERROR,nlog_region_lock.c,"D_PM_SIZE_H: 0x%08x"
3168981147,1,DEBUG,task_error_handler.c,"0x%08X: logging UECC fault"
3168823037,0,ERROR,ahb_unified_engine.c,"DMA Abort!"
3167743654,2,ERROR,algo_rx_dqs_training.c,"Advanced_Sxp_RxDqDqs failed margin check rank[%d] byte[%d]"
3167670809,0,WARNING,task_security.c,"Unable to set passphrase: Encryption Disabled"
3167456426,0,ERROR,fw_image_sync.c,"Image Sync got 2 separate buffer callbacks. Releasing the new buffer."
3164334080,0,DEBUG,command_features.c,"Set Admin Features: Platform Config Data"
3163486943,0,DEBUG,command_features.c,"Set Admin Features: FW Load Flag"
3161152171,0,WARNING,update_firmware.c,"Supplied image header fields are invalid"
3160514644,1,ERROR,sxp_init.c,"CPGC Test Failed on rankIndex %d"
3160142017,3,ERROR,core_dump.c,"SxpTimingTableVersion 1D: 0x%x | 2D: 0x%x | 4D: 0x%x"
3159386461,2,ERROR,core_dump.c,"OtherStateInfo - FwOccurence         : 0x%08x_%08x"
3158670468,1,ERROR,power_budgeting_engine.c,"Energy meter is in unknown state(%d)."
3157171442,5,ERROR,ddrt_scheduler.c,"ERROR: DDRT PLL did not lock before timeout DDRT_PLL_REF_CTRL=0x%X, DDRT_RESET_STATUS=0x%X, D_DDRT_DCLK_CTRL=0x%X, MSC_FNVIO_VISIBILITY_CSR=0x%X, IO_INIT_CTRL=0x%X"
3157028235,3,ERROR,task_error_handler.c,"Unexpected FERR: domain %d, ferrNum %d, ferrBit %d"
315670427,0,WARNING,fw_img_auth.c,"Image type is invalid"
3155732841,0,INFO,commands.c,"Obtaining DIMM information"
3155724086,0,ERROR,ait_dram.c,"DRAM load NOT started due to unsuccessful dram training!"
3155706516,2,ERROR,thermal_engine.c,"ThermalEngine_LoadSxpTemperatureCalibrationValues failed to Read SxpRegister Rank: %d FailMap: 0x%04x"
3153258834,0,DEBUG,overwrite_dimm.c,"Overwrite DIMM ait read Callback"
3152292903,1,ERROR,nlog_chn_fwrwcmd.c,"CHN_FWRWCMD3: 0x%x"
315187059,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustS15IRst at Window. Window : %d"
315037769,0,DEBUG,crypto_selftests.c,"Size of data for the 3DXP XTS-AES-256 Encryption Test exceeds size of buffer."
3149724422,2,ERROR,chn_no_cmd.c,"Chn no cmd with WLM for DPA 0x%08x_%08x deallocating WDB entry"
3149574244,3,WARNING,wear_level_move.c,"FBL tail pointer and FBL Head point to each other. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
3148896260,1,ERROR,wear_level_move.c,"WearLevelMove_Dispatch unexpected relocate block msg:%x"
3146369167,5,ERROR,die_error_emulator.c,"DieErrorEmulator: Invalid relative VDM level (VDM%d) for VDM%d. Valid levels are %d, %d and %d"
3145615361,0,ERROR,mm_block_move.c,"Failed to Pause the HW WLM engine within the expected timeout."
3144497372,3,WARNING,wear_level_move.c,"FBL tail pointer and FBL Head point to each other. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
3144450299,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaWrScrLfsrH: 0x%x"
3144063050,2,ERROR,chn_no_cmd.c,"failed to poison DPA 0x%08X_%08X"
3142635597,0,ERROR,thermal_manager.c,"AIT DRAM Thermal Shutdown"
3141847282,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr3: 0x%x"
3138317230,0,ERROR,thermal_manager.c,"AIT DRAM Thermal Shutdown"
3137693474,0,ERROR,dma_polled.c,"DMA retry failed with SRAM parity error again!"
3137310392,1,ERROR,ltec.c,"LTEC DDRT training VID update did not complete within timeout of %d microseconds."
3137230799,0,ERROR,log_ddrt_training_start.c,"DDRT training started."
3136657763,0,STATUS,hal_pmic_cap_test.c,"CAP Test result already Critical, not initiating any more testing\n"
3135249595,2,ERROR,short_stroke.c,"Short Stroke offset %d is invalid. It must be a multiple of Short Stroke Size %d when HW Short Stroke is enabled"
3135096478,0,STATUS,ait_dram.c,"Abandon DRAM Load"
3134591578,1,ERROR,spi.c,"Erase failed on sector 0x%08X"
3132953659,0,ERROR,ddrt_restore.c,"S3 Resume failed to restore"
3123831774,0,WARNING,command_features.c,"Not a Package Sparing capable SKU"
3123492289,0,ERROR,feature_state_data.c,"FSD loaded but init was not saved in FWS"
3120461275,2,ERROR,get_spi_manifest.c,"Spi read failed when reading SXP timing table %d version at offset x%08x"
3119531520,0,ERROR,dimm_fatal.c,"DIMM fatal error!"
3118821344,1,ERROR,security_md.c,"Security md version doesn't match on copy %d"
3115984310,0,ERROR,read_write_pmic.c,"ReadPmic Failure"
3115496030,0,ERROR,fw_state.c,"DMA failure when loading FW State"
3115149729,0,DEBUG,key_management.c,"Unwrapping S3 Saved Persistent Memory Keys"
3114245555,2,ERROR,sxp_rx_dqs_training.c,"Advanced_Sxp_RxDqDqs failed rank[%d] byte[%d]"
3112782569,0,ERROR,command_software_triggers.c,"Unsafe shutdown software trigger is injected"
3112683242,3,ERROR,dynamic_vdm.c,"Populate Far AdwlVdm rank %d die %d deck %d is invalid"
311151052,0,ERROR,dma_polled.c,"RACQ Parity error in dma polled"
3109024734,1,ERROR,log_emask_imask_regs.c,"PRUNIT_INTERRUPT_IMASK: 0x%x"
3108603628,0,DEBUG,command_inject_error.c,"Inject poison PM region needs to be unlocked"
3107422056,4,ERROR,sxp_scheduler.c,"SXP Mixed Stepping ID detected [%d] != [%d] at rank=%d die=%d"
310686339,0,ERROR,spi_debug.c,"Failed to log Spi Debug region due to SPI Read failure"
3106842745,3,ERROR,ddrt_training.c,"ERROR: Clock Alignment Failed-  DA_DDRT_TRAINING_STS0.DONE_DCKADJ_TRN= 0x%X, DDRT_CKDET=0x%X, DDRT_RESET_STATUS.PLLLOCKED=0x%X"
31059609,2,DEBUG,nlog.c,"rd 0x%08X = 0x%08X"
3105461629,4,ERROR,task_error_handler.c,"AIT Scrub failed 0x%08X_%08X; PDA 0x%08X_%08X"
3104326453,0,ERROR,format_device.c,"Invalid Feature State Data. Failed to preserve lifetime stats"
3102362354,1,WARNING,media_manager.c,"Requested to begin invalid operation %d."
3101786207,0,ERROR,overwrite_dimm.c,"Media interface DMA Queue Full"
3095790695,1,ERROR,feature_state_data.c,"DMA_STATUS_ERROR encountered while flushing feature state data ID: %d."
3094726427,0,ERROR,hw_init.c,"Failed to program safe vid to Rail D. Stop proceeding Rail D Floor Reduction."
3094555657,0,WARNING,sxp_commands.c,"Sxp ReadReg REQ bit still set after delay!"
3093887097,0,ERROR,fw_init.c,"Dynamic and Adaptive VDM features have both been disabled!"
3093691301,0,ERROR,power.c,"PLI is detected."
3093304175,0,DEBUG,life_span.c,"Percent Remaining alarm tripped"
3092562421,2,ERROR,pmic.c,"PMIC Write Failure: Address 0x%X, Error Code %d"
3089734526,3,INFO,ddrt_sense_amp_calibration.c,"CMD Fub: %d, SA Offset: %d, ACIO_DATA field : 0x%x"
3088150814,1,ERROR,assert.c,"ESP +  8: 0x%X [      Stack Pointer (ESP)       ]"
308725301,4,ERROR,kernel.c,"D_PWM_STS:0x%08X  D_PWM_MASK:0x%08X  NC_APIC_ISR:0x%08X  NC_APIC_IRR: 0x%08X"
3086317004,1,ERROR,commands.c,"BIOS Api version set to 0x%X"
3085509631,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtDqBcomCtrl: 0x%x"
3085439140,2,ERROR,core_dump.c,"LP OutputPayload Addr: 0x%08x_%08x"
308527709,1,ERROR,ras.c,"0x%08X: fault data is not valid!"
3085127488,1,ERROR,sxp_scheduler.c,"BGF_A_READY timed out with register value: 0x%X"
3083770158,3,INFO,dpa_for_pda.c,"0x%08X: DMA for line %d failed with status 0x%08X"
3083101651,0,INFO,sxp_scheduler.c,"Ten Device Read!"
3081645491,0,WARNING,command_fw_update.c,"Invalid packet number"
3081015667,2,ERROR,core_dump.c,"RefreshState - Sleep Time Stamp         : 0x%08x_%08x"
3080240682,0,ERROR,task_media_interface.c,"DMA command failed with AHB error twice in a row!"
3079843795,2,ERROR,fw_activate.c,"Fatal Activation error: 0x%08x, transaction fatal: 0x%x"
3079109503,0,DEBUG,command_features.c,"Set Features: Optional Configuration"
3078337805,0,ERROR,ltec.c,"LTEC received DDRT training VID update request while another is pending."
3076993954,1,ERROR,ait_dram.c,"Fatal Error: DRAM loading stall detected at the index 0x%x!"
3074352221,2,ERROR,commands.c,"Cmd Format Device, DMA returns a failure status. ""sxp address:  0x%08X_%08X"
3073193137,2,DEBUG,security_interface.c,"Security Free Pool -> QueueCount: %d, QueueEntries: %d"
3068178900,0,DEBUG,platform_config_data.c,"PCD_DmaDataSmallPayload: Enter"
3067537367,1,ERROR,nlog.c,"Failed to retrieve Nlog error: 0x%08X"
3067021207,2,ERROR,sxp_write_leveling.c,"SXP Coarse WrLvl failed rank[%d] bytePassFlag[%x]"
3066416716,7,ERROR,dma_polled.c,"Uncorrectable error! FaultData 0x%08X_0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
3065471632,0,DEBUG,scheduler_ddrt.c,"lockFailCounter is about to wrap"
3064281438,0,ERROR,core_dump.c,"Cpu Registers:"
3063947187,1,ERROR,log_emask_imask_regs.c,"MSC_EMASK: 0x%x"
3063250705,1,DEBUG,command_reset_policies.c,"0x%08X"
3061804478,1,INFO,error_logging.c,"Loading log %d"
3058350698,0,DEBUG,command_features.c,"Set Admin Features: Viral Policy"
3057999695,0,ERROR,crypto_selftests.c,"3DXP XTS-AES-256 Encryption Test FAIL: Result does not match expected KAT output."
305610300,0,ERROR,power_loss_log.c,"Could not load a PLI log (A) due to polled DMA error"
3055823188,0,ERROR,data_path_error.c,"Dclk is not enabled when handling DA FIFO U/O Flow errors."
3054505382,2,DEBUG,algo_tx_dq_dqs_training.c,"new dq delay for byte %d is %d"
3054086682,1,ERROR,data_path_error.c,"DN FIFO U/O Flow Errors: 0x%08X"
3052705590,1,DEBUG,barlow_creek_pmic_init_reason.c,"PMIC Fault Code[i] Raw Data 0x%x"
3052638,0,ERROR,security_interface.c,"Couldn't queue SHA-256 SDMA security request"
3052436573,1,ERROR,address_verify_error.c,"sDramData.FWP: 0x%08x"
3050394962,0,ERROR,feature_state_data.c,"FSD loaded but init was not saved in FWS"
3050285477,0,INFO,ait_dram.c,"Resume DRAM Load"
3049419529,0,ERROR,sxp_init.c,"Writing Training report to SPI failed"
3048151383,1,STATUS,spi_flash_driver.c,"Processing flash driver request took %d ticks"
3047166207,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr1: 0x%x"
3044453904,0,WARNING,command_features.c,"Invalid Mailbox SubOpcode"
3043217258,4,ERROR,dynamic_vdm.c,"Dynamic VDM SxpCmd_SendCommandWriteRegister failed on rank : %d, die : %d, address : 0x%08X, value : 0x%08X"
3042156753,0,ERROR,sxp_rank_interleave.c,"Unknown or mixed SXP devices, cannot set rank interleaving."
3041814260,1,ERROR,platform_config_data.c,"PCD Partition Invalid [%x]"
3040947142,0,ERROR,get_media_statistics.c,"Unknown stat total requested"
3040388177,2,ERROR,wear_level_move.c,"AitPolled_WriteReverseMap Failed on Entry Address 0x%08X_0x%08X: "
3040198829,0,DEBUG,command_features.c,"SS: S3 Resume Authenticate"
30378429,0,ERROR,error_logging.c,"Error log initialization failed. Not returning error logs."
3037521687,1,ERROR,core_dump.c,"ViralPolicy - Enable: 0x%02x"
3036440867,0,INFO,security_interface.c,"SecurityInterface_Initialize completed."
3036065019,1,ERROR,adaptive_vdm.c,"AdaptiveVdm_SetSampleErrorThresholds requested for invalid rank count : %d"
3036063689,3,STATUS,commands.c,"BIOS Api version set to 0x%X, FW API: 0x%X, Handshake API: 0x%X"
3035053289,0,DEBUG,command_features.c,"Set Admin Features: System Time"
303402547,2,ERROR,write_count_histogram.c,"Received more than expected steps for data retrieval. Number of steps: expected = %d, actual = %d"
30331950,3,DEBUG,dpa_for_pda.c,"0x%08X: block dpa 0x%08X has RO %d"
3032707114,1,ERROR,log_power_event_end.c,"D_FW_STATUS: 0x%x"
3031529676,0,INFO,wear_level_move.c,"FBE: Address is within spare block region"
3031527353,0,WARNING,command_features.c,"Invalid payload configuration"
3031403355,0,WARNING,command_log.c,"DMA Transfer Failure"
3031167502,0,INFO,ddrt_scheduler.c,"DDRT_RestoreRegisters!"
3030894458,0,WARNING,fw_img_auth.c,"Vendor ID invalid"
3030667191,0,ERROR,kechika_river_pmic_driver.c,"Unable to disable power on reset due to null pointer"
3028982217,1,ERROR,spi_migration.c,"SPI write failed when trying to save migration data (failedDie = %d)"
3027012275,1,ERROR,datastore.c,"Dropped token %d"
3026924350,0,ERROR,sxp_training.c,"Sxp Mrc Programming Error: No Table Date Found"
3026915037,0,ERROR,write_count_histogram.c,"WriteCountHistogram: Buffer address is 0x0"
3025426852,1,ERROR,log_power_event_end.c,"CHN_WCTL: 0x%x"
3024269313,2,ERROR,fconfig.c,"ParseAndUpdateTokens entry beyond buffer Token: 0x%X DwordLen: 0x%X"
3019136029,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz1: 0x%x"
301794405,1,ERROR,write_disturb_engine.c,"WD Threshold value (%d) is not supported"
3016718667,1,ERROR,log_emask_imask_regs.c,"CHN_IMASK_2: 0x%x"
3016510821,0,ERROR,dynamic_vdm.c,"Dynamic VDM cannot apply media policy to this DIMM! Either S2X or old S15 media has been detected."
3015806901,0,WARNING,key_management.c,"Security Metadata is not valid"
3015330325,4,STATUS,mm_wear_level_move.c,"HW WLM PLI timeout detected. Source DPA: 0x%08X_0x%08X Destination DPA: 0x%08X_0x%08X"
30151481,0,ERROR,format_device.c,"Cmd Format Device, failed to disable energy meter."
3014733012,5,ERROR,exception.c,"Exception: Instruction Pointer(eip) = 0x%x, Stack Pointer(esp) = 0x%x, info1 = 0x%x, info2 = 0x%x, eflags = 0x%x"
3013848052,2,DEBUG,data_path_error.c,"Illegal Access Occurred on AHB 0x%x, Error Index: %d"
3013184312,0,WARNING,fw_img_auth.c,"Header length invalid"
3012612830,1,ERROR,command_fw_update.c,"Error erasing SPI 4K range starting from 0x%x"
3012610373,0,ERROR,kechika_river_pmic_driver.c,"Cap self test getting result failed."
3011079180,5,ERROR,ddrt_scheduler.c,"ERROR: DDRT PLL did not lock before timeout MSC_FNVIO_INIT_CONTROL_0=0x%X, MSC_FNVIO_INIT_CONTROL_1=0x%X, D_DDRT_DCLK_CTRL=0x%X, MSC_FNVIO_VISIBILITY_CSR=0x%X, MSC_PLL_CTRL=0x%X"
30094654,0,INFO,address_scrub.c,"Address Range Scrub Stopping from Abort"
3008472497,1,ERROR,security_md_flush.c,"Wrong power event notification: %d"
30032318,1,ERROR,log_refresh_pointers.c,"P_RP_PDA_L: 0x%x"
3000968081,1,ERROR,nlog_chn_fwrwcmd.c,"CHN_FWRWCMD2: 0x%x"
3000833356,1,ERROR,context_block.c,"CB modified offset 0x%X while clean"
2999568010,0,WARNING,debug_log_data.c,"DMA transfer failed"
2997819336,0,ERROR,address_scrub.c,"Failed to get handle for DMA. Stopping Address Range Scrub"
2997068026,3,ERROR,ait.c,"AIT Log: Valid bit not set! base = 0x%x, lo = 0x%x, hi = 0x%x"
2996950804,1,ERROR,sxp_init.c,"Read DQ-DQS Training failed, Rank: %d"
2996723925,1,ERROR,buffers.c,"Invalid Buffer. Buffer address = 0x%08X. Going transaction fatal."
2994764455,1,ERROR,data_path_error.c,"DA FIFO U/O Flow Errors: 0x%08X"
2993006676,1,ERROR,log_power_event_end.c,"D_PWM_MASK: 0x%x"
2991169528,0,DEBUG,task_command_handler.c,"Mailbox Success"
2990135467,2,ERROR,core_dump.c,"HW CSR Address: 0x%08x Value: 0x%08x"
2990055393,1,ERROR,sxp_scheduler_init.c,"Invalid 3DXP DeviceID Fconfig token value: 0x%x"
2989902514,0,STATUS,command_features.c,"Config Lockdown Executed"
2986858585,0,DEBUG,command_inject_error.c,"Enabling poison on 4 cache lines"
2986404680,0,ERROR,thermal_manager.c,"Exiting thermal throttling"
2986109988,0,INFO,ait_update.c,"Ait Update Main Line State: Success Status!"
2984745111,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingRc0E: 0x%x"
2984715752,2,INFO,task_command_handler.c,"Currently in training, command not allowed: M[%x]m[%x]"
2984468308,1,ERROR,log_emask_imask_regs.c,"MCU_EMASK: 0x%x"
2983506971,0,WARNING,power_loss_log.c,"Requested PLI Log page is out of bounds"
2983363622,0,ERROR,fw_activate.c,"FW activate setup failed"
298256280,0,ERROR,sxp_commands.c,"RDWR_BUF_CTRL LINE_AVAIL did not return to idle"
2981365587,1,ERROR,algo_xover_calibration.c,"Xover calibration failed due to invalid edges. CmdFub[%d]"
2981263018,0,ERROR,adma.c,"Attempted DMA with invalid input."
2981123838,7,ERROR,dma_polled.c,"Address Verify Error! DPA 0x%08X_0x%08X PDA 0x%08X_0x%08X FaultData 0x%08X_0x%08X_0x%08X"
2980270064,0,DEBUG,crypto_selftests.c,"Read the decrypted Test Buffer from SXP executed."
2980268336,0,ERROR,command_fw_update.c,"Small Payload: DMA read of block of image failed"
2980219992,8,ERROR,dpa_verify_error_handler.c,"Address Verify Error. DPA 0x%08X_0x%08X PDA 0x%08X_0x%08X FaultData 0x%08X_0x%08X_0x%08X STYPE 0x%02X"
2980127128,3,ERROR,sxp_trim_bundle.c,"Could not populate AdReset %d from 0x%04x. Register Data: 0x%04x"
2979231478,0,WARNING,command_features.c,"The DDRT Alert Policy data is not valid - non-zero reserved bits!"
2978906722,2,ERROR,ddrt_scheduler.c,"Ddrt Mmrc Table Checksum did NOT match: c[0x%08x] != t[0x%08x]"
2978876291,1,ERROR,error_logging.c,"Wrong power event notification: %d"
2978065020,1,ERROR,kechika_river_pmic_driver.c,"Message Handler incorrectly called with message: %x"
2977763147,0,WARNING,dfx.c,"Mismatching module COMMIT ID with firmware COMMIT ID"
2975283869,9,ERROR,task_error_handler.c,"Uncorrectable error! Source Transaction Type 0x%02X; Initial VDM 0x%02X; Final VDM 0x%02X; FaultData 0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
2974842972,0,ERROR,throttling_engine.c,"A request to modify power credits was dropped since DIMM is in thermal throttling state"
2971712518,4,ERROR,update_firmware.c,"FW Update has successfully staged FW %02x.%02x.%02x.%04x."
2970963032,2,ERROR,wear_level_move.c,"FreeBlockExpansion_Transition Could not refresh all source lines of pda 0x%08X_%08X"
2970914,0,ERROR,wear_level_move.c,"Invalid Firmware State Data, Wear Level Resume State Machine could not complete!"
2969867546,1,ERROR,die_error_emulator.c,"Invalid relative VDM level %d"
2969097227,0,WARNING,task_security.c,"Unable to disable passphrase: Encryption Disabled"
2957417507,1,ERROR,media_manager_engine.c,"WLM Threshold in PW_WCCTRL had an unexpected value: %d. Re-initializing WLM threshold"
2957011891,1,DEBUG,checkpoint.c,"Update SMB Ready: %d"
2956426286,0,ERROR,power_wake_isr.c,"Warm reset entry is detected in PC6 transition flow"
2956341397,2,ERROR,security_md.c,"Security md version doesn't match on copy %d, version = 0x%08x"
2955915800,9,ERROR,dma_polled.c,"DMA Polled STYPE AIT UECC. Source Transaction Type 0x%02X; Initial VDM 0x%02X; Retry Index 0x%02X; Fault data 0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
295550555,0,ERROR,wear_level_move.c,"Bad Block Check read check FAILED!"
2955007302,0,STATUS,feature_state_data.c,"FSD Access Fconfig is set to SRAM, skipping FSD flush!"
2954316270,1,ERROR,nlog_chn_fwrwcmd.c,"CHN_FWRWCMD3: 0x%x"
2953691975,0,ERROR,dpa_verify_error_handler.c,"This AVF error is on a RMW, do NOT complete transaction and go DIMM fatal!"
2952969384,1,ERROR,power_budgeting_engine_imf.c,"Invalid time constant %dms requested. Power budgeting engine applies the value but does not store in FW state."
2952139208,1,ERROR,security_reset.c,"Wrong power event notification: %d"
2951490977,2,ERROR,fw_image_sync.c,"Image Sync failed with error SPI Read at 0x%x in state %d."
2950731094,0,DEBUG,spare_block.c,"Spare Block threshold alarm tripped"
2950178058,1,ERROR,core_dump.c,"OtherStateInfo - Media Disabled State: 0x%x"
2948220721,0,INFO,power_budgeting_engine.c,"Energy Meter hasn't been started yet."
294658860,0,ERROR,sxp_init.c,"Saving SxpIo register values to SPI failed"
2946183352,2,WARNING,data_path_error.c,"data path error DPA 0x%08X_%08X"
2945902315,0,ERROR,update_firmware.c,"Unexpected mailbox may not remain locked throughout operation."
2945420397,2,ERROR,fw_image_sync.c,"Image Sync failed with error requesting SPI Read at 0x%x in state: %d."
2944606893,0,ERROR,fw_init.c,"Adaptive VDM feature has been disabled!"
294397588,0,DEBUG,overwrite_dimm.c,"Overwrite DIMM DMA Callback"
2941846067,2,ERROR,sxp_write_leveling.c,"SXP Coarse WrLvl failed rank[%d] nibble[%d]"
2941666334,1,ERROR,core.c,"Core General Message Handler called with invalid message id: 0x%X. Going transaction fatal."
2940384771,0,ERROR,nlog.c,"The following nlog had log level disabled, promoting to error"
2940043138,0,INFO,wear_level_move.c,"Block Move: Address is within spare block region"
2939853767,2,INFO,ddrt_scheduler.c,"DDRT locked at %d us after %d tries"
2939623857,1,ERROR,ait_read_line.c,"Invalid handle after ait readline dma completed. Handle 0x%X."
2938894042,0,WARNING,address_scrub.c,"Address Range Scrub Error Found"
293875116,2,ERROR,command_features.c,"Illegal Write request detected in register = 0x%08X with bitmask = 0x%08X"
29380347,1,ERROR,kechika_river_pmic_driver.c,"PMIC Rail A set to [%d] as W/A since svid fuse returned 0x00"
2937876835,5,ERROR,die_error_emulator.c,"DieErrorEmulator: Invalid relative VDM level (VDM%d) for VDM%d. Valid levels are %d, %d and %d"
2937829876,1,ERROR,log_emask_imask_regs.c,"A_EMASK: 0x%x"
2937658944,1,ERROR,task_media_interface.c,"AitWrite. Invalid level provided. 0x%X."
2936910900,0,ERROR,ait_read_line.c,"MediaInterface handle returned NULL. AIT Read Failed."
2935149553,0,WARNING,dfx.c,"Mismatching module ID and ID received in input payload"
2931529651,1,DEBUG,core_dump.c,"Data: 0x%X"
2930549422,1,ERROR,sxp_scheduler_init.c,"Sxp_FirewallResetPin failed to write to SXP_MSR1 register rank: %d"
2929811780,0,WARNING,task_command_handler.c,"Unsupported command"
292969950,4,ERROR,sxp_scheduler.c,"SXP Mixed DeviceID detected [%d] != [%d] at rank=%d die=%d"
2929300870,1,ERROR,io_csr.c,"IO CSR invalid parameter command fub = 0x%x"
2928222473,1,ERROR,fconfig.c,"ParseAndUpdateTokens failed zero length Token: 0x%X"
2928093493,3,STATUS,warm_reset.c,"Warm Reset Start : Latch status = %d | eADR knob = %d | eADR Flush Status = 0x%X "
2927043487,0,DEBUG,task_error_handler.c,"Task_ErrorHandler Init"
2926423535,0,ERROR,power_event_at_image_auth.c,"Image sync timer was not initialized"
2924520325,2,DEBUG,error_logging.c,"Error Log size is 0x%08X and available size is 0x%08X"
2924422325,3,WARNING,core_wear_level_move.c,"FBL head pointer not in valid range. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
2923208697,2,ERROR,skip_img_sync_at_ddrt_training.c,"Skipping image sync in power up: %d, training state: %d"
2922751238,1,ERROR,core.c,"MessageHandler was previously set for this message id: 0x%X."
2921235950,4,ERROR,algo_write_leveling.c,"SXP Fine WrLvl failed due to invalid edges. Rank[%d] Byte[%d] Rising Edge[%d] Falling Edge[%d]"
2917354170,0,ERROR,write_count_histogram.c,"Start address > stop address"
2917125238,0,WARNING,task_security.c,"NULL command received"
2916387208,1,ERROR,log_pli_io_trig.c,"MSC_FNVIO_INIT_CONTROL_1: 0x%x"
2916218528,0,WARNING,command_features.c,"Invalid Value for Vendor Specific Additional Settings"
2916033253,0,DEBUG,key_management.c,"Unwrapping S3 Saved Persistent Memory Keys"
2915040619,0,WARNING,command_features.c,"Invalid PCD payload type"
2913449630,0,ERROR,crypto_selftests.c,"3DXP XTS-AES-256 Encryption self-test failed!"
2912400654,0,ERROR,ait_dram.c,"DRAM Loading stall detected."
2912124046,0,ERROR,sxp_device_access.c,"SXP Devices do not have Persistent ID fused. Cannot apply desired device mode."
2911413081,1,STATUS,thermal_engine.c,"Forced temperature calibration workaround, set: %08X"
2909022318,2,ERROR,message_channel.c,"Window Access READ Fail  Address = 0x%X, ReadData = 0x%X"
2907647125,0,DEBUG,task_security.c,"SECURITY_FREEZE_LOCK"
290676916,0,ERROR,log_zqcal_short.c,"Flush of Nlog buffer to media has occurred."
2906208611,0,ERROR,reg_flow.c,"RF Table Error: No Table Found"
290619377,1,ERROR,core_dump.c,"RefreshState - State                    : 0x%02x"
2905986954,0,INFO,command_log.c,"Get FW Image Info"
2905882347,1,ERROR,ait_read_line.c,"Invalid handle after ait readline dma completed. Handle 0x%X."
2904811528,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr4: 0x%x"
2904725676,0,ERROR,power_budgeting_engine.c,"Energy Meter is paused for more than 2 accumulation windows."
2899747600,2,ERROR,fconfig.c,"ParseAndUpdateTokens entry beyond buffer Token: 0x%X DwordLen: 0x%X"
289638244,0,ERROR,key_management.c,"Failed to wrap PM-RK with security disabled wrapping key"
2896093283,0,ERROR,thermal_manager.c,"Invalid power credits value. PCSCLR_PWR_CFG7 CSR should have a non zero value"
2895501119,1,DEBUG,ddrt_scheduler.c,"DDRT Divider Ratio is: 0x%08x"
2894629236,0,ERROR,read_write_pmic.c,"Vendor Specific Register Requested field had unexpected value. Assuming default register request."
2894004164,0,ERROR,dma_polled.c,"Started polled DMA when a DMA hadn't completed, not in PLI. Shouldn't be possible."
2892271577,0,WARNING,debug_log_data.c,"DMA write to large payload region Error"
2891528302,2,INFO,fw_image_sync.c,"Copying SPI from 0x%08X to 0x%08X"
2890285934,1,ERROR,read_write_pmic.c,"During processing I2C request DDRPHY_SXP_TOP_SXPHSIO_SCH_PWR_CFG7: 0x%08x"
2889452464,1,ERROR,log_emask_imask_regs.c,"DA_EMASK_1: 0x%x"
2889439757,0,WARNING,command_features.c,"Disabling Address Range Scrub"
2888175656,0,DEBUG,command_features.c,"Get Admin Features: DIMM Partition Info"
2887820365,1,ERROR,sxp_trim_bundle.c,"Could not populate ResetPulseEn value 0x%02x for write."
2884718653,0,ERROR,sxp_training.c,"SXP timing tables are unversioned!"
2884571374,0,ERROR,ltec.c,"LTEC disabled for PMIC rail VCCDDRD_DDRT (D) due to media device firewall reset failure."
2884481530,1,ERROR,log_pli_io_trig.c,"PC_AVDM_CTRL: 0x%x"
2882943976,1,WARNING,fconfig.c,"Fconfig_SetConfig unknown token Token: 0x%X"
2880624050,1,ERROR,nlog_region_lock.c,"D_PM_REG_LOCK: 0x%08x"
2880243337,0,WARNING,key_management.c,"Security Metadata Interface pointer is NULL"
2879474883,0,ERROR,i2c_bus_manager.c,"FW attempted to issue an I2C bus request with a NULL request routine."
2879384947,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz0: 0x%x"
2878488034,0,DEBUG,aes_bulk_encryption_selftest.c,"Verify AES Bulk Encryption successfully decrypted the first cacheline."
2878475356,1,ERROR,reg_protect.c,"Write request detected in restricted region! (%08X)"
2877879007,0,ERROR,dynamic_vdm.c,"Dynamic VDM cannot apply media policy to this DIMM! Either S2X or old S15 media has been detected."
2877691059,3,DEBUG,i2c_master_driver.c,"TX FIFO is not emptied in time. IC_STATUS = 0x%x, IC_RAW_INTR_STAT = 0x%x, IC_TX_ABRT_SOURCE = 0x%x"
2876168995,0,ERROR,hal_pmic_cap_test.c,"Cap self test start failed."
2875355905,0,WARNING,command_features.c,"Not BIOS Mailbox"
2875170121,0,ERROR,update_firmware.c,"Failed to hash and commit image body to SPI"
2872473970,2,ERROR,aclk_periodic.c,"ACLK Calibration : SxpCmd_SelectId failed on rank : %d, die : %d"
2871626119,2,ERROR,core_dump.c,"OtherStateInfo - FwOccurence         : 0x%08x_%08x"
286815196,8,ERROR,fw_init.c,"Current FW version - %x.%x.%x.%04x, DIMM Unique ID - 0x%02x%08x%08x, Power Cycle count - %d"
2867344778,0,INFO,task_command_handler.c,"Part is LOCKED, completing dfx command as unsupported"
2866769012,0,ERROR,die_error_emulator.c,"DieErrorEmulator: DQ failure not supported due to package migration is in progress/already complete."
2864280979,3,WARNING,core_wear_level_move.c,"FBL tail pointer not in valid range. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
2864122576,0,WARNING,command_features.c,"Unable to update the SKU"
2863521394,0,ERROR,sxp_rmt_tests.c,"RAS Rx Dqs Max Mask Test Failed"
2863245831,0,STATUS,dpa_verify_error_handler.c,"Address Verify flow completed successfuly!"
2860833749,1,ERROR,fw_image_sync.c,"Image Sync Message Handler called with invalid state: %d"
2859735926,1,ERROR,ras.c,"RAS Log: Valid bit not set - DS_LOG_HOST_POISON_1 = 0x%x"
2856516837,2,ERROR,core_dump.c,"LP InputPayload Addr : 0x%08x_%08x"
2854917515,3,ERROR,core_dump.c,"FwState Data: Top[0x%x] | Bot[0x%x] | Valid[%d]"
2854536015,1,ERROR,log_power_event_end.c,"DRDP_WCRD_CONFIG: 0x%x"
2854194807,1,DEBUG,command_inject_error.c,"Current poison config: 0x%08X"
2853506647,0,WARNING,command_features.c,"Invalid PCD payload type"
2851872587,0,ERROR,fw_init.c,"Going DIMM fatal because the criteria for an unfinished shutdown flow has been met"
2849143441,1,ERROR,ras.c,"RAS Log: Valid bit not set - DN_LOG_RDATA_POSION_1 = 0x%x"
2848839284,1,ERROR,power_event_at_image_sync.c,"Picked up random image chunk: %d"
284856552,1,ERROR,pmic.c,"PMIC I2C Failed to initialize, err_code: %d"
2848114316,0,ERROR,write_disturb_engine.c,"Shouldn't receive request other than WD."
2847784239,0,ERROR,task_error_handler.c,"AIT Scrub fails at VERIFY state"
2847210311,2,ERROR,sxp_write_leveling.c,"Fine WrLvl failed Rank[%d] Byte[%d]"
2847026650,1,ERROR,core_dump.c,"RefreshState - Current Refresh Pointer  : 0x%08x"
2846912664,0,ERROR,ltec.c,"LTEC received multiple requests to enter normal mode. DDRT IO Init. sequence may be invalid"
2846641601,0,WARNING,smart.c,"No supported vendor found"
284625850,1,ERROR,context_block.c,"Wrong power event notification: %d"
2846128507,0,ERROR,wear_level_move.c,"No Spare block for FreeBlockExpansion move, DROPPING REQUEST!"
2843756551,2,WARNING,get_fconfig.c,"DFX get Fconfig incorrect version Expected: 0x%X, Actual: 0x%X"
2843398372,2,ERROR,dynamic_vdm.c,"Dynamic_IRST cannot identify microamp table for rank : %d, die : %d"
2842884201,2,ERROR,message_channel.c,"Window Access WRITE Fail  Address = 0x%X, WriteData = 0x%X"
2841862456,0,ERROR,task_error_handler.c,"AIT Scrub fails at SCRUB state"
2841216803,0,ERROR,fw_img_auth.c,"EAU signature padding verification (padding 1, 3 and 4) failed"
2840497993,2,ERROR,task_error_handler.c,"Uncorrectable DPA DMA was in AIT Address range. Byte aligned AAU_CTRL DPA = 0x%08X_%08X"
2840308524,3,ERROR,aes_bulk_encryption_selftest.c,"*** FAIL *** read data (0x%x), source data (0x%x), at byte offset %d"
2838913452,1,DEBUG,memory_info.c,"DFX Memory Info Page Requested - Denied [%x]"
2838410824,0,ERROR,ltec.c,"PMIC rails are at Boot VIDs at the time of LTEC failure."
2838337001,0,WARNING,task_command_handler.c,"Mailbox Failure"
2837594172,0,ERROR,context_block.c,"Context Block Initialization Failed"
2836502167,0,ERROR,sku.c,"Security SXP Access disabled, bypassing sku cipher checker"
2835646436,0,INFO,refresh.c,"Set First Fast Refresh"
2834487544,1,ERROR,command_fw_update.c,"Error writing to SPI block at address 0x%X during FW Update"
2834322138,6,ERROR,core_dump.c,"2LM Size: 0x%x_%x | PM Size: 0x%x_%x | PM Base Address: 0x%x_%x"
2833536468,0,DEBUG,task_security.c,"SECURITY_SET_S3_KEY"
282929756,0,WARNING,dfx.c,"Mismatching module build config and firmware build config"
2827689772,0,ERROR,sxp_training.c,"SPI write failed during saving IO registers!"
2827466363,0,ERROR,command_fw_update.c,"Failed header corruption because of a verification test failure"
2827376503,0,DEBUG,power_state.c,"PC6 Exit: Clock Started"
2826623367,1,ERROR,context_block.c,"DMA_STATUS_ERROR encountered while flushing context block ID: %d."
2825567922,2,INFO,sxp_training.c,"Sxp Mmrc Table Checksum MATCHED: c[0x%08x] == t[0x%08x]"
2823898578,1,ERROR,sxp_scheduler.c,"Unable to initialize media latencies. Invalid media device ID %d"
2823513782,4,ERROR,core_dump.c,"CB Datastore Id | Header Version | Entries Size : 0x%x | 0x%x | 0x%x [%d]"
2821877260,0,ERROR,task_error_handler.c,"AIT Scrub fails at SCRUB state"
2820447659,0,WARNING,task_command_handler.c,"NULL Command"
2818839812,3,ERROR,update_firmware.c,"State machine attempted to transition to unknown state %d. Current state/substate is %d/%d"
2818649053,0,INFO,fw_image_sync.c,"Starting Sync"
2818446047,0,DEBUG,command_features.c,"Set Admin Features: Clear History"
2817433944,0,ERROR,ddrt_training.c,"DdrtTraining_StartTraining- Failure at DDRT Sense Amp Calibration"
2814743698,0,ERROR,health_manager.c,"Life Span Percentage Remaining = 0"
2812729358,1,ERROR,core.c,"Core Message queued when queue was full with Message = 0x%X."
2811746,0,INFO,task_command_handler.c,"MBox Command Unknown"
2811687348,2,ERROR,sxp_init.c,"Coarse RcvEn Training failed, Rank: %d Training type: %d"
281064619,0,ERROR,security_interface.c,"Security interface queue enqueue request failed"
2809378087,0,INFO,core_dump.c,"Using checksum instead of SHA - CoreDumpInfo"
280890356,1,ERROR,assert.c,"ESP +  4: 0x%X [ Vec # |       EFLAGS           ]"
2807649352,1,ERROR,sxp_rcven_training.c,"FineRcvenTraining failed rank index[%d]"
280741622,7,ERROR,dma_polled.c,"Address Verify Error! DPA 0x%08X_0x%08X PDA 0x%08X_0x%08X FaultData 0x%08X_0x%08X_0x%08X"
2807176666,2,INFO,ddrt_scheduler.c,"Ddrt Mmrc Table Checksum MATCHED: c[0x%08x] == t[0x%08x]"
2805500779,0,DEBUG,dfx.c,"Upload via small payload complete"
2804198022,0,INFO,security_interface.c,"Security_CompleteRequestWithNoEvent completed"
2802397608,1,ERROR,core_wear_level_move.c,"FreeBlockExpansion_Dispatch unexpected AIT get line msg:%x"
2801976828,3,INFO,commands.c,"Cmd Format Device, Capacity: %08X_%08Xd in %d-byte chunks."
2799518096,0,DEBUG,ddrt_scheduler.c,"lockFailCounter is about to wrap"
2798396588,3,ERROR,block_move_error_handler.c,"WLM interrupt log info: wlm_interrupt_log = 0x%x, wlm_interrupt_log2 = 0x%x, wlm_log = 0x%x"
2796508954,1,WARNING,command_features.c,"Training already has been completed State=%d"
2796005977,0,ERROR,ddrt_scheduler.c,"Ddrt Mrc Programming Error: No Table Date Found"
2795961178,2,DEBUG,platform_config_data.c,"Offset Address: 0x%08X_%08X"
2795004625,1,ERROR,power_state.c,"PowerState_ProcessNewSignal: Unexpected Power State event [0x%x] detected."
2793677011,0,DEBUG,platform_config_data.c,"Set Partition Over DDRT"
2792096323,1,ERROR,kechika_river_pmic_driver.c,"PMIC Rail D set to [%d] as W/A since svid fuse returned 0x00"
2791704532,1,ERROR,ras.c,"Host poison at the DPA address 0x%x"
2790982251,0,ERROR,log_msc_spare_ctrl.c,"Normal mode."
2790731460,1,DEBUG,breakpoint.c,"Breakpoint: %d"
2789667012,1,ERROR,get_ait_info.c,"A_LVLNM1_BASE_DPA: 0x%x"
2789036420,1,ERROR,power_state.c,"PowerState_ProcessNewSignal: Unexpected Power State event [0x%x] detected."
2788820722,0,ERROR,sxp_init.c,"Sxp_XoverCalibration failed"
2787464800,0,WARNING,task_security.c,"Unable to set S3 Resume passphrase: Encryption Disabled"
2787224500,1,STATUS,sxp_device_access.c,"3DXP Devices do not have Persistent ID fused on rank[%d]. Forcing 11 Device Mode"
2786010946,0,WARNING,command_inject_error.c,"Dma transfer not completed"
278554729,1,ERROR,sxp_scheduler.c,"Invalid 3DXP Device ID 0x%04x"
2783484693,1,ERROR,core_dump.c,"FwDebugData - bootCycleCount: %d"
2783206845,1,ERROR,sxp_reg.c,"Unsupported 3DXP media device type: 0x%08x"
2782911791,2,WARNING,command_features.c,"Invalid set power management params. Values do not meet minimum, maximum, or granularity requirements. peakPowerBudget == %dmW ; averagePowerBudget == %dmW"
2781892701,0,ERROR,thermal_manager.c,"Entering thermal throttling"
2781280945,1,DEBUG,commands.c,"Size of IdentifyData - %d"
2778869098,1,ERROR,get_ait_info.c,"A_LVLN_BASE_DPA: 0x%x"
2777660831,0,INFO,fw_img_auth.c,"Verifying decrypted hash"
2777647348,0,ERROR,buffers.c,"Core Buffer released when queue was full. Going transaction fatal."
2777353932,3,ERROR,ait_dram.c,"Platform API set -- DRAM Able to load: %d, Drift tracking ready: %d, load status: %d"
2775094495,0,ERROR,ddrt_training.c,"DdrtTraining_StartTraining- Failure at DDRT Sense Amp Calibration"
2775054410,4,STATUS,barlow_creek_pmic_init_reason.c,"Fault Code 0 = 0x%x, Fault Code 1 = 0x%x, Fault Code 2 = 0x%x, Fault Code 3 = 0x%x"
2774994519,0,WARNING,spi.c,"Write: Invalid Address or Transfer Size"
2773036747,2,ERROR,command_features.c,"Unexpected Command <Normal Mode Complete> for BIOS API: 0x%X | FW API: 0x%X"
2772836453,1,STATUS,ddrt_scheduler.c,"DDRT MMRC Revision %d"
277203329,1,ERROR,log_power_event_end.c,"D_PWM_STS: 0x%x"
2771768436,0,ERROR,dram_failure_trigger.c,"DRAM initialization status was corrupted."
2770288492,1,ERROR,log_emask_imask_regs.c,"AITDR_RAS_IMASK: 0x%x"
2767102498,0,ERROR,dpa_verify_error_handler.c,"AVF happens with DRAM disabled, complete the transaction and go DIMM fatal!"
2763024904,0,ERROR,platform_config_data.c,"Invalid Small Payload Part during set operation"
2761554613,1,ERROR,wear_level_move.c,"Free Block Expansion: Relocate Block reported an error %d on move operation"
2761211217,0,ERROR,mm_block_move.c,"HW WLMQ could not be restored due to invalid value of entriesCount"
276018554,1,ERROR,log_emask_imask_regs.c,"MSC_EMASK: 0x%x"
2759901550,1,ERROR,log_emask_imask_regs.c,"A_EMASK_1: 0x%x"
2759897094,0,ERROR,power_loss_log.c,"Could not load a PLI log (B) due to polled DMA error"
2759852311,0,DEBUG,task_command_handler.c,"Calling Security Interface Initialization"
275902566,2,ERROR,sxp_trims.c,"0x105 register read failed. Can't check media type on Rank: %d, Die: %d"
2758594818,0,WARNING,dfx.c,"Uploaded module's header is not valid!"
2757489856,2,INFO,ras.c,"pw_ras_interrupt_req is 0x%08X, fault data mask is 0x%08X"
275695823,0,DEBUG,cpgc.c,"Provide data pattern or set the zeroPattern flag to true"
2755460297,0,DEBUG,pmic.c,"PMIC Write Error"
2755382005,3,WARNING,task_error_handler.c,"Error found for domain %u ferr_%u bit %u, no handling other than clearing the bit"
2755036051,0,ERROR,ltec.c,"LTEC requested to enter normal update mode after it has been disabled."
2754495377,0,ERROR,command_log.c,"CEL entries did not fit in the buffer."
2753843747,6,ERROR,barlow_creek_pmic_init_reason.c,"Fault Code 0 = 0x%x, Fault Code 1 = 0x%x, Fault Code 2 = 0x%x, Fault Code 3 = 0x%x, Fault Code 4 = 0x%x, Fault Code 5 = 0x%x"
2753252500,1,ERROR,fw_image_sync.c,"Image Sync Abort called while Image Sync was in state: %d."
2750520886,1,ERROR,sxp_init.c,"After trim change ZQCalLong command failed for rank: %d"
2748533406,2,ERROR,sxp_init.c,"Coarse RcvEn Training failed, Rank: %d Training type: %d"
2747410043,0,ERROR,update_firmware.c,"Tried to do a production FW update while running debug image"
2747099816,0,ERROR,sku.c,"Unable to save updated sku with soft programmable cleared"
2745867358,1,ERROR,ait_dram.c,"DRAM loading stall detected at the index 0x%x!"
2745043107,3,INFO,sxp_training.c,"SXP Ranks: %d, DRAM Ranks: %d, Dies: %d"
2743674230,1,WARNING,media_manager.c,"Requested to begin invalid operation %d."
2740935525,0,ERROR,power_loss_log.c,"At least one PLI log was corrupt from last PLI."
2740687896,1,ERROR,fw_init.c,"WDB flush timeout - P_PWM_STS = 0x%X"
2740616336,0,DEBUG,task_security.c,"SECURITY_SET_NONCE"
2739749379,1,ERROR,log_emask_imask_regs.c,"PW_EMASK_0: 0x%x"
273950803,1,ERROR,nlog_chn_fwrwcmd.c,"CHN_FWRWCMD1: 0x%x"
2736415764,0,STATUS,command_software_triggers.c,"Injected package sparing software trigger error"
2735304917,3,DEBUG,spi.c,"Spi_Read sramAddress: 0x%08X, spiAddress: 0x%08X, size: 0x%08X"
273463594,0,DEBUG,command_inject_error.c,"Clear poison DPA out of mapped range."
2733812374,1,ERROR,fw_init.c,"WDB flush timeout - P_PWM_STS = 0x%X"
2733354139,0,ERROR,fw_activate.c,"FW activate detected invalid signature in saved runtime data"
2730919399,1,ERROR,get_ait_info.c,"A_LVLNM2_BASE_DPA: 0x%x"
2730625815,1,ERROR,power_budgeting_engine.c,"Energy Meter timer is shorter than I2C sequence execution time. em_status = 0x%x"
2730314016,1,ERROR,ait_dram.c,"AIT DRAM Controller Errors: 0x%08X"
2730297960,1,ERROR,short_stroke.c,"Short Stroke Size %d is invalid"
2729053668,2,ERROR,ddrt_sense_amp_calibration.c,"No transition found for DDRT Sense Amp Calibration CMD Fub %d cmd line: %d"
2727647916,0,DEBUG,core_wear_level_move.c,"WLM state machine calling complete!"
2727542813,1,ERROR,log_emask_imask_regs.c,"DN_IMASK: 0x%x"
2725634549,0,INFO,security_interface.c,"security SubmitWork RequestQueue was full FAIL."
2724209681,2,ERROR,sxp_trim_bundle.c,"Could not determine TcHnMirrorSelect%d from 0x%04x"
2724122506,1,WARNING,error_logging.c,"Failed to load Error Log %d"
2722199712,1,ERROR,address_scrub.c,"ARS being failed due to an invalid handle 0x%X."
27218446,1,ERROR,pmic.c,"PMIC I2C Failed to initialize, err_code: %d"
2721701688,0,ERROR,security_md.c,"Security MD rebuild, Security MD flush failed."
2720022331,1,INFO,power_budgeting_engine.c,"Energy meter was paused for %d msec."
2718246772,0,ERROR,power_budgeting_engine.c,"Wrong Coulomb count CSR address offset has been programmed in Energy Meter."
2717773814,1,ERROR,short_stroke.c,"Short Stroke Size %d is not a power of 2"
2716822002,0,ERROR,core_dump.c,"PowerLossLog Checkpoints:"
2715804075,2,STATUS,block_move_error_handler.c,"HW WLM Block Move timeout, pw_wcsts: 0x%X rpq_wdb_stat_empty_nddrt: 0x%X"
271487862,1,ERROR,write_disturb_engine.c,"Write Disturb Threshold in PW_WCCTRL had an unexpected value: %d. Re-initializing WD threshold"
2714495279,2,ERROR,sxp_trim_bundle.c,"Could not populate TcP3MirrorStep%d for 0x%04x"
2713069408,0,ERROR,ait_update.c,"AIT Update Backup Line State: Failure Status!"
2712588192,0,INFO,task_security.c,"Task_security processed Security_GetSecurityRequest"
2709683713,1,WARNING,get_fconfig.c,"DFX Get Fconfig incorrect transfer type: 0x%X"
2708245422,0,ERROR,command_inject_error.c,"Media temperature error injection is disabled"
2707637896,9,ERROR,dpa_verify_error_handler.c,"Address Verify Error. DPA 0x%08X_0x%08X PDA 0x%08X_0x%08X FaultData 0x%08X_0x%08X_0x%08X STYPE 0x%02X yieldAllowed %d"
2706894455,0,ERROR,fw_init.c,"Unsupported Device ID, regflow table is not loaded"
2705130378,0,ERROR,core_dump.c,"CsrDumpListTable overflowing"
2704751124,1,ERROR,nlog_config_lockdown.c,"D_FW_STATUS_H: 0x%x"
2703235571,0,DEBUG,command_features.c,"Get Admin Features: Config Lockdown"
2702372438,2,ERROR,power_loss_log.c,"Sequence error occurred in previous PLI. PLI LogA sequence number (%d) LogB (%d)"
2701983985,1,ERROR,task_media_interface.c,"DMA command %x failed, PSN or SXP error"
2701502151,1,WARNING,debug_log_data.c,"Failed to get persistant storage address at line %d."
2700012327,1,ERROR,pli_host_throttling_check.c,"DRDP_WCRD_THRES: 0x%x"
2699916718,1,ERROR,data_path_error.c,"CSR Error, valid bit not set in log registers! FnvError %d."
2699471314,0,ERROR,leaky_bucket.c,"Unknown stat requested"
2696951229,0,INFO,address_scrub.c,"Starting Address Range Scrub"
2696722057,1,ERROR,core_dump.c,"CallStack Logging started: 0x%X"
2692655478,3,ERROR,core_dump.c,"Ait Base Address: 0x%x_%x | AitTableWrapCount: 0x%x"
2691755995,0,ERROR,algo_tx_dq_dqs_training.c,"Calculated ODT On latency was somehow out of range, failing."
2690853048,0,ERROR,core_dump.c,"PowerLossLog:"
2688693506,0,ERROR,log_vsm_state.c,"Dynamic VDM Stop Media Access state: success."
268856042,8,ERROR,core_dump.c," - EAX: 0x%08x | EBX: 0x%08x | ECX: 0x%08x | EDX: 0x%08x | ESI: 0x%08x | ESP: 0x0%08x | EBP: 0x%08x | EIP: 0%08x"
2686950621,1,ERROR,thermal_manager.c,"Component[%d] temperature samples taken in three consecutive 100ms window are bad. Going transaction fatal."
2686665712,0,ERROR,block_move_error_handler.c,"Hardware wear level move: WLM filtering CSR access timeout!"
2686534093,0,WARNING,command_features.c,"Only 2LM enabled SKU"
2686424615,0,DEBUG,aes_bulk_encryption_selftest.c,"Enable Decryption Bypass"
2686383306,2,ERROR,fw_image_sync.c,"The non-loaded slot at address 0x%X failed authentication %d times"
268586208,0,ERROR,nlog.c,"Error detected with managing nlog SRAM pointers"
2685533044,0,DEBUG,aes_bulk_encryption_selftest.c,"Write Bulk_Encryption source data to SXP"
2684745767,1,ERROR,log_power_event_end.c,"PowerStateEvents: 0x%x"
2684649531,1,ERROR,core_dump.c,"***** CoreDump End: %x   *****"
2684410116,0,ERROR,log_block_move_ait_update.c,"Block Move Ait Update started."
268362744,0,ERROR,block_move_error_handler.c,"Hardware wear level move: WLM CSR response error!"
2683345914,0,DEBUG,dfx.c,"Upload via large payload complete"
2683211580,3,ERROR,data_path_error.c,"This error domain %d ferr_%d bit %d causes transaction fatal!"
2682193501,0,ERROR,hal_pmic_rail_cwv.c,"Rail A VID is not fused."
2681514547,1,ERROR,sxp_init.c,"CPGC Test Failed on rankIndex %d"
2680960072,0,INFO,ddrt_restore.c,"Ddrt_Restore -> No timer needed"
2678721435,0,WARNING,security_interface.c,"SHA SDMA security request timed out"
2678610796,0,ERROR,sxp_device_access.c,"Fconfig Partial Read Mode value is invalid. Forcing 11 Device Mode."
2677030595,0,DEBUG,task_security.c,"SECURITY_SET_PASSPHRASE"
2675899241,0,DEBUG,wear_level_move.c,"AIT Update Callback"
2675753522,1,ERROR,log_power_event_end.c,"P_PWM_STS: 0x%x"
2675698932,0,INFO,ddrt_scheduler.c,"DDRT Gate Pll!"
2674833360,1,ERROR,fw_image_sync.c,"Image Sync Message Handler called with invalid state: %d"
2673546156,0,ERROR,core_dump.c,"Current Mailbox Data:"
2672372381,0,ERROR,kechika_river_pmic_driver.c,"CAP test cleanup request denied. I2C bus request queue is full."
267181114,0,ERROR,dpa_verify_error_handler.c,"AVF happens with DRAM disabled, complete the transaction and go DIMM fatal!"
2671626912,3,ERROR,thermal_manager.c,"Controller: %d C; Highest Die Temp: %d C; DRAM Sensor Status: %d (0 = 1x refresh, 1 = 2x refresh, 2 = Shutdown)"
2670481094,0,ERROR,write_count_histogram.c,"Write Count Status results have some overflowed steps"
2670277765,0,ERROR,sxp_rmt_tests.c,"RAS Rx Vref Max Mask Test Failed"
2670046776,0,DEBUG,pmic.c,"PMIC Clear Bits Error"
2669967996,1,ERROR,read_write_pmic.c,"During processing I2C request EM_STATUS: 0x%08x"
2669961784,4,DEBUG,ahb_unified_engine.c,"Doing PDA Write. PDA: 0x%x_%x DPA: 0x%x_%x"
2669294779,1,ERROR,core_dump.c,"RefreshState - Failed Die               : 0x%02x"
2668266417,0,ERROR,ait_read_line.c,"DMA read failed after attempt on ait backup line."
2668123314,3,DEBUG,task_command_handler.c,"checking sequence: mb[%d] sequence[0x%x] command[0x%x]"
2668054247,1,DEBUG,task_error_handler.c,"AIT Scrub State Machine : %d"
2667898328,1,ERROR,sxp_scheduler.c,"Failed to read SXP_MSR1 register rank: %d during media reset pin firewalling"
2667490334,1,STATUS,command_fw_update.c,"Tried to stage a new FW image 0x%08x seconds too early."
2664796520,2,WARNING,error_logging.c,"Size passed (0x%x) is bigger than available buffer size (0x%x)"
2664049597,0,ERROR,security_md.c,"Wrap the AES part of PM-RK error"
2663890338,0,DEBUG,aes_bulk_encryption_selftest.c,"Read the encypted 256 Byte AES Bulk encryption test buffer from SXP executed"
2663518948,1,ERROR,log_emask_imask_regs.c,"PC_EMASK: 0x%x"
2659771025,1,ERROR,core_wear_level_move.c,"WLM BM aborted entered without BM abort status:%x"
2659698294,0,ERROR,energy_meter.c,"Energy meter failed to reset"
2659393801,0,STATUS,feature_state_data.c,"FSD loaded but init was not saved in CB"
265899838,2,ERROR,sxp_wr_dqs_training.c,"Basic_TxDqDqs failed rank[%d] byte[%d]"
2658564720,0,ERROR,sxp_training.c,"SPI read failure during reboot count fetch!"
2656375902,5,ERROR,core_dump.c,"MbType: %d, CommandReg: 0x%08x_%08x, StatusReg: 0x%08x, Abort: 0x%08x"
2655469161,0,ERROR,sxp_commands.c,"Test Mode Reg Read Latency WA for S26 media failed."
2655466097,2,INFO,task_command_handler.c,"Duplicate Cmd Detected: 0x%x -> Completing with Status [0x%x]"
2655153664,0,ERROR,thermal_manager.c,"Powering off DIMM: Critical Temperature"
2654303727,4,ERROR,task_media_interface.c,"Unknown handle. 0x%08X. Free(%d) WIP(%d) Pending(%d)."
2654290552,2,ERROR,power_budgeting_engine.c,"1.2V Power sample [%d mW] has exceeded high watermark threshold [%d mW]"
2654081617,7,ERROR,dma_polled.c,"Uncorrectable Error! DPA 0x%08X_0x%08X PDA 0x%08X_0x%08X FaultData 0x%08X_0x%08X_0x%08X"
2650315745,3,INFO,dpa_for_pda.c,"0x%08X: AIT lookup for block 0x%08X failed with status 0x%08X"
2649781110,8,ERROR,kechika_river_pmic_driver.c,"Current Rail Values: A[%x] B[%x] C[%x] D[%x] E[%x] F[%x] G[%x] H[%x]"
2649586877,1,DEBUG,platform_config_data.c,"PCD Part: 0x%08X"
2649076971,0,WARNING,command_features.c,"No Address Range Scrub in Progress and no enable sent"
2648715850,1,DEBUG,ddrt_scheduler.c,"DDRT Pll Bus Ratio is: 0x%08x"
2648702878,0,ERROR,fw_activate.c,"PMIC capacitor self-test in progress, Fw Activate is currently unavailable."
2645169670,0,INFO,power_state.c,"Removing Listener."
2644496703,0,DEBUG,task_security.c,"SECURITY_GENERATE_RANDOM_256BIT_VALUE"
2644218346,0,ERROR,training_rmt_tests.c,"Invalid schmoo type parameter."
2643977746,1,ERROR,core_dump.c,"RefreshState - Failed Die               : 0x%02x"
2642874199,1,ERROR,log_emask_imask_regs.c,"PW_EMASK_1: 0x%x"
264278001,1,INFO,power_state.c,"Signal Power Event: %d"
2642075845,2,ERROR,dynamic_vdm.c,"Dynamic_VDM Trim Error rank : %d, die : %d"
2641199062,3,ERROR,algo_write_leveling.c,"DRAM Internal Coarse WrLvl failed. Rank[%d] BytePassMask[%x] BytePassFlag[%x]"
2638510999,0,ERROR,command_software_triggers.c,"Fatal error software trigger is disabled"
2638274160,0,ERROR,sxp_training.c,"SPI read failure during restoring SXP IO registers!"
263804067,0,ERROR,power_loss_log.c,"Error translating PLI log buffer B's dpa address to pda"
2637224379,0,DEBUG,command_features.c,"SS: Security Secure Erase Policy"
2634425163,1,ERROR,command_fw_update.c,"SPI write no erase failed on chunk %d."
2628504643,2,DEBUG,wear_level_move.c,"Invalid Block: 0x%08X_0x%08X"
262833908,0,ERROR,log_power_event_start.c,"LogPowerEventStart"
262812400,0,ERROR,fw_image_sync.c,"SPI copy slot header read error!"
2627847185,2,ERROR,fw_image_sync.c,"The non-loaded slot at address 0x%X failed authentication %d times"
2625409381,0,ERROR,sxp_device_access.c,"Fconfig Partial Read Mode value is invalid. Forcing 11 Device Mode."
2624974444,0,WARNING,command_features.c,"Training already has been completed"
2622387671,0,DEBUG,command_features.c,"Set Admin Features: FW Load Flag"
2620182267,0,WARNING,security_interface.c,"REBUILD_MD security request timed out"
2619514999,0,ERROR,sxp_init.c,"Restoring SxpIo register values from SPI failed"
2616810784,0,INFO,command_log.c,"DMA Transfer Complete"
2614393591,4,ERROR,dma_polled.c,"Address Verify Error! DPA 0x%08X_%08X; PDA 0x%08X_%08X"
2614019976,0,ERROR,fw_image_sync.c,"SPI main slot header read error!"
2613763212,1,ERROR,barlow_creek_pmic_init_reason.c,"Failed to retrieve Fault Code %d."
2613046863,0,ERROR,log_ddrt_io_init.c,"DDRT IO Initialization started!"
2612831449,3,ERROR,datastore.c,"Datastore signatures didn't match. Dest Id: %x Top: %x Bottom: %x"
2610775996,1,ERROR,core_dump.c,"FwDebugData - version       : %d"
2610652213,0,ERROR,security_interface.c,"Security interface queue enqueue request failed"
2603323471,2,INFO,commands.c,"Cmd Format Device, Capacity: %d in %d-byte chunks."
260234550,2,ERROR,spi_manifest.c,"Spi read failed when reading SXP timing table %d version at offset x%08x"
260218279,0,INFO,ddrt_restore.c,"Ddrt_Restore -> No timer needed"
2601178341,1,INFO,checkpoint.c,"Media Status UMR: sBootMediaStatus = 0x%08x"
2599377557,1,ERROR,ltec.c,"ERROR: LTEC rail %d is not at BOOT VID and an update failed. Initiating shutdown."
2599026503,1,ERROR,log_emask_imask_regs.c,"CHN_IMASK_1: 0x%x"
2598377819,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr6: 0x%x"
2596692076,0,ERROR,key_management.c,"Failed to wrap PM-RK with KEK"
2596514986,1,ERROR,core.c,"Core Message queued when queue was full with Message = 0x%X."
2595882599,0,ERROR,log_ait_move_start.c,"AIT NM2 table move started!"
2593718478,0,ERROR,format_device.c,"Cmd Format Device, failed to erase SPI debug region."
2591538443,0,ERROR,spi.c,"Read of remainder bytes failed"
2591022546,0,ERROR,energy_meter.c,"Previously accumulated data hasn't been processed yet."
2589460058,3,ERROR,fw_image_sync.c,"Failed image sync abort: AbortedImgChunk(%d), Total garbage blocks to feed (%d), Failed at garbage block (%d), "
2586579335,1,DEBUG,ait_dram.c,"AIT DRAM Controller Error detected: 0x%08X"
2581922869,0,DEBUG,adma.c,"DN_LOG_RDATA_POISON_1 Error scrub. Scrub command will be sent again."
2581756117,0,ERROR,kechika_river_pmic_driver.c,"Failed to restore power on reset value"
2581651908,1,ERROR,media_management.c,"Media Management Message queued when queue was full with Message = 0x%X."
2580204188,4,ERROR,block_move_error_handler.c,"HW WLM Block Move timeout, cleared locks: src: 0x%08X%08X, dest: 0x%08X%08X"
2579928427,0,DEBUG,hal_pmic_cap_test.c,"Cap test Timer Callback"
2578899750,0,ERROR,power.c,"PLI is detected."
2577931829,0,ERROR,ddrt_training.c,"Ddrt_CoarseRcvenTraining failed"
2577301609,0,WARNING,task_security.c,"WARNING: Request not recognized in task_security"
2577226404,0,ERROR,ltec.c,"PMIC driver failed to apply LTEC update. Retrying."
2576660468,1,ERROR,wear_level_move.c,"FreeBlockExpansion_Dispatch unexpected relocate block msg:%x"
2575482784,1,ERROR,write_count_histogram.c,"Step size is invalid (%d)"
257536110,1,ERROR,sxp_trim_bundle.c,"Could not populate AdReset pulse width value 0x%02x for write."
2573298940,0,INFO,command_inject_error.c,"Dma transfer successful!"
2572491323,0,ERROR,ait_read_line.c,"AitReadLineRead SRAM buffer is too small!"
2572175235,0,ERROR,s3.c,"Failed to handle S3 Entry Request: Bus error"
2572079005,3,ERROR,data_path_error.c,"This error domain %d ferr_%d bit %d causes transaction fatal!"
257082703,3,ERROR,algo_write_leveling.c,"DRAM External Fine WrLvl failed. Rank[%d] BytePassMask[%x] BytePassFlag[%x]"
2569627543,1,WARNING,spi.c,"Write Invalid Size %d"
256800999,5,ERROR,main.c,"MPU exception: Instruction Pointer(eip) = 0x%x, Stack Pointer(esp) = 0x%x, Fault Permission = 0x%x, Fault Address = 0x%x, eflags = 0x%x"
2567963876,1,ERROR,fw_image_sync.c,"Got an unexpected authentication result. 0x%X."
256719240,1,ERROR,host_throttle.c,"HostThrottle_IncreaseThrottleLevelState called, current state %d"
2567071359,0,ERROR,pcr_permissions.c,"Either SXP clock frequency is not configured as 667MHz or d_ddrt_cfg4 is not set to 0x161 or 0x16c."
2565987659,0,ERROR,command_software_triggers.c,"Disabled package sparing software trigger"
2565904409,1,ERROR,fw_image_sync.c,"Image Sync completed with a null buffer in state: %d."
2564610271,0,ERROR,afwe.c,"Hal_Afwe_StartEngine has been called and there is no interrupt handler!"
256349148,3,ERROR,address_verify_error.c,"AddrVerifySetFWP: 0x%08x 0x%08x_%08x"
2560596784,2,INFO,ddrt_scheduler.c,"Ddrt Mmrc Table Checksum MATCHED: c[0x%08x] == t[0x%08x]"
2560111360,0,ERROR,task_error_handler.c,"AIT Scrub flow aborted due to HW WLM pause timeout"
255749724,0,STATUS,command_software_triggers.c,"Fatal error software trigger is disabled"
2557382632,3,ERROR,security_error.c,"Security Key Error Log: Valid bit not set! base = 0x%x, lo = 0x%x, hi = 0x%x"
2556886605,1,ERROR,command_inject_error.c,"Injected a media temperature of %d C"
2556878404,0,WARNING,command_features.c,"Partition in Locked Security State"
255351671,3,DEBUG,core_dump.c,"Found address: 0x%X in range (0x%X, 0x%X)"
2551993264,1,ERROR,get_ait_info.c,"A_AIT_TOP_BASE_ADDR_H: 0x%x"
2551972544,2,ERROR,thermal_engine.c,"Rank read of SXP_SR1 failed on rank:%d fail die map:0x%04x"
2551486136,0,ERROR,kechika_river_pmic_driver.c,"Null pointer in KechikaRiverPMIC_GetInitialDynamicRailSettings"
2551467067,4,INFO,address_scrub.c,"Start ARS: Start Address: 0x%08X_%08X End Address: 0x%08X_%08X"
2550654794,1,ERROR,log_power_event_start.c,"D_PWM_MASK: 0x%x"
2549505146,0,ERROR,thermal_manager.c,"Exiting thermal throttling"
2543926094,7,ERROR,data_path_error.c,"Media error log created for the FERR at domain %d ferr %d bit %d, Error Type %d, Transaction Type %d, PDA 0x%08X_%08X"
2543901588,3,ERROR,core_dump.c,"LatchedShutdownStatus - Latch: 0x%02x | Latch Dirty Shutdown Count: 0x%08x | Power State Events (raw): 0x%08x"
254328689,1,ERROR,security_md.c,"Security md checksum failed on copy: %d"
2542627828,1,ERROR,nlog_region_lock.c,"D_PM_BASE_ADDR_H: 0x%08x"
2541988922,0,ERROR,algo_tx_dq_dqs_training.c,"Mrw DRAM command failed when trying to set ODT latency."
254153439,1,DEBUG,task_command_handler.c,"Setting opcode as: 0x%08X"
2535130395,0,INFO,security_interface.c,"Security_GetSecurityRequest: No work waiting in RequestQueue"
2534215558,0,ERROR,kernel.c,"PLI status bit seen! Forcing a PLI!"
2533158146,0,ERROR,i2c_bus_manager.c,"I2C bus is in error state and is unavailable. Going transaction fatal."
2531099018,0,INFO,ddrt_restore.c,"DdrtRestore_TrainDdrtPostPllLocked called!"
2530988817,1,ERROR,kernel.c,"CFI Exception occured at address: 0x%08X"
2530440375,1,ERROR,nlog_chn_fwrwcmd.c,"CHN_FWRWCMD0: 0x%x"
2530119486,0,ERROR,update_firmware.c,"Tried to do a production FW update while running debug image"
2528702416,0,ERROR,task_media_interface.c,"got DMA completion while engine was hung!"
2528698406,0,INFO,wear_level_move.c,"Block Move: Cannot move CB or SMD or FSD"
2525065766,0,INFO,task_command_handler.c,"Part is LOCKED, completing dfx command as unsupported"
2522374217,0,ERROR,spi.c,"Erase Range: Not Sector Boundary"
2522013733,0,DEBUG,command_features.c,"SS: Set Passphrase"
2521498347,1,ERROR,power_state.c,"Surprise Reset: Unexpected Power State event [0x%x] detected."
2519654807,0,ERROR,ait_update.c,"AIT Dispatch Failure."
2516246839,2,ERROR,adaptive_vdm.c,"Adaptive VDM select ID or media register write command failed on rank : %d, die : %d"
2515490932,2,ERROR,sxp_init.c,"Read DQ-DQS Training failed, Rank: %d Training type: %d"
2514708120,0,INFO,security_interface.c,"Security_CompleteRequestWithResponse completed...Response queued...Event generated"
2513088202,0,DEBUG,command_features.c,"Get Admin Features: Viral Policy"
251231984,0,WARNING,command_features.c,"Only 2LM enabled SKU"
2509833386,0,ERROR,fw_state.c,"FwState_Save Failure - Retrying FwState_Save"
2509186628,0,INFO,power_budgeting_engine.c,"Energy Meter has missed samples, initiating safe mode"
2507985649,0,ERROR,nlog.c,"Error detected with managing nlog SRAM pointers"
2507824617,1,ERROR,log_power_event_start.c,"MSC_PLL_CTRL: 0x%x"
2507166838,1,ERROR,pli_host_throttling_check.c,"DRDP_WCRD_THRES: 0x%x"
2505550186,0,ERROR,sxp_init.c,"Reading Training RMT Report from SPI failed"
2505366540,1,ERROR,log_power_event_start.c,"RPQ_WDB_STAT_EMPTY: 0x%x"
2503466912,1,ERROR,nlog_region_lock.c,"D_TWO_LM_SIZE_L: 0x%08x"
2497696699,1,ERROR,task_media_interface.c,"AitWrite. Invalid level provided. 0x%X."
2494093452,0,WARNING,command_features.c,"Disabling Address Range Scrub"
2492676288,2,ERROR,sxp_trim_bundle.c,"irefSenseEnb could not be reduced by 2, setting to 0. rank = %d die = %d"
2491937747,2,STATUS,fw_init_profiler.c,"Image Sync completed @ 0x%08X after %d us."
249110945,0,INFO,dram_patrol_scrub.c,"DRAM patrol scrub started"
2490311111,1,ERROR,sxp_device_access.c,"Could not properly set the SXP Device Select IDs for rank[%d]"
2484371829,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD0: 0x%x"
2483996728,0,ERROR,task_media_interface.c,"DMA command failed with SRAM parity error twice in a row!"
2483094295,2,ERROR,message_channel.c,"Window Access WRITE Fail  Address = 0x%X, WriteData = 0x%X"
2481019183,1,ERROR,log_power_event_start.c,"PowerStateEvents: 0x%x"
2479954801,1,ERROR,drng_polled_fw.c,"DRNG Fatal error, cannot get random number (code %d)"
2479316202,0,ERROR,fw_image_sync.c,"Image Sync got 2 separate buffer callbacks. Releasing the new buffer."
2476415261,2,ERROR,fw_image_sync.c,"Image_Sync_Completed called in state (%d) with an unexpected status: %d"
2475421980,0,DEBUG,aes_bulk_encryption_selftest.c,"Read the encypted 256 Byte AES Bulk encryption test buffer from SXP executed"
2473719663,2,DEBUG,platform_config_data.c,"Aligned Address: 0x%08X_%08X"
247144820,4,ERROR,message_channel.c,"Message channel error! acc_info = 0x%08X, ctrl = 0x%08X, status = 0x%08X, ddrt_ckdet = %d"
2470458372,4,INFO,sxp_training.c,"SXP MRC Revision %d Build Date: %d/%d/%d"
2470031543,0,ERROR,command_features.c,"Setting FW Load Flag failed"
2469317129,1,ERROR,log_power_event_start.c,"P_PWM_STS: 0x%x"
2469078549,3,STATUS,spi_flash_driver.c,"Flash operation took longer than initial timeout. op: %d, current_time: %d, target: 0x%08X"
2468650432,2,ERROR,thermal_engine.c,"ThermalEngine_LoadSxpTemperatureCalibrationValues failed to Read SxpRegister Die: %d Rank: %d"
246863317,1,DEBUG,memory_info.c,"DFX Memory Info Page Requested - Denied [%x]"
246802649,0,ERROR,ait_dram.c,"DRAM loading completes!"
2467500163,2,ERROR,write_count_histogram.c,"Max write count (%d) < min write count (%d)"
2467104657,1,ERROR,vdm.c,"No Vdm Retry Path values to program for DeviceId = 0x%X."
246680694,1,ERROR,hal_pmic_vendor.c,"UNKNOWN IDT PMIC Stepping - Product Stepping: [0x%X]"
2466563310,0,ERROR,ait_dram_scheduler.c,"AIT DRAM refresh rate changed from 2x to 1x"
2463394810,1,ERROR,command_features.c,"NOT Going to Normal Mode - Host Side Training Incomplete: hostTraininingStatus=%d"
2461490101,0,ERROR,power_budgeting_engine.c,"Energy Meter is aborted."
2461290172,0,WARNING,command_features.c,"Only PM enabled SKU"
2461160177,1,ERROR,sxp_init.c,"No SelectId Table defined for Fab Module 0x%08x, using CPS SelectIds"
245877745,1,ERROR,core.c,"MessageHandler was previously set for this message id: 0x%X."
2458070189,0,ERROR,enqueue_media_request.c,"Media request cannot be enqueued as its queue is full."
2456766740,0,ERROR,dma_polled.c,"DMA Polled complete with SRAM error twice in a row!"
2455293551,3,ERROR,algo_write_leveling.c,"SXP Coarse WrLvl failed rank[%d] bytePassMask[%x] bytePassFlag[%x]"
2455223209,0,DEBUG,task_command_handler.c,"Completing commands that had to do long operations like DMA's"
2454668955,0,WARNING,command_features.c,"SS: Invalid SubOpcode"
2454234213,0,ERROR,log_prefetch_cache_invalidate.c,"PCHE_INV_ALLSETS bit in D_DDRT_TRAINING_OTHER_EN register was set!"
2451796620,2,ERROR,kernel.c,"Unsettable: %d | Event %x"
2451366652,0,ERROR,dma_polled.c,"RACQ Parity error in dma polled"
2451126364,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz0: 0x%x"
2449815377,0,ERROR,fw_init.c,"Adaptive VDM feature has been disabled!"
2449146668,0,WARNING,task_media_interface.c,"DMA abort failed!"
2448325699,0,DEBUG,wear_level_move.c,"WLM state machine calling complete!"
2447414227,0,ERROR,power_budgeting_engine.c,"Energy meter unresponsive (missed 3 accumulation windows), disabling closed loop power throttling."
2446437375,0,ERROR,ddrt_training.c,"Ddrt_FineRcvenTraining failed"
2445230980,1,ERROR,log_power_event_start.c,"D_PWM_STS: 0x%x"
2442941589,0,ERROR,security_interface.c,"Couldn't queue Clear S3 Key security request"
2442064479,2,ERROR,sxp_trims.c,"Unrecognized S26 media on Rank: %d, Die: %d"
2440571439,2,ERROR,sxp_training.c,"Sxp Mmrc Table Checksum did NOT match: c[0x%08x] != t[0x%08x]"
2439912076,1,ERROR,nlog_region_lock.c,"D_TWO_LM_SIZE_L: 0x%08x"
2439223954,3,DEBUG,crypto_selftests.c,"Write source data to SXP addr_hi=0x%x addr_lo=0x%x size=%d bytes."
2439065885,18,ERROR,kechika_river_pmic_driver.c,"Requested Update Values: A[%d][%d][%x] B[%d][%x] C[%d][%x] D[%d][%d][%x] E[%d][%x] F[%d][%x] G[%d][%x] H[%d][%x]"
2438709262,0,ERROR,sxp_commands.c,"Test Mode Reg Read Latency WA for S26 media failed."
2438201756,1,ERROR,ait_dram.c,"Abort DRAM Load at Index %x"
2437736477,2,WARNING,set_fconfig.c,"DFX Set Fconfig checksum failure InputPayload Checksum: 0x%X, Calculated: 0x%X"
2437713328,3,WARNING,ras.c,"0x%08X: no fault data for type 0x%02X (pw_ras_interrupt_req was 0x%08X)"
2435512646,0,ERROR,key_management.c,"Failed to wrap PM-RK with KEK"
2434757604,0,WARNING,dfx.c,"Module ID or Module Size do NOT match with previous chunk"
2434440033,0,ERROR,data_path_error.c,"2 WECC's detected within WECC_WINDOW"
2434248290,0,ERROR,pre_injection_module_framework.c,"Injection module header verification failed!"
2433066501,0,ERROR,ltec.c,"LTEC received DDRT training VID update request while another is pending."
2432065136,1,ERROR,core_dump.c,"OtherStateInfo - Media Disabled State: 0x%x"
2431652846,2,ERROR,sxp_trim_bundle.c,"Could not populate VDM3 vdm=%d to S2X_REG_ADDR_TMR_VDM_3_DAC (0x%04x)"
2429320381,1,DEBUG,host_interrupt.c,"Event[%d] DT is Ready, clearing block"
2424696439,0,ERROR,key_management.c,"Power up type is S3 RESUME! Do not re-generate keys!"
2421860442,9,ERROR,media_manager_engine.c,"BlockMoveIndex %d Src.DPA 0x%08X_0x%08X Src.PDA 0x%08X_0x%08X Src.RO %d Dest.PDA 0x%08X_0x%08X Dest.RO %d"
2419689,0,ERROR,wear_level_move.c,"AIT Read Callback DMA Failure"
241862456,0,INFO,fw_init.c,"Loaded Fw State, now dirtying saved state"
2416054879,1,ERROR,read_write_pmic.c,"During processing I2C request EM_CTRL: 0x%08x"
2413287329,0,ERROR,sxp_rmt_tests.c,"RAS Rx Vref Min Mask Test Failed"
2413274068,1,DEBUG,core_wear_level_move.c,"WLM transition State Machine : %d"
2413115812,0,DEBUG,command_features.c,"Get Admin Features: FW Load Flag"
2412701245,0,DEBUG,task_command_handler.c,"Task_CommandHandler: Background Operation Running"
241152757,1,ERROR,log_vsm_state.c,"Dynamic VDM Stop Media Access state: failure, value: 0x%x"
241021546,3,WARNING,task_error_handler.c,"Error found for domain %u nerr_%u bit %u, no handling other than clearing the bit"
2406328778,1,ERROR,power_budgeting_engine.c,"Fail to disable EM. EmResetStatus = 0x%x"
2405213283,0,ERROR,sxp_scheduler.c,"Failed to read/populate stepping/MPPR/lot IDs"
2403892758,0,DEBUG,command_features.c,"Get Admin Features: Config Lockdown"
2403840083,1,ERROR,log_power_event_start.c,"D_RST_STS: 0x%x"
2402965577,1,INFO,ddrt_scheduler.c,"DDRT locked at %d us"
2400961823,2,ERROR,core_wear_level_move.c,"AitPolled_Write Failed on Entry Address 0x%08X_0x%08X: "
2400070016,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr0: 0x%x"
2399759312,0,ERROR,refresh.c,"Package Migration Started"
2399443702,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr3: 0x%x"
2398801995,0,ERROR,season_device.c,"Seasoning finished"
2397885532,0,WARNING,fw_image_sync.c,"Hash of body of first block failed"
2396642248,0,ERROR,data_path_error.c,"Unknown CSR access error! This shouldn't happen!"
2394013453,0,DEBUG,task_security.c,"SECURITY_CLEAR_S3_KEY"
2393655666,2,ERROR,wear_level_move.c,"FreeBlockExpansion_Transition Could not refresh all source lines of pda 0x%08X_%08X"
239338136,4,ERROR,fw_init.c,"Current FW version is %d.%d.%d.%04x"
2392881950,0,ERROR,fw_activate.c,"Unexpected FW activate runtime data size loaded from media"
2391895378,2,ERROR,kechika_river_pmic_driver.c,"PMIC Manufacture ID: 0x%X    Product Stepping: 0x%X"
2391253753,0,WARNING,command_features.c,"Nonce is all zeroes!"
239016548,3,WARNING,core_wear_level_move.c,"BB pointer not in valid range. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
2388868857,0,ERROR,block_move_error_handler.c,"Hardware wear level move: Block Move Timeout!"
2388421133,0,ERROR,sxp_trims.c,"MA17 cannot be toggle bit for PCL reg access"
2388394796,1,ERROR,log_emask_imask_regs.c,"A_EMASK_2: 0x%x"
238777923,0,DEBUG,command_features.c,"Get Features: Power Management Policy"
2383505655,0,INFO,write_count_histogram.c,"Stop address > DIMM capacity"
2382536689,4,ERROR,task_media_interface.c,"MI 0x%X request made when no free requests were available. Free(%d) WIP(%d) Pending(%d)."
2382451572,3,ERROR,core_dump.c,"InputPayload QWORD[%d]: 0x%08x_%08x"
2382368844,1,ERROR,log_power_event_start.c,"CHN_WCTL: 0x%x"
2382263197,2,DEBUG,nlog.c,"rd 0x%08X = 0x%08X"
2379100043,1,WARNING,core_media_manager.c,"Requested to begin invalid operation %d."
2378956406,0,WARNING,task_command_handler.c,"Error: Media Not Ready"
237867050,1,ERROR,security_md.c,"Caller retrieving invalid value. Offset being retrieved: %d"
2374330126,0,ERROR,hw_init.c,"Failed to program safe vid to Rail D. Stop proceeding Rail D Floor Reduction."
2371450671,8,ERROR,host_interrupt.c,"Packet ACK for DDR-T interrupt timed out - eird = 0x%02X|type=%d|D_DDRT_INTR_CTRL=0x%X|D_DDRT_INTR_STS=0x%X|D_DDRT_INTR_NOACK=0x%X|Timeout Reason=%d|Status_Check=%d|Time elapsed since issue=%d|"
2370178784,0,ERROR,core_wear_level_move.c,"Invalid Firmware State Data, Wear Level Resume State Machine could not complete!"
2369453344,0,ERROR,sxp_scheduler.c,"Failed to read/populate stepping/MPPR/lot IDs"
2367564009,0,ERROR,command_effect_log.c,"Invalid access value for command"
2366430341,1,DEBUG,i2c_master_driver.c,"RX FIFO empty. IC_STATUS = 0x%x"
2365523535,0,ERROR,spi_debug.c,"Error information found in spi debug region"
236408150,2,ERROR,sxp_rx_dqs_training.c,"Advanced_Sxp_RxDqDqs failed margin check rank[%d] byte[%d]"
2362972227,1,DEBUG,wear_level_move.c,"Bad Block Check transition State Machine : %d"
2361552647,0,ERROR,ltec.c,"LTEC failed to set PMIC VCCDDRD_SXP (A) and VCCDDRD_DDRT (D) rails to DDRT training voltages."
236136920,2,ERROR,sxp_trim_bundle.c,"Could not determine TcResetCurrentStep%d from 0x%04x"
2360701093,2,ERROR,wear_level_move.c,"AitPolled_Write Failed on Entry Address 0x%08X_0x%08X: "
2357339091,0,ERROR,spi.c,"Read of bulk data failed"
2356600260,0,DEBUG,crypto_selftests.c,"Read the encrypted Test Buffer from SXP."
2356389695,0,ERROR,feature_state_data.c,"Feature state data flushing failed."
2354637386,0,DEBUG,command_inject_error.c,"Poison: DPA is undergoing relocation!"
2352717595,1,ERROR,log_emask_imask_regs.c,"DA_IMASK: 0x%x"
2352394907,0,ERROR,command_inject_error.c,"Enabling poison on 4 cache lines"
2351368301,1,DEBUG,i2c_master_driver.c,"MST_ACTIVITY times out. IC_STATUS = 0x%x"
2350697267,3,ERROR,update_firmware.c,"DMA read of block %d of image failed. State: %d. Substate: %d"
2349074948,1,ERROR,nlog_chn_fwrwcmd.c,"CHN_FWRWCMD1: 0x%x"
2348220366,0,ERROR,write_count_histogram.c,"WriteCountHistogram: Buffer address is 0x0"
2348180516,0,ERROR,spi_logger.c,"SPI Read Failed, can't log data from spi debug region."
234655064,2,ERROR,dynamic_vdm.c,"Dynamic_IRST Trim Error rank : %d, die : %d"
234501288,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustLegacyVdm at Window. Window : %d"
2344653911,0,WARNING,fw_image_sync.c,"Non loaded slot signature invalid"
2343360015,3,ERROR,hal_pmic_rail.c,"PMIC Rail 0x%x did not ramp to target value 0x%x. Current value is 0x%x."
2341738957,2,ERROR,core_dump.c,"RefreshState - Sleep Time Stamp         : 0x%08x_%08x"
2340713768,0,STATUS,warm_reset.c,"Warm Reset Start"
2340088267,0,ERROR,power_wake_isr.c,"Surprise clockstop received"
2340040902,1,ERROR,sxp_init.c,"No SelectId Table defined for Fab Module 0x%08x, using BPS SelectIds"
233984830,0,ERROR,sxp_init.c,"ZQCalLongInit failed"
2337217251,0,DEBUG,command_features.c,"SS: Set Master Passphrase"
2336642155,0,DEBUG,task_security.c,"SECURITY_OVERWRITE_DIMM"
2336036864,0,WARNING,health_manager.c," Life Span Percentage Remaining <= 1%"
2335140362,4,ERROR,ltec.c,"Error detected in LTEC Voltage Calculation, programming boot voltage. BootVid: %d, slope: %d, temperature: %d, newVid: %d"
2334937065,1,ERROR,sxp_scheduler.c,"Invalid rank count %d. Not assigning the internal address offsets."
2333427092,0,ERROR,ltec.c,"LTEC unable to initialize due to PMIC initialization failure"
2332327373,0,ERROR,fw_init.c,"Crypto self-test failed!\n"
2331237104,0,ERROR,task_error_handler.c,"Completing AIT Scrub"
2327528507,0,ERROR,ait_dram.c,"DRAM load NOT started due to dram device failed!"
2327242387,0,STATUS,thermal_manager.c,"Temperature polling disabled"
2327186372,0,WARNING,sxp_commands.c,"Sxp ReadReg REQ bit still set after delay!"
2326706009,0,ERROR,key_management.c,"Power up type is S3 RESUME! Do not re-generate keys!"
2325885097,1,ERROR,log_power_event_start.c,"PowerEvent: 0x%x"
2323151395,0,DEBUG,command_features.c,"Get Features: Package Sparing Policy"
2322513712,1,ERROR,read_write_pmic.c,"During processing I2C request PCSCLR_PWR_CFG7: 0x%08x"
2319151950,2,ERROR,sxp_trims.c,"0x105 register read failed. Can't check media type on Rank: %d, Die: %d"
2319149480,2,ERROR,algo_tx_dq_dqs_training.c,"DRAM Basic TxDqDqs: Coarse step failed rank[%d] byte[%d]"
2318923292,2,ERROR,sxp_init.c,"Read DQ-DQS Training failed, Rank: %d Training type: %d"
2318542930,1,INFO,kechika_river_pmic_driver.c,"PMIC Detected PRODUCT: 0x%x\n"
2315500413,1,ERROR,core_dump.c,"OtherStateInfo - IsShutdownTimeSet   : 0x%02x"
2314844956,0,ERROR,kechika_river_pmic_driver.c,"Erroneous Cap test tick value"
231272562,2,ERROR,algo_tx_dq_dqs_training.c,"Basic_TxDqDqs failed rank[%d] byte[%d]"
2312644515,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz1: 0x%x"
2312209665,0,INFO,fw_image_sync.c,"Initialize the image sync"
2312099829,0,ERROR,task_media_interface.c,"Attempted to complete a DMA when there is no active DMA."
2311293868,0,INFO,wear_level_move.c,"FBE: AIT line of address contains SMD or CB or FSD"
2308324268,4,INFO,ras.c,"0x%08X: fault data: info0 0x%08X, info1 0x%08X, info2 0x%08X"
2308125994,2,ERROR,algo_tx_dq_dqs_training.c,"DRAM Basic TxDqDqs: Fine step failed rank[%d] byte[%d]"
2304863383,1,WARNING,fconfig.c,"Fconfig_SetConfig token cannot be changed Token: 0x%X"
2304846850,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustVdm at Window. Window : %d"
2303929844,0,ERROR,fast_zero.c,"FZ: key change, out of versions!"
230269690,1,ERROR,core_dump.c,"RefreshState - Current Refresh Pointer  : 0x%08x"
2302657584,0,ERROR,ltec.c,"PMIC rails are at Boot VIDs at the time of LTEC failure."
2298229107,1,WARNING,host_interrupt.c,"packet ack for DDR-T interrupt 0x%02X timed out; consider increasing D_DDRT_INTR_TIMER val"
2297992034,1,ERROR,log_emask_imask_regs.c,"CHN_IMASK_3: 0x%x"
2295413464,1,ERROR,sxp_trims.c,"Invalid toggle mux setting. Register value = 0x%08x"
2293137855,0,INFO,security_interface.c,"Security free pool is unavailable!"
2292397843,0,DEBUG,kechika_river_pmic_driver.c,"Cap test Timer Callback"
2292292537,0,ERROR,ait_read_line.c,"MediaInterface handle returned NULL. AIT Read Failed."
2292009645,0,DEBUG,command_features.c,"SS: Get Security State"
2291679801,4,ERROR,dma_polled.c,"Uncorrectable error! DPA 0x%08X_%08X; PDA 0x%08X_%08X"
2291559308,0,ERROR,power_budgeting_engine.c,"Setting average power budget to pTarget and entering open loop as FW is unable to process EM data in a timely manner for two consecutive accumulation windows"
2291330615,0,ERROR,log_zqcal_short.c,"Flush of Nlog buffer to media has occurred."
2290877143,0,WARNING,command_features.c,"Clear History can only be executed on Bios Mailbox"
2290135611,1,ERROR,sxp_rank_interleave.c,"Rank interleaving boundary (%d) is not supported!"
2290104039,1,WARNING,health_manager.c,"Complete Package Sparing has occurred. Failing Die: %d."
2289765336,0,WARNING,task_security.c,"Unable to set master passphrase: Encryption Disabled"
2288955590,1,ERROR,core_dump.c,"SXP MMRC Version: %d"
2287607577,1,ERROR,ras.c,"fault data is not valid! Log Register 2: 0x%X"
2287310215,0,ERROR,dynamic_vdm.c,"Dynamic VDM cannot apply media policy to this DIMM! TR2 or older media has been detected with EKVB0."
2286291968,0,DEBUG,command_features.c,"Get Admin Features: SKU"
2284797800,0,DEBUG,core_wear_level_move.c,"FBE AIT DMA Line Callback"
2284785311,1,ERROR,reg_protect.c,"Unaligned write request detected (%08X)"
2283460805,1,ERROR,sxp_init.c,"This board 0x%08x does not support 10 Die Mode without rework"
2282335099,0,DEBUG,address_scrub.c,"DN_LOG_RDATA_POISON_1 Error scrub. Scrub command will be sent again."
2280881906,0,DEBUG,refresh.c,"fast refresh already started"
2280261918,3,ERROR,data_path_error.c,"This error domain %d ferr_%d bit %d causes DIMM fatal!"
2276271466,0,STATUS,command_software_triggers.c,"Percentage remaining software trigger is disabled"
2276082007,0,INFO,ddrt_scheduler.c,"DDRT Ungate Pll!"
2273610372,1,ERROR,command_software_triggers.c,"Percentage remaining software trigger is injected with a value of %d"
2273514470,1,ERROR,kechika_river_pmic_driver.c,"Message Handler incorrectly called with message: %x"
2272127064,0,ERROR,pre_injection_module_framework.c,"Injection module header verification failed!"
227062554,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz4: 0x%x"
2270119896,2,DEBUG,platform_config_data.c,"Offset Address: 0x%08X_%08X"
2270014446,0,ERROR,dpa_verify_error_handler.c,"This error happens on AIT line, complete transaction and go DIMM fatal!"
2267272831,1,ERROR,log_vdm_for_wlm.c,"WearLevelMoveState: %d"
2266914445,0,INFO,refresh.c,"Migration Completion Callback"
2265381137,0,DEBUG,command_features.c,"CONFIG_LOCKDOWN Executed"
2263371765,15,ERROR,dma_polled.c,"Uncorrectable error! FaultData Rank: 0x%01X; Stype: 0x%01X; RetryIndex: 0x%01X; Vdm: 0x%01X; FwErrComp: 0x%01X; FwErrAddrComp: 0x%01X; Length: 0x%01X; Rdir: 0x%01X; WdbAddr: 0x%02X; Rid: 0x%02X; Rtype: 0x%02X; WriteCount: 0x%01X; InitialVdm: 0x%01X; AitSecondCopyPoison: 0x%02X; PoisonStatus: 0x%06X;"
2262845773,0,DEBUG,power_budgeting_engine.c,"Do nothing as FW is falsely detecting a miss on the first accumulation window after energy meter starts."
225968567,3,ERROR,sxp_trims.c,"Unsupported S15 media (%d) on Rank: %d, Die: %d. Only Tranche3 is supported."
2256708145,0,ERROR,wear_level_move.c,"FBE AIT Read Callback DMA Failure"
225611778,3,DEBUG,dpa_for_pda.c,"0x%08X: PDA 0x%08X_%08X"
2255722586,2,STATUS,command_features.c,"Performance Knob %d is updated with value %d"
225477769,0,WARNING,security_interface.c,"HMAC security queue request timed out"
2253396090,1,DEBUG,host_interrupt.c,"HostInterrupt PowerStateNotify Event[%d]"
2252793173,0,ERROR,log_power_event_end.c,"LogPowerEventEnd"
2252156943,0,ERROR,vdm.c,"Vdm_AdjustVdm, trying to adjust VDM0 on S15 media!"
2251957069,2,ERROR,sxp_init.c,"Fine RcvEn Training failed, Rank: %d Training type: %d"
2251383623,1,ERROR,nlog_region_lock.c,"D_TWO_LM_SIZE_H: 0x%08x"
2250767993,0,ERROR,crypto_selftests.c,"PKCS #5 v2.0 PBKDF2 [PRF=HMAC-SHA-384] self-test failed!"
2250562545,1,ERROR,sxp_scheduler.c,"Invalid 3DXP Device ID 0x%04x"
2249507087,0,DEBUG,crypto_selftests.c,"Failed to perform key expansion of bulk subkey from XTS-AES-256 key."
224881587,4,WARNING,command_features.c,"Invalid set power management params. Values do not meet minimum, maximum or granularity requirements.AveragePowerLimit = %d; averagePowerTimeConstant = %d; turboModeState = %d; turboPowerLimit = %d"
2247988808,0,ERROR,sku.c,"Security SXP Access disabled, bypassing sku cipher checker"
2247958413,1,ERROR,sxp_init.c,"Sxp_RxDqsTraining failed rank: %d"
224745530,0,ERROR,command_software_triggers.c,"Injected package sparing software trigger error"
2247224034,2,ERROR,core_dump.c,"Context Block Data: Top[0x%x] | Bot[0x%x]"
2245841001,0,ERROR,die_error_emulator.c,"DieErrorEmulator: Spare die is not part of the common id group. DQ failure is not supported on this die."
2245835608,1,ERROR,write_count_histogram.c,"Error: Invalid stats mode: %d"
2244052849,2,ERROR,dynamic_vdm.c,"Dynamic VDM SxpCmd_SelectId failed on rank : %d, die : %d"
224093758,0,DEBUG,refresh.c,"Power Transition: Pausing Refresh/Migration"
2240856116,1,ERROR,partition_error.c,"Partition Error Log: Valid bit not set! DN_LOG_ADDR_REGION_ERR_1_VLD = 0x%x"
2239625716,2,DEBUG,refresh.c,"Resuming Migration at Address 0x%08x for failing Die %d "
2239572929,3,ERROR,datastore.c,"Datastore signatures didn't match. Dest Id: %x Top: %x Bottom: %x"
223825129,0,ERROR,ltec.c,"LTEC requested to enter normal update mode after it has been disabled."
2238198019,0,WARNING,security_interface.c,"REBUILD_MD security request timed out"
2237755889,1,ERROR,fw_init.c,"The DIMM serial number is 0x%08x"
2236843464,3,ERROR,algo_xover_calibration.c,"Xover calibration failed due to invalid edges. Byte[%d], Rising Edge[%d] Falling Edge[%d]"
2236800411,0,ERROR,overwrite_dimm.c,"Overwrite DIMM could not pause HW WLM."
2235579838,0,ERROR,mmrc_parser.c,"MMRC Invalid Table Entry"
2232250086,2,DEBUG,security_interface.c,"Security Free Pool -> QueueCount: %d, QueueEntries: %d"
223091741,1,ERROR,mm_free_block_expansion.c,"Invalid handle after AIT line read for FBLE Cold Block request. Handle 0x%X."
2230735905,2,ERROR,chn_no_cmd.c,"Chn no cmd with WLM for DPA 0x%08x_%08x deallocating WDB entry"
222733273,3,INFO,dpa_for_pda.c,"0x%08X: no DPA found for PDA %08X_%08X"
2225831729,0,DEBUG,task_security.c,"SECURITY_REBUILD_MD"
2223871516,0,INFO,security_interface.c,"Security_GetSecurityResponse: No response present in ResponseQueue"
2222743208,4,WARNING,command_features.c,"Invalid set power management params. Values do not meet minimum, maximum or granularity requirements.AveragePowerLimit == %d; averagePowerTimeConstant == %d; turboModeState=%d; turboPowerLimit=%d"
2222674909,1,ERROR,short_stroke.c,"Short Stroke offset %d is invalid"
222131317,0,ERROR,security_interface.c,"Couldn't queue SHA SDMA security request"
2219770658,1,DEBUG,core_dump.c,"Address provided was not found in searched regions: 0x%X"
2219642862,1,ERROR,ltec.c,"Invalid power transition %d for Ltec_PowerStateListener"
221870817,0,DEBUG,breakpoint.c,"Single Step Breakpoint"
2218464171,1,ERROR,sxp_init.c,"No SelectId Table defined for Fab Module 0x%08x, using BPS SelectIds"
2217675131,0,ERROR,core_dump.c,"Current Mailbox Data:"
2217484547,0,DEBUG,key_management.c,"Unwrapping S3 Saved Volatile Memory Keys"
2215199369,0,ERROR,ait_dram.c,"Abandon DRAM Load"
2214705641,0,WARNING,command_features.c,"Address Range Scrub: Doing a Disable - Skipping Data Validation"
2210987553,0,DEBUG,command_inject_error.c,"Inject poison invalid memory type provided"
2209944971,0,ERROR,format_device.c,"Invalid FW State. Failed to preserve lifetime stats"
2209442447,0,STATUS,command_inject_error.c,"Media temperature error injection is disabled"
2208232489,0,DEBUG,task_command_handler.c,"Task_CommandHandler: Media Disabled DFx Command Not Allowed"
2207869612,0,ERROR,format_device.c,"Cmd Format Device, failed to disable energy meter."
2207625804,1,ERROR,data_path_error.c,"DS FIFO U/O Flow Errors: 0x%08X"
2207304746,2,ERROR,algo_rx_dqs_training.c,"Advanced_Sxp_RxDqDqs failed rank[%d] byte[%d]"
2204502365,4,ERROR,task_error_handler.c,"domain %u ferr_%u bit %u was set, ferr = 0x%x"
2202286455,0,ERROR,adaptive_vdm.c,"AVDM_GetVdmDimmData requested VDM0 with S15 media."
2199087867,0,ERROR,aes_bulk_encryption_selftest.c,"*** FAIL *** decryption test"
2197613360,0,ERROR,throttling_engine.c,"During system throttling state, detected a request to change the power credits by other than thermal manager "
2195641996,2,ERROR,core_dump.c,"LP OutputPayload Addr: 0x%08x_%08x"
2193212686,0,DEBUG,task_security.c,"SECURITY_UNLOCK_UNIT"
2192840538,0,ERROR,s3.c,"Failed to handle S3 Entry Request: PMIC communication error"
2190344708,2,ERROR,power_event_at_image_sync.c,"Stopping image sync at chunk: %d, in state: %d"
2188737318,0,INFO,refresh.c,"Starting Refresh Engine"
2188454589,0,INFO,security_interface.c,"Security State: Frozen"
2186720259,0,INFO,security_interface.c,"security_SubmitWork completed."
2186533679,3,ERROR,io_csr.c,"IO CSR invalid parameter rank = 0x%x, byte = 0x%x, bit = 0x%x"
2186101338,0,ERROR,sxp_training.c,"SPI failed during SXP IO register table read!"
218553257,3,ERROR,algo_xover_calibration.c,"Xover calibration failed due to invalid strobe duty cycle. Byte[%d] Rising Edge[%d] Falling Edge[%d]"
2182849232,1,INFO,ddrt_sense_amp_calibration.c,"DDRT Sense Amp CMD VOC, CTT Termination = %d"
2182106190,0,ERROR,command_features.c,"NOT Going to Normal Mode - Host Side Training Failed!"
2181535126,2,ERROR,dpa_verify_error_handler.c,"DRAM read at DPA LvL N address Lo: %x Hi: %x  failed"
2181320846,0,ERROR,power_budgeting_engine.c,"EM reset operation failed due to I2C operations timing out"
2180912039,0,ERROR,ait_dram.c,"DRAM load NOT started due to media is not trained or disabled!"
2180895697,1,ERROR,log_vsm_state.c,"Dynamic VDM Stop Media Access state: failure, value: 0x%x"
2180416870,1,ERROR,task_media_interface.c,"We received a DMA completion event, but there is a DMA active afwe_status: 0x%X"
2179123768,1,ERROR,nlog_region_lock.c,"D_PM_SIZE_L: 0x%08x"
2179052604,0,WARNING,burn_in.c,"SXP WriteReg REQ bit still set after delay!"
2176234198,0,DEBUG,aes_bulk_encryption_selftest.c,"Enable Decryption Bypass"
2169833224,1,ERROR,sxp_commands.c,"Unexpected FGPK SXP Trim Reg Read Offset value of 0x%X."
2168591127,0,DEBUG,command_inject_error.c,"Inject poison invalid memory type provided"
2168437319,0,INFO,command_log.c,"Get Smart/Health Info"
2168400948,0,ERROR,health_manager.c,"Life Span Percentage Remaining = 0"
2164785610,1,ERROR,kechika_river_pmic_driver.c,"PMIC Error returned while updating rail %d"
2162703686,7,ERROR,cmd_timer_end.c,"CMDCC: %d %02x %02x %08x %u %u %u"
216126719,0,ERROR,hal_pmic_cap_test.c,"Cap self test setup failed."
2161101649,1,INFO,checkpoint.c,"Media Status UMR: sBootMediaStatus = 0x%08x"
2159831511,0,WARNING,sxp_commands.c,"ZQCal Long REQ bit still set after delay!"
215905521,1,ERROR,hal_pmic_init_reason_cwv.c,"Failed to retrieve Fault Code %d."
2158816684,7,ERROR,fw_init.c,"Current FW version is %x.%x.%x.%04x and DIMM Unique ID is %02x%08x%08x"
2156361909,0,INFO,refresh.c,"Getting Refresh Interval"
2154536782,1,ERROR,power_budgeting_engine.c,"Failed to suspend EM. EM reset status = 0x%x"
2154104464,0,INFO,core_dump.c,"Failed to retrieve SPI manifest"
2154057974,1,ERROR,wear_level_move.c,"WearLevelMove_Dispatch unexpected relocate block msg:%x"
2152953340,2,ERROR,algo_receive_enable.c,"Coarse Rcven failed rankIndex[%d] byte[%d]"
2152746524,2,ERROR,adaptive_vdm.c,"Adaptive VDM Trim Error rank : %d, die : %d"
2150636367,0,ERROR,fw_img_auth.c,"Hashing image block failed"
2150453847,3,WARNING,write_disturb_refresh.c,"Write Disturb Refresh failed with %d on PDA 0x%08x_%08x"
2149989553,0,ERROR,fw_init.c,"Injection module from SPI was not loaded"
2149533384,0,ERROR,update_firmware.c,"SPI Read of FW failed after successfully staging FW Image."
2149436859,0,DEBUG,task_security.c,"SECURITY_SET_S3_KEY"
2149284873,3,ERROR,write_disturb_refresh.c,"Aggressor Address: 0x%08X_0x%08X Victim map 0x%08X"
2148520363,0,ERROR,power_event_at_image_sync.c,"Image sync timer was not initialized"
2145847815,1,ERROR,log_emask_imask_regs.c,"CHN_IMASK_3: 0x%x"
2144672413,0,INFO,command_features.c,"The DDRT Alert Policy data is valid!"
2143276133,2,INFO,sxp_training.c,"SXP Timings Rev[%d] Build Date: [%d]"
2142499658,0,ERROR,refresh.c,"Package Migration Completed"
2137920204,7,ERROR,core_dump.c,"FW Version: %x%x.%x%x.%x%x.%d"
2137498055,2,DEBUG,crypto_selftests.c,"Verify 3DXP XTS-AES-256 engine successfully decrypted data from sxp addr_hi=0x%x addr_lo=0x%x "
2136899967,1,ERROR,nlog_config_lockdown.c,"DA_IO_PCR_PERMISSIONS0: 0x%x"
2134832324,0,WARNING,command_features.c,"Address Range Scrub: Doing a Disable - Skipping Data Validation"
2133283278,1,ERROR,assert.c,"ESP +  0: 0x%X [    Instruction Pointer (EIP)   ]"
2132300527,0,DEBUG,command_features.c,"SS: Security Secure Erase"
2131535127,0,ERROR,task_error_handler.c,"spurious error IRQ!"
2130919422,0,WARNING,command_features.c,"Invalid Value for Power Management Policy Enable"
2130143451,0,WARNING,security_interface.c,"EAU security request timed out"
2129246489,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtRxDqSwz3: 0x%x"
2128637730,0,DEBUG,command_features.c,"Get Features: Optional Config"
2127739687,1,WARNING,dfx.c,"ModuleSize was either NOT DMA_DATA_BLOCK_SIZE aligned, less than DMA_DATA_BLOCK_SIZE, or greater than 0x%08X"
2125087261,0,ERROR,ddrt_scheduler.c,"SPI read error during reading DDRT IO MMRC table!"
2124654719,0,ERROR,read_write_pmic.c,"WritePmic Failure"
2124083649,0,ERROR,spi_debug.c,"Failed to write spi debug data"
2123247005,0,ERROR,command_log.c,"DMA Submission entry failed to queue."
2122160095,0,WARNING,command_features.c,"Invalid PCD Payload Type"
212187010,2,ERROR,dynamic_vdm.c,"Dynamic_IRST cannot identify microamp table for rank : %d, die : %d"
2121221729,1,ERROR,die_error_emulator.c,"sxp_reg library returned with status = %d"
2120685649,0,ERROR,sxp_rmt_tests.c,"RAS Tx Dq Max Mask Test Failed"
2118744544,1,ERROR,power_wake_isr.c,"Surprise clockstop received and current PowerStateEvents is 0x%x"
2115981574,1,ERROR,power_budgeting_engine.c,"Invalid time constant %dms requested. Power budgeting engine applies the value but does not store in FW state."
2115819862,3,ERROR,task_error_handler.c,"domain %u nerr_%u = 0x%x"
2115687640,1,ERROR,data_path_error.c,"PC ERR STS FIFO U/O Flow Errors: 0x%08X"
2111996898,6,ERROR,core_dump.c,"2LM Size: 0x%x_%x | PM Size: 0x%x_%x | PM Base Address: 0x%x_%x"
2111440157,0,DEBUG,ait_dram.c,"Unknown AIT DRAM Error -> should never see this"
2107861033,0,DEBUG,task_error_handler.c,"Retrieving settings for Package Sparing"
2106277578,0,WARNING,command_features.c,"Config Lockdown not supported"
2105872321,3,ERROR,sxp_scheduler.c,"read SXP_MSR11 failed! value = 0x%x, die = %d, rank = %d \n"
210575036,1,ERROR,ras.c,"fault data is not valid! PC_LOG_WCTL_NO_CMD_2: 0x%X"
210487343,10,STATUS,kechika_river_pmic_driver.c,"Current Rail Values: A[%d][%x] B[%x] C[%x] D[%d][%x] E[%x] F[%x] G[%x] H[%x]"
21045178,3,ERROR,sxp_trims.c,"Unsupported S15 media (%d) on Rank: %d, Die: %d. Only Tranche3 is supported."
2102819487,1,ERROR,log_emask_imask_regs.c,"DN_FIFO_EMASK: 0x%x"
2101032116,4,WARNING,command_features.c,"Invalid set power management params. Values do not meet minimum, maximum or granularity requirements.AveragePowerLimit = %d; averagePowerTimeConstant = %d; turboModeState = %d; turboPowerLimit = %d"
2099853640,0,ERROR,thermal_manager.c,"Temperature polling disabled"
2099344923,2,ERROR,sxp_rx_dqs_training.c,"Advanced_Sxp_RxDqDqs failed rank[%d] byte[%d]"
2099191036,0,ERROR,get_media_statistics.c,"Unknown stat total requested"
2094530284,0,INFO,wear_level_move.c,"Invalid address value"
2093091517,0,WARNING,task_security.c,"Unable to set passphrase: Encryption Disabled"
20927806,1,ERROR,sxp_init.c,"Sxp_AdvancedTxDqsTraining failed rank: %d"
2092616906,1,ERROR,log_power_event_start.c,"D_FUNC_DEFEATURE1: 0x%x"
2091289613,0,ERROR,log_block_move_ait_update.c,"Block Move Ait Update started."
2085514869,3,DEBUG,task_command_handler.c,"Recd. Mailbox Cmd. 0x%08x:%08x , %x"
208521702,0,ERROR,command_fw_update.c,"Failed to write to SPI."
2084895606,2,ERROR,wear_level_move.c,"AitPolled_WriteReverseMap Failed on Entry Address 0x%08X_0x%08X: "
208445413,0,ERROR,key_management.c,"Failed to generate the key encryption key from passphrase based derived key"
2084321148,1,INFO,fw_image_sync.c,"Image Sync was aborted in state %d. Buffer released."
208410127,1,ERROR,ras.c,"RAS Log: Valid bit not set - DS_LOG_WDATA_POSION_1 = 0x%x"
208266394,0,STATUS,power_state.c,"Warm Reset Start"
2081507906,0,ERROR,host_interrupt.c,"HostInterrupt AbortInFlight - Aborting Pending"
2080203298,0,WARNING,command_features.c,"Alarm Threshold: Invalid Percentage Remaining parameter"
2080042448,1,ERROR,log_power_event_end.c,"D_PWM_STS: 0x%x"
2078250305,2,ERROR,commands.c,"Cmd Format Device, DMA returns a failure status. sxp address:  0x%08X_%08X"
2076758111,1,ERROR,log_emask_imask_regs.c,"DS_EMASK: 0x%x"
2076719397,0,INFO,task_command_handler.c,"Part is UNLOCKED, executing dfx command"
2076658181,2,ERROR,algo_sense_amp_calibration_cmd.c,"No transition found for Sense Amp Calibration Cmd Fub %d, Bit %d"
2075783158,0,INFO,host_interrupt.c,"HostInterrupt Issue Alert"
2074699978,2,ERROR,hal_pmic_cfg.c,"PMIC Returned invalid Product ID. Expected: 0x%X, Received: 0x%X"
2072932024,1,ERROR,security_md.c,"Security md version doesn't match on copy %d"
2071147823,1,ERROR,log_bsr.c,"D_FW_STATUS_H: 0x%x"
207070774,0,ERROR,hal_pmic_init_reason_cwv.c,"Could not unlock the PMIC."
207015018,0,WARNING,command_fw_update.c,"Uploaded binary is not 256B aligned"
2068824868,1,ERROR,spi_manifest.c,"Spi read failed when reading MMRC table version at address x%08x"
2068803885,1,ERROR,training_scheduler_init.c,"Unsupported SXP Device Device ID read error. DeviceId = 0x%X"
2068381955,3,ERROR,ras.c,"RAS PC_WPDA Log: Valid bit not set! base = 0x%x, lo = 0x%x, hi = 0x%x"
2068159740,3,WARNING,wear_level_move.c,"BB pointer not in valid range. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
2067804341,0,DEBUG,aes_bulk_encryption_selftest.c,"Verify AES Bulk Encryption successfully encrypted the first cacheline."
2065933121,1,ERROR,sxp_rank_interleave.c,"Rank interleaving boundary (%d) is not supported!"
2064960991,0,DEBUG,crypto_selftests.c,"Verify 3DXP XTS-AES-256 engine successfully encrypted the plaintext."
2063485635,2,ERROR,core_wear_level_move.c,"AitPolled_WriteReverseMap Failed on Entry Address 0x%08X_0x%08X: "
2062495347,1,ERROR,pli_log_entries.c,"Requested PLI Log page is out of bounds 0x%x"
2061193366,1,ERROR,nlog_config_lockdown.c,"D_FW_STATUS_H: 0x%x"
2061141197,1,ERROR,nlog_config_lockdown.c,"DA_IO_PCR_PERMISSIONS0: 0x%x"
2060861087,0,DEBUG,wear_level_move.c,"Wear Level Move No Spare Blocks!"
205942754,1,ERROR,log_bsr.c,"D_FW_STATUS_H: 0x%x"
2057729684,2,ERROR,power_state.c,"PowerState_SignalPowerEvent: Unexpected Power State event [0x%x] detected in power transition state  [0x%x]."
2057329108,3,DEBUG,core_dump.c,"Found address: 0x%X in range (0x%X, 0x%X)"
2054769229,0,DEBUG,overwrite_dimm.c,"Overwrite DIMM ait write Callback"
2054139193,1,ERROR,sxp_scheduler_init.c,"Sxp_FirewallResetPin failed to read SXP_MSR1 register rank: %d"
2054082459,0,ERROR,kechika_river_pmic_driver.c,"Failed to disable power on reset"
2053519006,0,ERROR,data_path_error.c,"PW ERR STS FIFO U/O Flow Errors: PW_ERR_STS_GL_DAT_BUFF_UNF is detected"
2053412136,1,ERROR,log_ddrt_io_init.c,"MSC_SPARE_CTRL: 0x%x"
2051764504,7,ERROR,core_dump.c,"FW Version: %x%x.%x%x.%x%x.%d"
205020352,0,ERROR,command_software_triggers.c,"Unsafe shutdown software trigger is disabled"
2050058011,1,ERROR,log_power_event_start.c,"MSC_PLL_CTRL: 0x%x"
2047525076,1,ERROR,core_dump.c,"PowerStateEvents Raw: 0x%x"
2047060163,0,ERROR,context_block.c,"Context Block Initialization Failed"
2045499200,0,ERROR,dma_polled.c,"Both AIT UECC, don't complete the transaction!"
204412900,0,ERROR,power.c,"PMIC Rail A got svid fuse value 0x0"
2043736519,0,ERROR,power_event_at_image_auth.c,"POWER_EVENT_AT_IMAGE_AUTH function has been removed"
2043036304,3,ERROR,ait_dram.c,"Platform API set -- DRAM Able to load: %d, Drift tracking ready: %d, load status: %d"
2035300208,0,ERROR,sxp_rank_interleave.c,"Unknown SXP devices, cannot set rank interleaving."
2034758691,0,DEBUG,wear_level_move.c,"AIT Read Callback"
2034403265,0,ERROR,key_management.c,"Failed to generate the passphrase based derived key"
2033988572,0,ERROR,media_manager.c,"Bad Block Check queue is full, dropping request!"
2031720124,0,INFO,wear_level_move.c,"FBE: AIT line of address contains SMD or CB or FSD"
2030724461,0,ERROR,sxp_scheduler_init.c,"Aep Scheduler Init failed"
2030280978,0,DEBUG,pmic.c,"I2C Failed to initialize"
202995933,0,WARNING,command_features.c,"The DDRT Alert Policy data is not valid - low and high priority both set!"
2023736096,1,ERROR,hal_pmic_rail_cwv.c,"Failed to disable power-on reset on Rail 0x%x"
2022851411,0,ERROR,aes_bulk_encryption_selftest.c,"*** FAIL *** encryption test"
2021958178,0,WARNING,command_features.c,"Not BIOS Mailbox"
2020288802,0,DEBUG,command_features.c,"Get Features: PMON Registers"
2019683367,0,ERROR,fw_img_auth.c,"EAU signature padding verification (padding 2) failed"
2017789342,0,WARNING,update_firmware.c,"Tried to do a dfx FW update while DIMM is locked or not whitelisted"
2017743048,1,ERROR,get_spi_manifest.c,"Spi read failed when reading pIMF Header at address 0x%08x"
2016199875,1,ERROR,core_wear_level_move.c,"FreeBlockExpansion_Dispatch unexpected relocate block msg:%x"
201549540,1,STATUS,command_inject_error.c,"Injected a media temperature of %d C"
2014220436,0,ERROR,task_error_handler.c,"Dclk is not enabled when handling DA_NERR"
2013844189,0,WARNING,command_inject_error.c,"Media temperature error is cleared because error injection is disabled"
2012050167,1,ERROR,power_state.c,"PC6: Unexpected Power State event [0x%x] detected."
2008854339,0,ERROR,dynamic_vdm.c,"Dynamic VDM cannot apply media policy to this DIMM! Mixed media with pre and post MPPR 85 detected."
2008682095,1,ERROR,nlog_notify_ddrt_normal_mode.c,"D_FW_STATUS: 0x%x"
2008397970,1,ERROR,fw_activate.c,"DDRT Read Transactions during FW Activate: 0x%08x"
2006562195,1,ERROR,nlog_chn_fwrwcmd.c,"CHN_FWRWCMD2: 0x%x"
2005744398,0,INFO,power_state.c,"Surprise Reset Start"
2004933689,1,INFO,format_device.c,"HW supports up to 0x%x random WC. FW WC Randomization will be used that extended format time should be given."
2004048170,4,ERROR,algo_write_leveling.c,"Fine WrLvl failed due to invalid strobe duty cycle. Rank[%d] Byte[%d] Rising Edge[%d] Falling Edge[%d]"
2003542366,2,ERROR,sxp_rx_dqs_training.c,"Advanced_Sxp_RxDqDqs failed margin check rank[%d] byte[%d]"
2003504031,0,ERROR,update_firmware.c,"Could not retrieve SPI Image Address"
200321804,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtDqBcomCtrl: 0x%x"
200073042,0,ERROR,commands.c,"Cmd Format Device, context block rebuild failed."
2000219610,1,ERROR,backside_training.c,"CPGC Test Failed on rankIndex %d"
2000179354,0,WARNING,key_management.c,"Security Metadata is not valid"
1999382272,1,ERROR,nlog_set_ddrt_io_init_info.c,"D_FW_STATUS: 0x%x"
1997596259,0,ERROR,ltec.c,"PMIC driver failed to apply LTEC update. Retrying."
1996704008,0,ERROR,key_management.c,"Failed to wrap PM-RK with security disabled wrapping key"
1990246004,1,WARNING,command_features.c,"Knob Identifier %d is not supported"
1990165701,0,ERROR,ait_dram.c,"Attempted to resume access without blocking first"
1989044606,1,ERROR,i2c_bus_manager.c,"Invalid core message 0x%X passed to I2C bus manager"
1988835678,1,ERROR,log_emask_imask_regs.c,"DA_EMASK_1: 0x%x"
1988785714,2,STATUS,ddrt_scheduler.c,"DDRT locked at %d us after %d tries"
1987100008,1,ERROR,fw_upd_halt_at_spi_write.c,"FwUpdate has been halted at block: %d"
1987012763,0,WARNING,command_features.c,"Operating frequency is invalid"
1986457531,0,ERROR,command_fw_update.c,"Cannot update FW because Security Engine is busy"
1981119390,0,ERROR,sxp_init.c,"Writing Training RMT Report to SPI failed"
1980170253,1,WARNING,spi.c,"Invalid Write Size: %d"
1979982773,3,ERROR,sxp_scheduler.c,"read SXP_REG_ADDR_PARAM_103 failed! value = 0x%x, die = %d, rank = %d \n"
1979378906,2,ERROR,spi_debug_structures.c,"Found In SPI Debug Region: RACQ Parity Error -> glb_ferr_1: 0x%08X, glb_nerr_1: 0x%08X"
1979281433,1,ERROR,command_fw_update.c,"Unexpected state %d"
1978682893,0,STATUS,command_software_triggers.c,"Fatal error software trigger is injected"
1978168173,1,WARNING,dfx.c,"ModuleSize was either NOT 256B aligned, less than 256B, or greater than 0x%08X"
1977248584,1,ERROR,nlog_config_lockdown.c,"D_FW_STATUS: 0x%x"
1976710392,0,DEBUG,key_management.c,"Wrapping S3 Stored Volatile Memory Keys"
1976333992,0,WARNING,command_features.c,"Invalid NLOG level selected"
1975009918,2,ERROR,mm_free_block_expansion.c,"Free block expansion AIT Read failed on byte aligned address 0x%08X_%08X"
1971043924,1,ERROR,log_emask_imask_regs.c,"PW_RAS_INTERRUPT_REQ: 0x%x"
1970075201,6,STATUS,barlow_creek_pmic_init_reason.c,"Fault Code 0 = 0x%x, Fault Code 1 = 0x%x, Fault Code 2 = 0x%x, Fault Code 3 = 0x%x, Fault Code 4 = 0x%x, Fault Code 5 = 0x%x"
1969620201,0,INFO,security_interface.c,"Security_GetSecurityResponse: ResponseQueue has response ready to process"
196934556,4,INFO,sxp_training.c,"SXP MRC Revision %d Build Date: %d/%d/%d"
1968497871,2,ERROR,thermal_manager.c,"Rank %d had all failedDies for Temp reading 0x%x"
1968019776,0,DEBUG,command_features.c,"SS: Set Master Passphrase"
1967732411,1,ERROR,log_power_event_start.c,"D_FUNC_DEFEATURE1: 0x%x"
1967209459,0,INFO,address_scrub.c,"Address Range Scrub Complete"
1962776953,1,ERROR,sxp_init.c,"Sxp_AdvancedRxDqsTraining failed rank: %d"
1960662223,0,ERROR,ddrt_scheduler.c,"Ddrt Mrc authentication failed!"
1958250207,0,ERROR,dma_polled.c,"Both AIT UECC, don't complete the transaction!"
1957918921,1,DEBUG,checkpoint.c,"Update WDT status: %d"
1957756755,0,WARNING,command_features.c,"Set Vendor Specific Command: Invalid Mailbox SubOpcode"
1956081956,7,ERROR,data_path_error.c,"Media error log created for the FERR at domain %d ferr %d bit %d, Error Type %d, Transaction Type %d, DPA 0x%08X_%08X"
1954153740,0,ERROR,sxp_init.c,"Reading Training RMT Report from SPI failed"
1952958157,0,ERROR,zqcal_periodic.c,"ZQCal one or more refreshes were unsuccessful"
1951285618,1,ERROR,data_path_error.c,"FIFO overflow / underflow error (%d)"
1950005229,1,ERROR,log_emask_imask_regs.c,"PW_EMASK_1: 0x%x"
1948992968,1,INFO,format_device.c,"HW supports up to 0x%x random WC. FW WC Randomization will be used that extended format time should be given."
1948112402,2,ERROR,sxp_decode_media.c,"0x50D register read failed. Can't check media type on Rank: %d, Die: %d"
1943532960,0,ERROR,task_error_handler.c,"First copy of AIT was poison.  FW prepare read of AIT copy!"
1942584673,1,ERROR,log_power_event_end.c,"RPQ_WDB_STAT_EMPTY: 0x%x"
1940199725,0,ERROR,security_md.c,"Failed to AES key wrap Salt with KEK - security enable base key"
1939823990,1,ERROR,ait_nm3_csr.c,"AIT N-3 entry has single bit correctable error. Index: %d"
1938977677,1,ERROR,log_emask_imask_regs.c,"CHN_IMASK_0: 0x%x"
1938646864,0,ERROR,power_budgeting_engine.c,"Setting average power budget to pTarget and entering open loop as FW is unable to process EM data in a timely manner for two consecutive accumulation windows"
1934774630,0,DEBUG,aes_bulk_encryption_selftest.c,"Verify AES Bulk Encryption successfully decrypted the first cacheline."
1933251809,1,ERROR,fw_init.c,"Training Retry Failed at Count: %d"
1933097936,0,ERROR,command_software_triggers.c,"Fatal error software trigger is injected"
1931814808,1,STATUS,log_ddrt_training_start.c,"DN_SPARE_CTRL: 0x%x"
1931186281,0,ERROR,hal_pmic_cap_test.c,"Cap self test getting result failed."
1930108008,0,ERROR,hal_pmic_rail.c,"Null pointer passed in, not updating dynamic rails,"
1928754479,1,ERROR,commands.c,"Cmd Format Device, security MD rebuild failed. %d"
1928740260,0,WARNING,breakpoint.c,"Invalid Breakpoint"
1926933255,1,ERROR,command_features.c,"Going to Normal Mode -> Current BSR: 0x%08x"
192677786,0,INFO,address_scrub.c,"Continue Address Range Scrub"
1924679483,0,ERROR,spi_debug.c,"Data won't fit in remaining SPI area, skipping SaveData call"
1921979292,0,WARNING,dfx.c,"Injection module framework is in DEBUG mode. Be careful!"
1921738773,0,ERROR,dpa_verify_error_handler.c,"This error happens on AIT line, complete transaction and go DIMM fatal!"
1921200119,5,INFO,dpa_for_pda.c,"0x%08X: found DPA 0x%08X_%08X for PDA %08X_%08X"
1920815331,1,ERROR,core_dump.c,"Stack address not found in stack regions! Failed to get call trace. addr: 0x%X"
1920221092,16,ERROR,kechika_river_pmic_driver.c,"Requested Update Values: A[%d][%x] B[%d][%x] C[%d][%x] D[%d][%x] E[%d][%x] F[%d][%x] G[%d][%x] H[%d][%x]"
1916996411,0,DEBUG,command_features.c,"Get Features: Alarm Threshold"
1915443139,1,ERROR,get_ait_info.c,"A_LVLNM2_BASE_DPA: 0x%x"
1915274769,0,ERROR,dpa_verify_error_handler.c,"Address Verify flow completed successfuly!"
1914943528,2,ERROR,package_spare_monitor.c,"Package sparing criteria met for package %d, error type %d"
1914600735,0,ERROR,power_budgeting_engine.c,"Energy meter missed an accumulation window"
1911357073,1,ERROR,partition_manager.c,"Unexpected number of mb %d payload unlock requests while media disabled."
1911306711,0,ERROR,ddrt_restore.c,"S3 Resume Restore has completed"
191119714,0,INFO,address_scrub.c,"Continue Address Range Scrub"
1909494995,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD2: 0x%x"
1908843152,4,ERROR,die_error_emulator.c,"DieErrorEmulator SxpCmd_SendCommandWriteRegister failed on rank : %d, sxpDie : %d, address : 0x%08X, value : 0x%08X"
1908504553,0,ERROR,core_dump.c,"SPI write failure during FW debug data flush!"
1906110682,5,ERROR,exception.c,"Exception: Instruction Pointer(eip) = 0x%x, Stack Pointer(esp) = 0x%x, info1 = 0x%x, info2 = 0x%x, eflags = 0x%x"
1904445995,0,DEBUG,task_security.c,"SECURITY_DISABLE_PASSPHRASE"
1904258694,0,DEBUG,task_security.c,"SECURITY_ERASE_UNIT"
1904103763,0,ERROR,ddrt_training.c,"Ddrt_CoarseRcvenTraining failed"
1904068352,0,ERROR,chn_no_cmd.c,"channel no command error queue overflow!"
1903115033,0,ERROR,sxp_training.c,"Sxp Mrc authentication failed!"
1902089689,1,DEBUG,commands.c,"Size of device characteristics - %d"
1899623832,0,ERROR,fw_img_auth.c,"Computed and derived hash do not match"
1896995115,0,WARNING,update_firmware.c,"Staged Major, Minor, or Security version is older than running FW. FW downgrades are not allowed."
1896851091,0,WARNING,command_features.c,"Invalid SKU"
1894229589,0,ERROR,task_command_handler.c,"Unknown mailbox rate limitting timer provided to rate limit timer callback"
1894050364,0,ERROR,ltec.c,"I2C bus request queue full at time of LTEC update."
1892125054,0,ERROR,update_firmware.c,"DMA Submission entry failed to queue."
1891153707,0,ERROR,sxp_platform_fgpk.c,"ZQCalLongInit failed"
1890302346,0,ERROR,power_budgeting_engine.c,"Energy meter 12V Coulomb count overflows."
1890127588,2,ERROR,sxp_rx_dqs_training.c,"Basic Sxp_RxDqDqs failed rank[%d] byte[%d]"
1888541650,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaWrScrLfsrL: 0x%x"
1887240386,1,ERROR,wear_level_move.c,"WLM BM aborted entered without BM abort status:%x"
1886291469,0,ERROR,dpa_verify_error_handler.c,"This error happens again after the transaction fatal, complete the transaction and go DIMM fatal!"
1884366191,1,ERROR,core_dump.c,"ViralPolicy - PmEnable: 0x%02x"
1882900629,2,ERROR,wear_level_move.c,"AitPolled_Write Failed on Backup Entry Address 0x%08X_0x%08X: "
1882183863,1,ERROR,spi_manifest.c,"Spi read failed when reading MMRC table version at address x%08x"
1881906645,1,ERROR,core.c,"MessageId is out of range. MessageId: 0x%X."
1878782486,1,ERROR,log_refresh_pointers.c,"P_EP_PDA_L: 0x%x"
1878575304,2,ERROR,short_stroke.c,"Short Stroke offset %d + size %d exceed DIMM capacity"
187789069,2,ERROR,ddrt_scheduler.c,"ERROR: DDRT PLL did not lock before timeout MSC_FNVIO_INIT_CONTROL_1.DDRTPLLLOCKED=0x%X, DDRT_CKDET=0x%X"
1875195070,1,INFO,hal_pmic_cfg.c,"PMIC Detected PRODUCT: 0x%x\n"
1873560897,0,ERROR,pcsclr_engine.c,"RDWR_BUF_CTRL REQ did not return to idle"
1873021332,0,ERROR,fw_state.c,"FwState_Save Failure - Retrying FwState_Save"
1871935751,5,ERROR,sxp_training.c,"Register 0x%08X at offset 0x%08X with maskValue 0x%08X wrote 0x%08X read 0x%08X"
1871847714,1,ERROR,dpa_for_pda.c,"Invalid Handle during dpa for pda ait dispatch. 0x%X."
1871786384,4,ERROR,sxp_scheduler.c,"SXP Mixed DeviceID detected [%d] != [%d] at rank=%d die=%d"
1869745196,0,ERROR,kechika_river_pmic_driver.c,"Cap self test getting result failed."
1869261024,0,ERROR,security_md.c,"Security MD rebuild failed."
1868530026,0,INFO,update_firmware.c,"Supplied image signature RSA decrypt failed"
1867882967,0,ERROR,translate_address.c,"HW WLM didn't pause in time."
1867112757,0,ERROR,ddrt_sense_amp_calibration.c,"Sense Amp Calibration Training- Failure did not find an SA Offset"
1867053675,0,ERROR,thermal_engine.c,"Controller temperature read failure"
1867020676,2,DEBUG,core_wear_level_move.c,"Invalid Block: 0x%08X_0x%08X"
1866672923,1,ERROR,update_firmware.c,"Supplied image is signed with wrong key. Debug signed images work only on PRE_PRQ part and release signed images work only on PRQ part. This part type: 0x%x"
1866169059,1,ERROR,power_budgeting_engine.c,"Wrong Coulomb count CSR address offset has been programmed in Energy Meter. em_status = 0x%x"
1863985668,1,DEBUG,ait_dram.c,"AIT DRAM Read Error detected: 0x%08X"
1863726529,1,WARNING,core.c,"Unknown subId for Core General Message Handler [%d]"
1863464791,0,DEBUG,task_command_handler.c,"Completing commands that had to do long operations like DMA's"
1862656216,0,INFO,host_interrupt.c,"HostInterrupt Issue Alert"
1859141847,1,ERROR,log_refresh_pointers.c,"P_EP_PDA_L: 0x%x"
1859128632,1,ERROR,nlog_region_lock.c,"D_DBUF_REG_LOCK: 0x%08x"
1858091180,0,ERROR,power_state.c,"Warm Reset Start"
1857946274,1,DEBUG,checkpoint.c,"Update DDRT Init Complete: %d"
1857401399,0,ERROR,security_md.c,"Security MD rebuild, Security MD flush failed."
1856514745,2,DEBUG,platform_config_data.c,"Aligned Address: 0x%08X_%08X"
1855056948,1,ERROR,security_md_flush.c,"Wrong power event notification: %d"
1853749439,1,ERROR,kechika_river_pmic_driver.c,"CAP test error - communication problem - promoting state from: %d - no further cap tests for this boot"
1851300909,0,ERROR,scheduler_dram.c,"DRAM Rcomp failed"
1850417030,4,ERROR,barlow_creek_pmic_init_reason.c,"Fault Code 0 = 0x%x, Fault Code 1 = 0x%x, Fault Code 2 = 0x%x, Fault Code 3 = 0x%x"
1849953565,1,STATUS,fw_init.c,"Previous boot PowerStateEvents is 0x%08x"
1849100585,0,ERROR,command_software_triggers.c,"Percentage remaining software trigger is disabled"
1848385568,1,ERROR,wear_level_move.c,"WearLevelMove_Dispatch unexpected AIT read msg:%x"
1847928994,3,STATUS,command_features.c,"DDRT IO init - Going to Normal Mode: trainingStatus=%d | -> Current BSR: 0x%08x_%08x"
1846368880,0,INFO,command_features.c,"The DDRT Alert Policy data is valid!"
1845832170,2,ERROR,core_dump.c,"CallStack Logging started: (stackPointer = 0x%08x, basePointer = 0x%08x)"
1845434169,12,INFO,sxp_scheduler.c,"SXP Addr Offset R[%d]:%x,%x,%x,%x,%x,%x,%x,%x,%x,%x,%x"
1845245703,0,ERROR,thermal_manager.c,"Entering thermal throttling"
1842780750,4,DEBUG,algo_rx_dqs_training.c,"Advanced_RxDqs Rising_Mid_Falling%d: %d_%d_%d"
1842365179,2,ERROR,message_channel.c,"Message channel timed out! ctrl = 0x%08X, status = 0x%08X"
1841872298,1,ERROR,log_power_event_start.c,"PowerStateEvents: 0x%x"
1840039763,0,ERROR,reg_flow.c,"RF Table Error: No Table Found"
1837722073,1,WARNING,host_interrupt.c,"packet ack for DDR-T interrupt 0x%02X timed out; consider increasing D_DDRT_INTR_TIMER val"
1836852100,3,ERROR,core_dump.c,"FwDebugData - assert[%d] = src [%d] line [%d]"
1835375534,0,ERROR,ait_dram.c,"DRAM load NOT started due to incomplete ait initialization!"
1834772901,0,INFO,overwrite_dimm.c,"Initialize Overwrite DIMM"
183421233,0,ERROR,barlow_creek_pmic_init_reason.c,"Fail to erase fault code."
183288449,3,INFO,commands.c,"Cmd Format Device, Capacity: %08X_%08Xd in %d-byte chunks."
1832416613,0,INFO,error_logging.c,"Initializing Logging"
1830013359,0,WARNING,task_command_handler.c,"DDRT Training In Progress - Command Not Valid"
1828914353,1,ERROR,ait_dram.c,"Wrong power event notification: %d"
1828542538,1,ERROR,platform_config_data.c,"Invalid Small Payload Part during get operation. pcd_spPart = 0x%08X"
1824967574,1,ERROR,command_fw_update.c,"Unexpected state %d"
1823236283,1,ERROR,sxp_trim_bundle.c,"Could not get VDM3 from S2X_REG_ADDR_TMR_VDM_3_DAC registerdata: 0x%04x"
1822632099,2,WARNING,get_fconfig.c,"DFX get Fconfig incorrect version Expected: 0x%X, Actual: 0x%X"
1821827345,1,WARNING,get_fconfig.c,"DFX Get Single Fconfig not found token: 0x%X"
1820051420,1,WARNING,get_fconfig.c,"DFX Get Fconfig incorrect transfer type: 0x%X"
1819489238,4,ERROR,aclk_periodic.c,"ACLK Calibration : SxpCmd_SendCommandWriteRegister failed on rank : %d, die : %d, address : 0x%08X, value : 0x%08X"
1816522375,0,ERROR,security_utils.c,"Secure Erase Unit key setup failed "
1815485141,2,STATUS,commands.c,"BIOS Api version restored to 0x%X, FW API: 0x%X"
1814470264,0,INFO,refresh.c,"Resuming Migration"
1813117742,3,ERROR,fconfig.c,"Fconfig_SetConfig mismatch token length Token: 0x%X actual: 0x%X expected: 0x%X"
1812928115,0,INFO,ait_dram.c,"Resume DRAM Load"
1812117650,2,ERROR,core_dump.c," Call[%d]: 0x%08x"
1811167415,0,INFO,task_command_handler.c,"MBox Command Unknown"
1809801207,0,ERROR,sxp_training.c,"Sxp Timings Error: No Table Found"
1808335914,1,ERROR,wear_level_move.c,"Default case in FBE state machine hit! STATE = %d"
1807879541,10,ERROR,kechika_river_pmic_driver.c,"Current Rail Values: A[%d][%x] B[%x] C[%x] D[%d][%x] E[%x] F[%x] G[%x] H[%x]"
1805775706,1,ERROR,log_emask_imask_regs.c,"DN_EMASK: 0x%x"
1802410674,0,WARNING,dfx.c,"Chunk index was not received incrementally"
180223719,0,ERROR,sxp_training.c,"SPI read failure during PMIC cycle count clear!"
1802183272,0,ERROR,ait_dram_scheduler.c,"Invalid AIT DRAM size from fconfig."
1801801088,0,STATUS,power_wake_isr.c,"S3 flow was aborted"
1801178285,0,INFO,fw_img_auth.c,"Decrypting image signature"
1799831063,2,ERROR,barlow_creek_pmic_init_reason.c,"Retrieved invalid code from Fault Code %d: 0x%x."
1799819129,0,ERROR,fw_init.c,"Insecure SPI FW Header was not erased!"
1798763125,0,ERROR,command_fw_update.c,"Cannot update FW because image sync has not completed"
1793733679,2,ERROR,ait.c,"AIT Log: Valid bit not set! base = 0x%x, hi = 0x%x"
1790455021,1,ERROR,command_features.c,"S3 Key not set %d"
1787172959,2,ERROR,sxp_rcven_training.c,"Sxp_CoarseRcven failed rank[%d] status[%x]"
1784859612,1,ERROR,adaptive_vdm.c,"AdaptiveVdm_SetSampleErrorThresholds requested for invalid rank count : %d"
178249616,2,WARNING,fconfig.c,"Set Fconfig failed Token: 0x%X, Status: 0x%X"
1781269146,0,ERROR,nlog_region_lock.c,"VDM tracking after DRAM load has finished."
1780354349,0,WARNING,fw_img_auth.c,"Date field is invalid"
1780058164,1,ERROR,power_budgeting_engine.c,"Energy meter 1.2V Coulomb count overflows. em_status = 0x%x"
1778020842,1,ERROR,core_dump.c,"  - CurrentMbTracker: %d"
1773390944,1,ERROR,power_budgeting_engine.c,"Energy meter 1.2V Coulomb count overflows. em_status = 0x%x"
1773100537,1,ERROR,get_ait_info.c,"A_AIT_DEFEATURE: 0x%x"
1770169746,2,WARNING,error_logging.c,"Size passed (0x%x) is bigger than available buffer size (0x%x)"
1768844319,4,ERROR,task_error_handler.c,"domain %u ferr_%u bit %u was set, ferr = 0x%x"
1765190876,1,ERROR,power_state.c,"Warm Reset: Unexpected Power State event [0x%x] detected."
176403271,1,ERROR,partition_manager.c,"Unexpected number of mb %d payload semaphore lock requests."
1763436204,2,ERROR,block_move_error_handler.c,"WLM CSR access response error: opcode = %d, error address = 0x%x"
1760511831,0,INFO,ddrt_sense_amp_calibration.c,"Starting Sense Amp Calibration Training"
1759237639,0,ERROR,ddrt_training.c,"Ddrt_RmtRxVrefTest failed"
175828029,1,ERROR,nlog_notify_ddrt_normal_mode.c,"D_FW_STATUS: 0x%x"
1757610715,1,INFO,checkpoint.c,"BSR Checkpoint: %X"
1756452312,0,DEBUG,ait.c,"AIT lookup is disabled!"
1756378651,1,ERROR,write_disturb_engine.c,"WD Threshold value (%d) is invalid in SetQueuePolicy during MediaManagerInit"
1752825012,1,ERROR,context_block.c,"Wrong power event notification: %d"
1750298846,1,ERROR,sxp_scheduler_init.c,"Unsupported SXP Device Device ID read error. DeviceId = 0x%X"
1749732664,1,INFO,ddrt_scheduler.c,"DDRT locked at %d us"
1749384268,1,ERROR,log_bsr.c,"D_FW_STATUS: 0x%x"
1746154321,0,INFO,power_state.c,"PC6 Exit: Clock Started"
1745602068,0,ERROR,commands.c,"Cmd Format Device, creating fw state failed."
1744799944,1,ERROR,reg_protect.c,"Write request detected in restricted region! (%08X)"
1741973990,1,ERROR,power_budgeting_engine.c,"Failed to suspend EM. EM reset status = 0x%x"
1740936688,2,ERROR,data_path_error.c,"overflow mask register at address 0x%x has value 0x%x"
1739204243,0,ERROR,thermal_manager.c,"Invalid power credits value. DDRPHY_SXP_TOP_SXPHSIO_SCH_PWR_CFG7 CSR should have a non zero value"
1737197610,1,INFO,read_disturb.c,"Read Disturb Random Interval is not 1 less than power of 2: 0x%X"
1735627880,0,ERROR,kechika_river_pmic_driver.c,"Failed to restore power on reset value"
1732939718,0,WARNING,command_features.c,"Set Vendor Specific Command: Invalid Mailbox SubOpcode"
1732760766,0,ERROR,power_loss_log.c,"Could not erase a PLI log due to polled DMA error"
173150529,0,ERROR,energy_meter.c,"Previously accumulated data hasn't been processed yet."
1731162379,0,ERROR,command_fw_update.c,"DMA Submission entry failed to queue."
172783311,1,INFO,ait_read_line.c,"Transition Ait Readline State Machine : %d"
172773809,1,ERROR,log_emask_imask_regs.c,"PRUNIT_ERR_SOURCE_EMASK: 0x%x"
1727552950,0,ERROR,fw_activate.c,"Activation complete, but ROM rejected the staged FW image."
1724301143,0,WARNING,fw_img_auth.c,"Module type invalid"
1724285312,0,WARNING,dfx.c,"Mismatching module build arch and firmware build arch"
1723604902,0,ERROR,command_fw_update.c,"Failed header corruption because of a verification test failure"
1723334090,0,ERROR,dma_polled.c,"RACQ Parity failure in dma polled"
1723007476,0,DEBUG,pmic.c,"PMIC Clear Bits Error"
1722868648,0,ERROR,fw_init.c,"The Dynamic and Adaptive VDM features have both been disabled!"
1722493108,1,ERROR,ait_nm3_csr.c,"AIT N-3 entry has double bit uncorrectable error. Index: %d"
1721392122,1,ERROR,command_fw_update.c,"Error erasing SPI block at address 0x%X during FW Update"
1718048944,0,INFO,command_log.c,"Output payload was filled with CEL entries."
171611916,0,DEBUG,power_state.c,"Warm Reset Flow PM Idle"
1715871023,2,ERROR,rom_api_fw_assert.c,"ROM API ASSERT HIT, pFileName = 0x%x, lineNum = %d"
1712965588,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD3: 0x%x"
1712861829,0,INFO,overwrite_dimm.c,"Starting Overwrite DIMM"
1712530604,1,ERROR,chn_no_cmd.c,"Channel no command flow started but there's no fault data, pw_ras_interrupt_req: 0x%X"
1712429141,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz3: 0x%x"
171220833,3,ERROR,core_dump.c,"  - MB[%d] Opcode [0x%04x] Status [0x%02x]"
1709792236,1,WARNING,spi.c,"Erase Range: Invalid Size %d"
1707646592,0,WARNING,update_firmware.c,"Tried to do a dfx FW update while DIMM is locked or not whitelisted"
1706889234,1,ERROR,thermal_manager.c,"Skipping Die [%d] for runningMaxTemp"
1706142018,0,ERROR,commands.c,"Invalid FW State. Failed to preserve lifetime stats"
1704876598,0,ERROR,cpgc.c,"CPGC FIFOs are not cleared"
1704337719,1,ERROR,log_emask_imask_regs.c,"PRUNIT_INTERRUPT_IMASK: 0x%x"
1702790683,1,DEBUG,wear_level_move.c,"WLM transition State Machine : %d"
1702279256,4,DEBUG,command_log.c,"-> version: %d. %d. %d. %d."
1702166994,0,ERROR,wear_level_move.c,"Bad Block Check write check FAILED!"
169815923,2,ERROR,task_media_interface.c,"More requests exist then should be possible. Free(%d) WIP(%d)."
1696326516,0,ERROR,command_inject_error.c,"Error Injection is enabled"
169272558,2,ERROR,sxp_training.c,"Sxp Mmrc Table Checksum did NOT match: c[0x%08x] != t[0x%08x]"
1692533996,1,ERROR,command_features.c,"NOT Going to Normal Mode - Undefined DDRT Trainining State: hostTraininingStatus=%d"
1691661869,1,ERROR,nlog_region_lock.c,"D_TWO_LM_BASE_ADDR_H: 0x%08x"
1691455927,0,ERROR,write_count_histogram.c,"Start address > stop address"
1690815659,0,DEBUG,task_security.c,"SECURITY_SET_MASTER_PASSPHRASE"
1689322329,3,ERROR,task_error_handler.c,"domain %u nerr_%u = 0x%x"
1686939860,0,WARNING,command_features.c,"Address Range Scrub: Invalid Address"
1686625255,0,ERROR,data_path_error.c,"AHB_BRG Error, no valid set in log registers!"
1686093078,0,WARNING,command_fw_update.c,"Cannot update FW because FW Update already occurred"
1685037881,1,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustS26Vdm at Window. Window : %d"
1683293644,1,ERROR,kechika_river_pmic_driver.c,"PLI Cap Value is Critically Low. Self Test Time : %d"
1681228858,1,ERROR,log_pli_io_trig.c,"DDRT_RESET_STATUS: 0x%x"
1681071222,1,ERROR,data_path_error.c,"SXPHSIO SCH error status register: 0x%x"
1680080574,0,ERROR,dpa_verify_error_handler.c,"Address Verify flow ends!"
1679532607,0,WARNING,dfx.c,"Payload type selected was not small (1) or large (0)"
1678954398,0,WARNING,command_fw_update.c,"Invalid initial packet number"
1675799292,0,DEBUG,refresh.c,"Power Transition: Pausing Refresh/Migration"
1674299057,1,ERROR,power_budgeting_engine.c,"Failed to disable EM preparing for FW activate. EmResetStatus = 0x%x"
1672927774,0,DEBUG,breakpoint.c,"Single Step Breakpoint"
1672042019,0,ERROR,power_budgeting_engine.c,"Energy Meter is paused for more than 2 accumulation windows."
1671070359,0,WARNING,command_features.c,"Both PM and 2LM disabled SKU"
1670567592,0,ERROR,dram_failure_trigger.c,"DRAM initialization status was corrupted."
1669641607,0,DEBUG,command_features.c,"SS: Unlock Unit"
166873059,0,DEBUG,aes_bulk_encryption_selftest.c,"Read the decrypted 256 Byte AES Bulk encryption test buffer from SXP executed"
1668211203,3,ERROR,kechika_river_pmic_driver.c,"Over Current Count: %d, Over Voltage Count: %d, Under Voltage Count: %d"
1668108006,2,ERROR,core_dump.c,"PowerCounters - Power Cycle Count: %d | Dirty Shutdowns: %d"
1666704201,2,ERROR,fw_image_sync.c,"Image Sync failed with error SPI Read at 0x%x in state: %d."
166665524,0,WARNING,fw_img_auth.c,"Header version field is invalid"
1664684726,1,ERROR,kechika_river_pmic_driver.c,"Pmic Init Reason Previously Logged: %d"
1663183020,0,DEBUG,platform_config_data.c,"MediaInterface returned NULL handler, exiting with error"
1663070792,1,ERROR,core_wear_level_move.c,"WearLevelMove_Dispatch unexpected relocate block msg:%x"
1662603409,1,ERROR,ltec.c,"LTEC received controller temperature of %d which is beyond thermal shutdown threshold"
1661928815,0,STATUS,command_software_triggers.c,"Unsafe shutdown software trigger is injected"
1660316377,2,WARNING,set_fconfig.c,"DFX Set Fconfig incorrect version Expected: 0x%X, Actual: 0x%X"
1658726390,1,ERROR,dynamic_vdm.c,"Dynamic VDM in FW activate reset on device ID 0x%X is not supported. Disabling."
1657044779,0,WARNING,command_features.c,"Invalid value for Package Sparing Policy Enable"
1656548297,1,ERROR,sxp_init.c,"Write DQ-DQS Training failed, Rank: %d"
1655847368,1,ERROR,fw_init_profiler.c,"Invalid FwInit_Event provided = 0x%X"
1654744417,4,ERROR,task_media_interface.c,"Unknown handle. 0x%08X. Free(%d) WIP(%d) Pending(%d)."
165365385,1,ERROR,kechika_river_pmic_driver.c,"UNKNOWN IDT PMIC Stepping - Product Stepping: [0x%X]"
165106077,0,ERROR,core_wear_level_move.c,"No Spare block for FreeBlockExpansion move, DROPPING REQUEST!"
1650327481,0,WARNING,spi.c,"Read: Invalid Address or Transfer Size"
1648273168,1,ERROR,core_dump.c,"SXP MMRC Version: %d"
1648144677,1,ERROR,data_path_error.c,"Error type reported by HW - %d (2-Unsuccessful, 1-DDRT SAI Error, 0-PCR Violation)"
164764211,0,ERROR,barlow_creek_pmic_init_reason.c,"Could not unlock the PMIC to erase the Fault Code Registers"
1646418501,3,ERROR,task_media_interface.c,"More requests exist then should be possible. Free(%d) WIP(%d) Pending(%d)."
1646224518,0,ERROR,fw_init.c,"Crypto self-test failed!\n"
1644684548,2,DEBUG,platform_config_data.c,"Start Address: 0x%08X_%08X"
1644044895,1,ERROR,sxp_training.c,"PMIC cumulative reboot count [%d]"
1643866555,1,ERROR,fw_init.c,"Recovery FW used %d times"
164297145,0,ERROR,cpgc.c,"CPGC failed to complete"
1642255350,1,DEBUG,host_interrupt.c,"Event[%d] -> set device blocking"
1641164998,2,ERROR,ddrt_scheduler.c,"Ddrt Mmrc Table Checksum did NOT match: c[0x%08x] != t[0x%08x]"
1638345883,2,ERROR,message_channel.c,"Message channel timed out! ctrl = 0x%08X, status = 0x%08X"
1636977642,3,ERROR,data_path_error.c,"This error domain %d ferr_%d bit %d causes DIMM fatal!"
1635270791,0,DEBUG,command_features.c,"Get Admin Features: SKU"
1634574256,1,WARNING,fw_image_sync.c,"Hash of body of block %d failed"
163327504,0,WARNING,dfx.c,"Mismatching module build platform and firmware build platform"
1631580681,0,DEBUG,power_state.c,"Removing Listener."
1630495396,0,DEBUG,command_features.c,"Set Admin Features: Platform Config Data"
1625780230,1,ERROR,nlog.c,"Failed to retrieve Nlog error: 0x%08X"
1625481417,0,ERROR,power_loss_log.c,"Error translating PLI log buffer A's dpa address to pda"
1623478252,0,INFO,fw_img_auth.c,"Calculating hash on fw image"
1623112085,8,STATUS,hal_pmic_init_reason_cwv.c,"Fault Code 0 = 0x%x, Fault Code 1 = 0x%x, Fault Code 2 = 0x%x, Fault Code 3 = 0x%x, Fault Code 4 = 0x%x, Fault Code 5 = 0x%x, Fault Code 6 = 0x%x, Fault Code 7 = 0x%x"
1622869274,2,DEBUG,data_path_error.c,"Illegal Access Occurred on AHB 0x%x, Error Index: %d"
1621283519,0,ERROR,commands.c,"Cmd Format Device, context block rebuild failed."
1620280422,2,ERROR,datastore.c,"Detected invalid datastore size: %d for datastore id: %d"
1615920935,2,ERROR,wear_level_move.c,"AitPolled_Write Failed on Backup Entry Address 0x%08X_0x%08X: "
1615249241,0,DEBUG,task_error_handler.c,"Task_ErrorHandler Init"
1614318896,1,ERROR,short_stroke.c,"Short Stroke Mode %d is invalid"
1613355033,2,ERROR,sxp_decode_media.c,"0x60F register read failed. Can't check media type on Rank: %d, Die: %d"
161202254,0,WARNING,task_security.c,"NULL command received"
1611438400,2,ERROR,kernel.c,"Unsettable: %d | Event %x"
1611414440,0,WARNING,command_features.c,"GetSecurityInfo: Invalid SubOpcode"
1607263388,1,ERROR,sxp_scheduler.c,"Failed to read SXP_MSR1 register rank: %d when checking reset pin enable field"
1606714014,0,WARNING,fw_image_sync.c,"Hash of body of first block failed"
1606467904,0,ERROR,command_features.c,"Transaction Fatal was detected and ERR# pin assertion is deferred on entry to normal mode"
1605529618,0,ERROR,power_budgeting_engine.c,"Energy Meter timer is shorter than I2C sequence execution time."
1605153340,1,ERROR,log_emask_imask_regs.c,"PW_RAS_INTERRUPT_REQ: 0x%x"
1604574159,0,DEBUG,platform_config_data.c,"DMA transfer complete"
1604245119,4,STATUS,fw_init_profiler.c,"FW changed Bus Frequency @ 0x%08X after %d us. Timer Frequency Before = %d MHz - After = %d MHz."
1603305152,0,ERROR,ltec.c,"Missed LTEC update. LTEC normal mode update requested prior to completing previous update request."
1601790617,1,ERROR,log_refresh_pointers.c,"P_RP_PDA_L: 0x%x"
1599787157,1,ERROR,log_emask_imask_regs.c,"MSC_IMASK: 0x%x"
1598949411,0,INFO,ait_dram.c,"Initialize the DRAM Load"
1597435495,0,ERROR,kernel.c,"PLI status bit seen! Forcing a PLI!"
1597335653,0,DEBUG,command_inject_error.c,"Inject poison PM region needs to be unlocked"
1596995342,1,ERROR,data_path_error.c,"Data path Error: This error %d causes Transaction Fatal!"
159648278,0,ERROR,commands.c,"Cmd Format Device, building AIT failed."
1595837324,1,INFO,task_command_handler.c,"Current Mailbox: %d"
1595676532,0,ERROR,command_features.c,"FW DDRT post-training steps failed"
1594064427,0,ERROR,wear_level_move.c,"No Spare block for FreeBlockExpansion move, DROPPING REQUEST!"
1590976798,3,DEBUG,dpa_for_pda.c,"0x%08X: DPA 0x%08X_%08X is in AIT level N-2"
1588924855,0,DEBUG,command_features.c,"SS: Security Freeze Lock"
1585135834,1,WARNING,command_features.c,"Knob Identifier %d is not supported"
1585110169,1,ERROR,power_state.c,"PowerState_Shutdown: GLB data buffer underflow is detected [PW_ERR_STS = 0x%x]."
1584028661,1,DEBUG,ddrt_scheduler.c,"DDRT Pll Bus Ratio is: 0x%08x"
1580561544,1,ERROR,core_dump.c,"FwDebugData - numAsserts    : %d"
1580441786,8,STATUS,update_firmware.c,"FW Update has successfully staged FW %02x.%02x.%02x.%04x, activation version: 0x%02x,""API version: 0x%04x. Current handshake API version: 0x%04x. FW Update Staging Count: %d"
1579882859,0,ERROR,adaptive_vdm.c,"AVDM_GetVdmDimmData requested VDM3 with S2X media."
1579407346,3,ERROR,sxp_scheduler.c,"read SXP_REG_IDREG failed! value = 0x%x, die = %d, rank = %d \n"
1579315749,0,ERROR,log_power_event_start.c,"LogPowerEventStart"
1578019327,0,ERROR,i2c_bus_manager.c,"I2C bus is in error state. Executing error handlers of queued requests."
1576754724,2,INFO,sxp_training.c,"Sxp Mmrc Table Checksum MATCHED: c[0x%08x] == t[0x%08x]"
1575869356,0,STATUS,command_inject_error.c,"Error Injection is disabled"
157539064,0,INFO,wear_level_move.c,"WLM: Address is within spare block region"
1575351113,1,ERROR,hal_pmic_rail_cwv.c,"Failed to restore power-on reset on Rail 0x%x"
1569954701,0,WARNING,update_firmware.c,"Supplied image header fields are invalid"
1569616686,0,ERROR,format_device.c,"Cmd Format Device, failed to flush fw state with life time statistic."
1567177009,1,ERROR,address_scrub.c,"ARS being failed due to an invalid handle 0x%X."
1566763386,0,DEBUG,command_features.c,"Set Features: PMON Registers"
1565707393,0,DEBUG,command_features.c,"Set Features: Alarm Threshold"
1564647539,0,ERROR,media_manager.c,"Bad Block queue is full, dropping request!"
1564049110,1,ERROR,log_emask_imask_regs.c,"AITDR_RAS_EMASK: 0x%x"
156231663,0,ERROR,dpa_verify_error_handler.c,"Address Verify flow ends with DIMM fatal!"
1561112866,1,ERROR,log_pli_io_trig.c,"MSC_SPARE_CTRL: 0x%x"
1560527905,0,ERROR,dma_polled.c,"DMA Polled complete with SRAM error twice in a row!"
156037984,0,ERROR,spi.c,"Program of remainder bytes failed"
1559060242,2,ERROR,die_error_emulator.c,"DieErrorEmulator: SxpCmd_SelectId failed on rank : %d, sxpDie : %d"
155833972,1,ERROR,power_budgeting_engine.c,"Energy meter 12V Coulomb count overflows. em_status = 0x%x"
1558327557,1,INFO,error_logging.c,"Loading log %d"
1556688165,2,ERROR,power_loss_log.c,"Sequence error occurred in previous PLI. PLI LogA sequence number (%d) LogB (%d)"
155522848,0,ERROR,dma_polled.c,"DMA Polled started while previous interrupt based DMA was not fully processed yet"
1554252990,0,INFO,command_errorlog.c,"Retrieving Error Logs"
1552644710,2,ERROR,die_error_emulator.c,"DieErrorEmulator: Invalid relative VDM level (VDM%d) for VDM%d"
1551468486,0,ERROR,drng_polled_fw.c,"DRNG engine is not ready to generate random number!\n"
1550729397,0,INFO,power_state.c,"PC6 Enter: Power down."
1549624210,0,ERROR,ait_dram.c,"Abandon DRAM Load"
1548931714,0,ERROR,format_device.c,"Cmd Format Device, failed to set initial write count to non-zero from DRNG."
1547340473,1,ERROR,log_power_event_end.c,"MSC_PLL_CTRL: 0x%x"
1545848740,0,ERROR,key_management.c,"Security key initialization failed!"
1541947721,0,WARNING,task_security.c,"Unable to authenticate S3 Resume passphrase: Encryption Disabled"
154034212,0,ERROR,kechika_river_pmic_driver.c,"Cap self test error flow failed."
1540189309,0,ERROR,vdm.c,"Vdm_AdjustVdm, trying to adjust VDM3 on S26 media!"
1540016469,0,ERROR,dpa_verify_error_handler.c,"Address Verify flow ends with DIMM fatal!"
1539950701,0,WARNING,command_features.c,"Partition in Locked Security State"
1539743068,0,ERROR,fw_image_sync.c,"SPI read error during copying one section of SPI to another!"
1539546537,2,WARNING,refresh.c,"system time 0x%08X_%08X is less than the power on time"
15379558,0,ERROR,kechika_river_pmic_driver.c,"Erroneous Cap test tick value"
1537746113,2,ERROR,sxp_trim_bundle.c,"irefSenseEnb could not be reduced by 2, setting to 0. rank = %d die = %d"
1537512990,0,DEBUG,task_error_handler.c,"New AIT Scrub Event"
1533955628,0,WARNING,command_fw_update.c,"Invalid SVN Downgrade Opt-in input Payload value"
1533224461,0,WARNING,dfx.c,"Mismatching module ID and ID received in input payload"
1531350121,0,WARNING,command_features.c,"Get Features: Invalid Mailbox SubOpcode"
1525438828,2,ERROR,spi_manifest.c,"Spi read failed when reading SXP timing table %d version at offset x%08x"
1525372921,1,DEBUG,task_command_handler.c,"Task Command Handler (0x%08X)"
1525353888,0,INFO,sxp_scheduler.c,"Sxp_GetDieInventory()!\n"
1524555044,0,ERROR,scheduler_dram.c,"AIT DRAM command timed out"
152448659,2,DEBUG,platform_config_data.c,"Start Address: 0x%08X_%08X"
1524409611,12,ERROR,adma.c,"Attempted DMA with invalid input. dpa_valid: %d, pda_valid: %d, sram_valid: %d, cmd = 0x%X, sram = 0x%X, dpa = 0x%08X_%08X, pda = 0x%08X_%08X, size = 0x%08X, flags = 0x%08X, capacity GB: %d"
1522134296,0,ERROR,authenticate_spi_region.c,"SPI read Failure during hash calculation on fw image header!"
1521885364,1,ERROR,log_power_event_end.c,"D_FUNC_DEFEATURE1: 0x%x"
1518630447,0,ERROR,fw_init.c,"Failed to program boot vid to Rail D."
1518381218,0,DEBUG,task_security.c,"SECURITY_GET_INFO"
1516858567,0,ERROR,ddrt_restore.c,"S3 Resume Failed- Unable to complete DDRT MMRC training "
1516028721,1,ERROR,log_emask_imask_regs.c,"DA_EMASK: 0x%x"
1514859574,0,ERROR,command_software_triggers.c,"Fatal error software trigger is injected"
1513946691,0,ERROR,write_delay_read.c,"Buffer address is 0x0"
1513657113,1,ERROR,sxp_trims.c,"PCL reg access PDA generation not supported for DIMMs with ranks %d"
1512588549,0,DEBUG,command_features.c,"SS: Security Freeze Lock"
15117455,2,ERROR,message_channel.c,"Message channel error! ctrl = 0x%08X, status = 0x%08X"
1511685322,3,ERROR,core_dump.c,"Context Block Data: Top[0x%x] | Bot[0x%x] | Valid[%d]"
1511298192,0,DEBUG,command_inject_error.c,"Inject poison DPA to memory type mismatch"
150854451,0,ERROR,command_features.c,"Clear History has been executed."
1507354308,0,ERROR,key_management.c,"Wrapping VM-RK with S3 wrapping key failed"
1506708071,0,ERROR,update_firmware.c,"DMA Submission entry failed to queue."
1506147059,0,ERROR,power_budgeting_engine.c,"Energy Meter is aborted."
1505283532,0,STATUS,update_firmware.c,"Previous FW Update failed to complete"
150463160,0,ERROR,ras.c,"Host poison queue overflow!"
1501253060,1,DEBUG,high_priority_message_handlers.c,"High Priority Surprise Interrupt handler: pm events = 0x%08x"
1497104117,0,ERROR,buffers.c,"Core Buffer released when queue was full. Going transaction fatal."
1496866911,0,WARNING,fw_img_auth.c,"Vendor ID invalid"
1495888229,6,ERROR,nc_bus_isr.c,"Nanocore SRAM RMW error. Error Count 0x%08X SRAM Rank 0x%08X Error Address 0x%08X Error Data 0x%08X Parity 0x%08X IRQ status 0x%08X"
1495780578,0,ERROR,security_utils.c,"Secure Erase Unit key setup failed "
1494928272,1,ERROR,io_csr.c,"IO CSR invalid parameter lane number = 0x%x"
1494288978,0,WARNING,command_fw_update.c,"Invalid transfer type in transfer header"
1490709795,0,WARNING,security_interface.c,"SET_S3_KEY security request timed out"
14903632,0,ERROR,power_budgeting_engine.c,"FW was unable to process energy meter data in a timely manner"
1488219865,1,ERROR,ras.c,"RAS Log: Valid bit not set - PC_LOG_RPDA_P0_PE = 0x%x"
1487376524,0,ERROR,format_device.c,"Cmd Format Device, failed to erase PMIC init reason."
1485669524,0,ERROR,commands.c,"Cmd Format Device, failed to flush fw state with life time statistic."
1485323985,0,ERROR,spi_debug.c,"Failed to initialize Spi Debug region due to Spi Erase failure."
1482967499,1,ERROR,data_path_error.c,"PW ERR STS FIFO U/O Flow Errors: 0x%08X"
1482561710,3,ERROR,sxp_scheduler.c,"read SXP_REG_ADDR_PARAM_103 failed! value = 0x%x, die = %d, rank = %d \n"
1481710524,0,ERROR,spi_debug.c,"Failed to initialize Spi Debug region due to SPI Read failure"
1481484361,0,INFO,command_log.c,"Get Smart/Health Info"
1479350573,2,ERROR,skip_img_sync_at_ddrt_training.c,"Skipping image sync in power up: %d, training state: %d"
1477589975,0,ERROR,write_count_histogram.c,"Write Count Status: WD pending counter overflowed"
1473235322,0,ERROR,sxp_rank_interleave.c,"Unknown SXP devices, cannot set deck bits."
147290567,0,ERROR,sxp_init.c,"Sxp_SaveSxpIoRegisters failed"
1472020074,0,INFO,command_inject_error.c,"Mailbox command completed"
1471115123,1,WARNING,set_fconfig.c,"DFX Set Fconfig length too big: 0x%X"
1470648038,0,INFO,ait_dram.c,"DRAM Load already completed! No need to resume!"
1469695944,0,ERROR,drng_polled_fw.c,"DRNG Fatal error, cannot get random number!"
1469523578,0,ERROR,mm_block_move.c,"Unexpected:  Asynchronous cascaded calls to Mm_BlockMove_PauseEngine when not already paused."
1469439904,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTxDqSwz4: 0x%x"
146923519,0,INFO,address_scrub.c,"Initialize Address Range Scrub"
1469150680,0,ERROR,ltec.c,"I2C bus request queue full at time of LTEC update."
1468335627,2,ERROR,ras_error_log.c,"Unmapped Transaction Type in Media Error Log! stype = 0x%x, write = %d"
1464294516,0,ERROR,core_dump.c,"SPI read failure during FW debug data init!"
1463561765,4,ERROR,ddrt_sense_amp_calibration.c,"[0-71]SENSE AMP CAL TRANSITION VALUES FAILURE SEEN AT 1's     [0-31] = 0x%x | [32-63] = 0x%x | [64-95] = 0x%x | [96-127] = 0x%x"
1462845441,0,WARNING,command_fw_update.c,"Invalid transfer type in transfer header"
1461210358,0,DEBUG,command_features.c,"Set Features: Alarm Threshold"
1457742518,1,ERROR,command_features.c,"NOT Going to Normal Mode - Undefined DDRT Training State: hostTrainingStatus=%d"
1457478167,0,INFO,address_scrub.c,"Abort Requested"
1456866490,1,ERROR,long_op.c,"Wrong power event notification: %d"
145634410,1,ERROR,thermal_manager.c,"Skipping Die [%d] for runningMaxTemp"
1454885183,0,INFO,security_interface.c,"Security State: Frozen"
1454259768,18,STATUS,kechika_river_pmic_driver.c,"Requested Update Values: A[%d][%d][%x] B[%d][%x] C[%d][%x] D[%d][%d][%x] E[%d][%x] F[%d][%x] G[%d][%x] H[%d][%x]"
144809071,1,INFO,kechika_river_pmic_driver.c,"PLI Cap value is good. Self Test time: %d"
1445575297,0,DEBUG,error_logging.c,"DMA Callback"
1444118199,3,INFO,sxp_training.c,"SXP Ranks: %d, DRAM Ranks: %d, Dies: %d"
1443568890,0,ERROR,ltec.c,"Setting Health Status Critical. HSR is set to performance degraded"
1438464298,9,ERROR,task_error_handler.c,"STYPE AIT UECC. Source Transaction Type 0x%02X; Initial VDM 0x%02X; Retry Index 0x%02X; Fault data 0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
1437968080,1,ERROR,data_path_error.c,"SRAM read parity error is found at SRAM address 0x%x, retry the request!"
1437578412,1,INFO,error_logging.c,"Saving log %d"
1437224483,0,ERROR,buffers.c,"Core Buffer requested when queue was full. Going transaction fatal."
1436303450,0,WARNING,command_features.c,"Knob Value is not valid"
1435623000,1,ERROR,sxp_trim_bundle.c,"Could not populate ResetPulseEn for read. Register Data: 0x%04x"
1435529861,0,ERROR,algo_tx_dq_dqs_training.c,"Calculated ODT Off latency was somehow out of range, failing."
1435433623,3,ERROR,sxp_trim_bundle.c,"Could not populate AdwlVdm %d from S2X_REG_ADDR_TMR_ADWLVDM_NEAR_FAR_DECK_%d. Register Data: 0x%04x"
1435381271,0,ERROR,security_interface.c,"Couldn't queue SHA-256 SDMA security request"
143113086,0,INFO,write_disturb_refresh.c,"Resuming Write Disturb Refresh"
1431007446,1,WARNING,error_logging.c,"Failed to load log %d"
1429525809,0,ERROR,command_software_triggers.c,"Percentage remaining software trigger is disabled"
1429453917,0,DEBUG,task_security.c,"SECURITY_DISABLE_PASSPHRASE"
1429155841,1,ERROR,ras.c,"RAS Log: Valid bit not set - DS_LOG_RDATA_WIDB_UECC_1 = 0x%x"
1428383559,2,ERROR,spi_debug_structures.c,"Found In SPI Debug Region: Assertion -> Source: %d, Line: %d"
142750154,0,ERROR,command_features.c,"s3 resume path but not s3 complete handshake"
1427367271,2,WARNING,set_fconfig.c,"DFX Set Fconfig checksum failure InputPayload Checksum: 0x%X, Calculated: 0x%X"
1426372383,2,ERROR,kechika_river_pmic_driver.c,"PMIC Returned invalid Product ID. Expected: 0x%X, Received: 0x%X"
142547542,1,ERROR,reg_flow.c,"SPI Table Error: Bad CSR Entry [%x]"
1424201348,1,ERROR,log_pli_io_trig.c,"PC_AVDM_CTRL: 0x%x"
1422677858,2,ERROR,spi_logger.c,"SPI 0x%08X: 0x%08X"
1422300629,2,ERROR,power.c,"config empty or wdb ddrt empty check timeout - D_DDRT_FUNC_STS = 0x%X, RPQ_WDB_STAT_EMPTY = 0x%X"
1422133321,0,ERROR,die_error_emulator.c,"DieErrorEmulator: Error map due to earlier request exists."
1417630619,1,ERROR,log_emask_imask_regs.c,"A_EMASK_1: 0x%x"
1417490988,0,ERROR,i2c_bus_manager.c,"Energy meter failed to resume after queued I2C bus requests were processed."
1414237461,1,ERROR,sxp_init.c,"Sxp_RcvenTraining failed rank: %d"
1411733075,2,ERROR,sxp_scheduler.c,"Failed to write to SXP_MSR1 register rank: %d die: %d during media reset pin firewall"
1411483578,2,ERROR,commands.c,"BIOS Api version set to 0x%X, FW API: 0x%X"
1411093547,0,WARNING,command_features.c,"Attempted to set a invalid System Time"
140905570,0,WARNING,command_fw_update.c,"Unexpected packet number"
1402966680,0,DEBUG,pmic.c,"PMIC Set Bits Error"
1402266405,0,ERROR,power_loss_log.c,"Could not load a PLI log (A) due to polled DMA error"
1400696187,0,WARNING,fw_image_sync.c,"Hash of header failed"
1399356762,0,WARNING,task_security.c,"Unable to set master passphrase: Encryption Disabled"
1397966892,1,ERROR,kechika_river_pmic_driver.c,"Invalid pmic rail passed to UpdateRailValue. rail: %d"
1397302507,1,ERROR,log_power_event_start.c,"IO_INIT_CTRL: 0x%x"
1397134802,1,ERROR,kechika_river_pmic_driver.c,"UNKNOWN IDT PMIC Stepping - Product Stepping: [0x%X]"
1397025943,0,WARNING,security_interface.c,"SHA-256 SDMA security request timed out"
1396655700,1,ERROR,nlog_notify_ddrt_normal_mode.c,"MSC_PLL_CTRL: 0x%x"
1396012788,3,DEBUG,dpa_for_pda.c,"0x%08X: block DPA 0x%08X has FWP 0x%08X"
1394789894,1,ERROR,security_md_flush.c,"DMA_STATUS_ERROR encountered while flushing security metadata ID: %d."
1394166767,2,ERROR,core_dump.c,"FwState Data: Top[0x%x] | Bot[0x%x]"
1392925234,0,WARNING,command_features.c,"Kernel has not set system time"
1392676177,2,ERROR,core_dump.c,"Call[%d]: 0x%X"
1391514174,1,ERROR,log_power_event_start.c,"D_FW_STATUS: 0x%x"
1390365618,0,DEBUG,address_scrub.c,"DN_LOG_RDATA_POISON_1 Error scrub. Scrub command will be sent again."
1389764217,3,ERROR,core_dump.c,"  - MB[%d] Opcode [0x%04x] Status [0x%02x]"
1387236419,1,ERROR,feature_state_data.c,"Failed to retrieve any valid FSD copy with error opcode: 0x%x - going to partial read."
1386452083,0,ERROR,kechika_river_pmic_driver.c,"Null pointer in KechikaRiverPMIC_GetInitialDynamicRailSettings"
1384366998,3,ERROR,sxp_scheduler.c,"read SXP_MSR12 failed! value = 0x%x, die = %d, rank = %d \n"
1383215000,0,ERROR,dpa_verify_error_handler.c,"Address Verify flow ends!"
1381747557,0,DEBUG,command_features.c,"CONFIG_LOCKDOWN Executed"
1381641667,1,ERROR,io_csr.c,"IO CSR invalid parameter regOffset = 0x%x"
1380759144,0,INFO,ddrt_sense_amp_calibration.c,"Starting Calibration Training"
1379841001,1,ERROR,log_power_event_end.c,"P_PWM_STS: 0x%x"
1379321137,1,ERROR,die_error_emulator.c,"Invalid VDM level %d"
1377947449,2,ERROR,sxp_write_leveling.c,"SXP Coarse WrLvl failed rank[%d] bytePassFlag[%x]"
1377424839,2,DEBUG,platform_config_data.c,"dstAddress: 0x%08X_%08X"
1377010135,1,ERROR,sxp_init.c,"After trim change ZQCalLong command failed for rank: %d"
1376207783,1,ERROR,log_emask_imask_regs.c,"CHN_IMASK_2: 0x%x"
1376047430,0,DEBUG,command_features.c,"Set Admin Features: FW Debug Log Level"
1375194162,2,DEBUG,refresh.c,"Starting Refresh from Address 0x%08X to 0x%08X"
1374928735,3,ERROR,task_media_interface.c,"MI 0x%X request made when no free requests were available. Free(%d) WIP(%d)."
1374375745,1,ERROR,data_path_error.c,"CSR Error, valid bit AND valid_unimpl_bit not set in log registers! FnvError %d."
1374312779,4,ERROR,host_interrupt.c,"Packet ACK for DDR-T interrupt timed out - eird = 9x%02X | type=%d | D_DDRT_INTR_CTRL=0x%X | D_DDRT_INTR_STS=0x%X"
1374008868,2,ERROR,sxp_write_leveling.c,"Fine WrLvl failed Rank[%d] Byte[%d]"
1373305723,0,DEBUG,task_security.c,"SECURITY_SET_MASTER_PASSPHRASE"
1371830971,0,ERROR,memory_info.c,"Unknown stat total requested"
1371595062,0,ERROR,command_features.c,"Host Side DDRT Link Training Failure detected - Link unstable!"
1370878685,2,ERROR,command_features.c,"System Time Set at boot. Time: 0x%x_%x"
1370456528,0,ERROR,feature_state_data.c,"Hashing 0's failed"
1363383319,0,INFO,core_dump.c,"Sha Hash failed for coreDump"
1362191973,0,INFO,address_scrub.c,"Address Range Scrub Stopping from Abort"
1361997564,0,ERROR,key_management.c,"Wrapping VM-RK with S3 wrapping key failed"
1361942129,1,ERROR,adaptive_vdm.c,"AdaptiveVdm_Pull_StartFlow cannot start pull sample. Target block DPA 0x%08x, is not an unused block!"
136064679,1,DEBUG,task_command_handler.c,"Event Flag: 0x%08X"
1359371146,0,ERROR,media_statistics.c,"RMW Uncorrectable encountered but max write count CSR contains a value of 0. Could not decrement MWC."
1359227201,3,ERROR,partition_error.c,"write address region error %u at DPA 0x%08X_%08X"
1359015945,0,WARNING,fw_image_sync.c,"Hash of header failed"
1356258183,1,INFO,reg_flow.c,"RF Table Version[0x%x]"
135625754,1,ERROR,core_dump.c,"***** CoreDump Start: %x *****"
1354265067,0,ERROR,ait_read_line.c,"AitReadLineRead Complete with Failure Status!"
1351927558,0,ERROR,dfx.c,"Krnl Event Timer Expired"
1350844633,3,STATUS,security_error.c,"Security Key Error Log: 0x%08x = 0x%08x_%08x"
1347129240,0,ERROR,fw_init.c,"Watch dog timer event in previous boot detected!"
1347010313,1,ERROR,security_reset.c,"Wrong power event notification: %d"
1346619492,2,ERROR,sxp_wr_dqs_training.c,"Adv_TxDqDqs failed rank[%d] byte[%d]"
1344225411,2,ERROR,sxp_rx_dqs_training.c,"Basic Sxp_RxDqDqs failed rank[%d] byte[%d]"
1344183906,4,WARNING,sxp_write_leveling.c,"WARNING: WL Rank[%d] Byte[%d]: Rising[%d] Falling[%d]"
1344054418,3,ERROR,fw_image_sync.c,"Failed image sync abort: AbortedImgChunk(%d), Total garbage blocks to feed (%d), Failed at garbage block (%d), "
1342989975,3,ERROR,power.c,"EADR Flush failure detected in current Warm Reset path EADR Status = 0x%X | prev status = 0x%X | prev value = 0x%X"
1342040621,1,ERROR,partition_manager.c,"Unexpected number of mb %d payload lock requests."
134109602,1,ERROR,log_emask_imask_regs.c,"PC_EMASK: 0x%x"
1340102244,2,ERROR,sxp_wr_dqs_training.c,"Basic_TxDqDqs failed rank[%d] byte[%d]"
1339197603,2,ERROR,sxp_init.c,"Sxp_AdvancedRxDqsTraining failed rank: %d Training type: %d"
1338734504,0,WARNING,command_features.c,"Unknown Command"
1338433861,0,DEBUG,refresh.c,"Power Transition: Pausing Refresh"
1338185477,0,ERROR,ddrt_training.c,"Ddrt_SenseAmpCalibration failed"
1337543889,0,DEBUG,command_features.c,"Get Admin Features: DDRT IO Init Info"
1336318099,1,ERROR,log_emask_imask_regs.c,"DA_EMASK: 0x%x"
1335020383,1,ERROR,command_features.c,"Host Side DDRT Link Training Failure detected: 0x%x. Link unstable!"
1334640997,0,INFO,command_log.c,"Get Long Operation Status"
1333112864,1,ERROR,thermal_engine.c,"Set temperature calibration: %08X"
1332982531,1,ERROR,fw_image_sync.c,"Image Sync buffer callback occurred when we were not expecting it. Current state = %d."
1332584485,0,DEBUG,task_security.c,"SECURITY_OVERWRITE_DIMM"
1332525340,0,WARNING,dfx.c,"Uploaded module's header is not valid!"
1329805049,2,ERROR,sxp_rcven_training.c,"Fine Rcven failed rank[%d] byte[%d]"
1328613373,1,ERROR,command_features.c,"Going to Normal Mode -> Current BSR: 0x%08x"
1328073136,4,WARNING,command_features.c,"Invalid set power management params. Values are not within minimum and maximum limits"" AveragePowerLimit = %d; averagePowerTimeConstant = %d; turboModeState = %d; turboPowerLimit = %d"
1327584189,4,ERROR,barlow_creek_pmic_init_reason.c,"Fault Code 0 = 0x%x, Fault Code 1 = 0x%x, Fault Code 2 = 0x%x, Fault Code 3 = 0x%x"
1327558926,2,ERROR,ras_error_log.c,"Unmapped Transaction Type in Media Error Log! stype = 0x%x, write = %d"
1327464867,0,WARNING,platform_config_data.c,"Failed to get handle from Media Interface"
1327436771,1,ERROR,health_manager.c,"Die on package %d met failure criteria with no spare package available."
132503705,4,ERROR,sxp_scheduler.c,"Error (%d) writing to register addr: 0x%04x rank: %d die %d"
1324043323,1,ERROR,context_block.c,"DMA_STATUS_ERROR encountered while flushing context block ID: %d."
1323329683,0,ERROR,kechika_river_pmic_driver.c,"Failed to enter power good state"
1321317471,1,ERROR,log_emask_imask_regs.c,"PRUNIT_ERR_SOURCE_EMASK: 0x%x"
1321266492,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr2: 0x%x"
1318314623,0,ERROR,command_software_triggers.c,"Unsafe shutdown software trigger is disabled"
1317802630,1,ERROR,kechika_river_pmic_driver.c,"PMIC Init Reason: %d"
1317146308,1,ERROR,wear_level_move.c,"FBE Block Move aborted entered without BM abort status:%x"
1315884361,0,ERROR,dma_polled.c,"DMA Polled started while previous interrupt based DMA was not fully processed yet"
1315485187,0,WARNING,command_features.c,"Invalid PCD Payload Type"
1314866364,1,ERROR,ras.c,"RAS Log: Valid bit not set - PW_LOG_WDB_UE = 0x%x"
1313481281,0,STATUS,ait_dram.c,"DRAM loading completes!"
1312786246,0,ERROR,sxp_scheduler.c,"Resync reset: PLL lock timed out!"
1312517677,0,ERROR,sxp_commands.c,"FGPK Test Mode Reg Read Latency WA for S26 MPPR 18 failed."
1312031693,1,ERROR,core_dump.c,"FwDebugData - bootCycleCount: %d"
1311084003,1,DEBUG,kechika_river_pmic_driver.c,"Waiting %d microseconds for PMIC voltage ramp to complete"
1308828088,0,DEBUG,wear_level_move.c,"FBE AIT Read Callback"
1307462279,1,INFO,ddrt_restore.c,"Ddrt_Restore -> No timer needed [%d]"
1306609740,0,WARNING,fw_img_auth.c,"Module type invalid"
1306292667,0,ERROR,command_fw_update.c,"Updated firmware failed a verification test"
1305657229,2,INFO,refresh.c,"the system was powered off for %08X_%08X seconds"
1305446605,2,ERROR,ddrt_training.c,"Clock alignment failure detected- applying workaround. gIsColdBoot = %d caf_delay = 0x%x"
1304966099,1,ERROR,sxp_training.c,"Sxp Timings Error: Bad CSR Entry [%x]"
1304429429,0,ERROR,dynamic_vdm.c,"DynamicVdm_AdjustVdm one or more refreshes were unsuccessful"
1302201820,1,ERROR,log_emask_imask_regs.c,"DS_IMASK: 0x%x"
1301735417,0,WARNING,platform_config_data.c,"Failed to get handle from Media Interface"
1301426958,1,DEBUG,command_reset_policies.c,"0x%08X"
1301029490,0,DEBUG,power_state.c,"Warm Reset Flow Retrain DDRT"
1300878185,0,ERROR,command_features.c,"s3 resume path but not s3 complete handshake"
1300155806,3,ERROR,update_firmware.c,"DMA read of block %d of image failed. State: %d. Substate: %d"
129859152,7,ERROR,dma_polled.c,"Uncorrectable error! FaultData 0x%08X_0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
1296848025,0,ERROR,drng_polled_fw.c,"DRNG Fatal error, cannot get random number!"
1296734489,0,STATUS,fw_activate.c,"Unsupported HW type."
1295664630,1,ERROR,nlog_notify_ddrt_normal_mode.c,"PCSCLR_CFG6: 0x%x"
1295329784,0,STATUS,fw_activate.c,"FW Activation Complete."
1293784772,0,ERROR,ddrt_sense_amp_calibration.c,"No transition found on more than 2 CMD Lines for DDRT Sense Amp Calibration CMD"
1292431522,0,DEBUG,command_features.c,"SS: Set Security OptIn"
129181713,0,INFO,security_interface.c,"security SubmitWork RequestQueue was full FAIL."
1288995923,7,ERROR,data_path_error.c,"Media error log created for the FERR at domain %d ferr %d bit %d, Error Type %d, Transaction Type %d, PDA 0x%08X_%08X"
1288702080,1,ERROR,assert.c,"ESP +  4: 0x%X [ Vec # |       EFLAGS           ]"
1288440182,12,INFO,sxp_scheduler.c,"SXP Stepping ID R[%d]:%x,%x,%x,%x,%x,%x,%x,%x,%x,%x,%x"
1285092815,1,ERROR,log_power_event_start.c,"D_RST_STS: 0x%x"
1284598536,0,DEBUG,task_security.c,"SECURITY_SET_NONCE"
1282735224,0,ERROR,adaptive_vdm.c,"AVDM_GetVdmDimmData requested VDM0 with S15 media."
1281124004,2,DEBUG,command_features.c,"Nonce Setting To: 0x%08X:0x%08X"
1280846439,0,ERROR,ait_dram.c,"DRAM load NOT started due to incomplete ait initialization!"
1278823297,1,ERROR,dma_polled.c,"Completed in-flight DMA inside polled DMA! Inside PLI: %d"
1278415294,2,ERROR,core_dump.c,"PowerCounters - Power Cycle Count: %d | Dirty Shutdowns: %d"
1277640343,4,ERROR,core_dump.c,"CB Datastore Id | Header Version | Entries Size : 0x%x | 0x%x | 0x%x [%d]"
1275893696,2,ERROR,algo_tx_dq_dqs_training.c,"Adv_TxDqDqs failed rank[%d] byte[%d]"
1274122572,0,WARNING,command_features.c,"Alarm Threshold: Invalid Percentage Remaining parameter"
1273372426,0,ERROR,fw_init.c,"VCAP self-test failure reported"
1273042802,2,ERROR,ltec.c,"Unsupported rail ID %d passed to Ltec_GetSlopeOffset. Using default slope offset of %d uv/C."
1272967033,0,DEBUG,error_logging.c,"DMA Callback"
1271851187,0,INFO,update_firmware.c,"Supplied image signature RSA decrypt failed"
1271047344,2,INFO,fw_image_sync.c,"Copying SPI from 0x%08X to 0x%08X"
1270590874,0,ERROR,refresh.c,"Package Migration Started"
1269971642,0,ERROR,ltec.c,"LTEC failed to set PMIC VCCDDRD_SXP (A) and VCCDDRD_DDRT (D) rails to DDRT training voltages."
1268463850,1,ERROR,log_power_event_end.c,"D_RST_STS: 0x%x"
1264091752,0,ERROR,sxp_training.c,"SPI write failed during saving raw data buffer!"
1260058316,0,INFO,ddrt_restore.c,"DdrtRestore_TrainDdrtPostPllLocked called!"
1260002758,1,ERROR,buffers.c,"Invalid Buffer released. Buffer address = 0x%08X. Going transaction fatal."
1259576869,2,ERROR,kechika_river_pmic_driver.c,"PLI Cap Value is Critically Low. Self Test Time : %d, Voltage: %d"
1256552070,3,ERROR,fconfig.c,"Fconfig_SetConfig mismatch token length Token: 0x%X actual: 0x%X expected: 0x%X"
1256371182,0,WARNING,command_features.c,"Kernel has not set system time"
125631445,3,ERROR,core_dump.c,"Context Block Data: Top[0x%x] | Bot[0x%x] | Valid[%d]"
1255773938,1,ERROR,log_power_event_end.c,"D_FW_STATUS: 0x%x"
1255621311,2,DEBUG,nlog.c,"wr 0x%08X = 0x%08X"
1255615203,0,ERROR,log_zqcal_short.c,"Polled flush of Nlog buffer to media has occurred."
1255263537,4,ERROR,ltec.c,"Error detected in LTEC Voltage Calculation, programming boot voltage. BootVid: %d, slope: %d, temperature: %d, newVid: %d"
1254923440,0,ERROR,fw_init.c,"Security key initialization failed!\n"
1253923877,0,ERROR,security_utils.c,"Failed to AES key wrap Salt with KEK - security enable base key"
1253535752,0,ERROR,sxp_scheduler.c,"SXP PLL is not locked"
1252230349,0,STATUS,command_inject_error.c,"Enabling poison on 4 cache lines"
1251098299,0,INFO,command_inject_error.c,"Dma transfer successful!"
1251092773,0,DEBUG,task_command_handler.c,"Task_CommandHandler: Media Disabled Command Not Allowed"
1249875506,3,ERROR,core_dump.c,"FwDebugData - assert[%d] = src [%d] line [%d]"
1247111744,0,ERROR,dpa_verify_error_handler.c,"Address Verify flow completed successfuly!"
1246213720,0,ERROR,ddrt_scheduler.c,"Ddrt Mrc Programming Error: No Table Found"
1245605169,1,ERROR,nlog_region_lock.c,"D_TWO_LM_BASE_ADDR_L: 0x%08x"
1244760538,0,ERROR,dma_polled.c,"DMA retry failed with SRAM parity error again!"
1244462549,0,INFO,security_interface.c,"security_SubmitWork completed."
1244375019,1,ERROR,power_budgeting_engine.c,"Energy Meter timer is shorter than I2C sequence execution time. em_status = 0x%x"
1242270735,15,ERROR,dma_polled.c,"Uncorrectable error! FaultData Rank: 0x%01X; Stype: 0x%01X; RetryIndex: 0x%01X; Vdm: 0x%01X; FwErrComp: 0x%01X; FwErrAddrComp: 0x%01X; Length: 0x%01X; Rdir: 0x%01X; WdbAddr: 0x%02X; Rid: 0x%02X; Rtype: 0x%02X; WriteCount: 0x%01X; InitialVdm: 0x%01X; AitSecondCopyPoison: 0x%02X; PoisonStatus: 0x%06X;"
1240840039,1,ERROR,sxp_init.c,"Fine RcvEn Training failed, Rank: %d"
1240567229,0,WARNING,command_features.c,"Nonce is all zeroes!"
1235681683,0,WARNING,dfx.c,"Payload type selected was not small (1) or large (0)"
123459809,9,ERROR,task_error_handler.c,"STYPE AIT UECC. Source Transaction Type 0x%02X; Initial VDM 0x%02X; Retry Index 0x%02X; Fault data 0x%08X_0x%08X; DPA 0x%08X_%08X; PDA 0x%08X_%08X"
1233282586,7,ERROR,data_path_error.c,"Media error log created for the FERR at domain %d ferr %d bit %d, Error Type %d, Transaction Type %d, DPA 0x%08X_%08X"
1232873794,1,ERROR,update_vsm_block_sxp_io_traffic.c,"PCSCLR_CFG1: 0x%x"
1232715711,0,STATUS,command_features.c,"Clear History has been executed."
123152720,0,DEBUG,fw_image_sync.c,"Image Sync Allocate Callback"
1229529542,1,DEBUG,memory_info.c,"DFX Memory Info Page Requested - Allowed [%x]"
1229341173,1,ERROR,nlog_region_lock.c,"D_PM_BASE_ADDR_L: 0x%08x"
1229265140,0,DEBUG,task_security.c,"SECURITY_EXPONENTIATE"
1224380313,0,STATUS,fw_activate.c,"FW Activate Starting..."
1224098509,0,ERROR,command_inject_error.c,"Error Injection is disabled"
1223905358,0,DEBUG,task_command_handler.c,"Task_CommandHandler: Host is trying to call a disabled command."
1223306720,0,DEBUG,command_features.c,"SS: Set Passphrase"
1220644779,0,WARNING,command_features.c,"Incompatible DIMM type"
1216570224,4,WARNING,command_features.c,"Invalid set power management params. Values do not meet granularity requirements"" AveragePowerLimit = %d; averagePowerTimeConstant = %d; turboModeState = %d; turboPowerLimit = %d"
1215440682,0,ERROR,task_error_handler.c,"spurious error IRQ!"
1214580022,1,ERROR,season_device.c,"Season trims uploaded on rank: %d"
1214420408,4,INFO,ddrt_scheduler.c,"DDRT MRC Revision %d Build Date: %d/%d/%d"
1213897248,1,ERROR,fw_image_sync.c,"Image Sync buffer callback occurred when we were not expecting it. Current state = %d."
1213132864,1,ERROR,ait_dram.c,"AIT DRAM Uncorrectable read error detected at index 0x%x"
1212581003,1,DEBUG,data_path_error.c,"AHB Address translated to DPA 0x%x"
1210820739,2,ERROR,short_stroke.c,"Short Stroke offset %d + size %d exceed DIMM capacity"
1209580610,0,ERROR,power_budgeting_engine.c,"Failed to resume energy meter - energy meter is in unknown state."
120946911,1,INFO,fw_image_sync.c,"Image Sync was aborted in state %d. Buffer released."
1209273848,1,ERROR,core_dump.c,"RefreshState - State                    : 0x%02x"
1209147360,1,ERROR,power_state.c,"PowerState_SignalPowerEvent: Unexpected Power State event [0x%x] detected."
1207682915,5,ERROR,wdt.c,"Watchdog Timeout: Instruction Pointer(eip) = 0x%x, Stack Pointer(esp) = 0x%x, Fault Permission = 0x%x, Fault Address = 0x%x, eflags = 0x%x"
1204527427,0,DEBUG,wear_level_move.c,"FBE AIT DMA Line Callback"
1204192338,1,ERROR,warm_reset.c,"Warm Reset: Unexpected Power State event [0x%x] detected."
1203963530,1,ERROR,nlog_chn_fwrwcmd.c,"CHN_FWRWCMD0: 0x%x"
1203544197,1,ERROR,security_md_flush.c,"DMA_STATUS_ERROR encountered while flushing security metadata ID: %d."
1202260252,2,ERROR,dynamic_vdm.c,"Dynamic VDM SxpCmd_SelectId failed on rank : %d, die : %d"
1201478952,2,ERROR,ltec.c,"Unsupported rail ID %d passed to Ltec_GetSlopeOffset. Using default slope offset of %d uv/C."
1199206119,1,ERROR,core_wear_level_move.c,"FBE Block Move aborted entered without BM abort status:%x"
1199139875,0,WARNING,commands.c,"Invalid Mailbox SubOpcode"
1198848176,1,ERROR,sxp_trim_bundle.c,"Could not populate HnlwlSelv RD%d value 4 in register"
1198441575,1,DEBUG,high_priority_message_handlers.c,"High Priority Power Management task handler: pwrMgmtStatus = 0x%08x"
1197631731,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr0: 0x%x"
119610826,1,ERROR,thermal_manager.c,"Component[%d] temperature samples taken in three consecutive 100ms window are bad. Going transaction fatal."
1194633878,0,ERROR,fw_init.c,"Dynamic VDM/IRST feature has been disabled!"
1192834557,2,ERROR,algo_receive_enable.c,"Fine Rcven failed rankIndex[%d] byte[%d]"
1192463873,0,ERROR,platform_config_data.c,"Internal Device Error: Handle was NULL"
1190736957,0,INFO,ddrt_restore.c,"Ddrt_Restore -> Starting Timer"
1190734318,0,WARNING,health_manager.c," Life Span Percentage Remaining <= 1%"
1190536508,0,WARNING,address_scrub.c,"Error limit reached. Aborting Address Range Scrub"
1187594217,0,ERROR,mmrc_parser.c,"MMRC Programming Error: No Mode Flags"
1186641829,0,ERROR,crypto_selftests.c,"3DXP XTS-AES-256 Decryption Test FAIL: Result does not match expected KAT output."
1186416574,2,ERROR,sxp_init.c,"Sxp_AdvancedTxDqsTraining failed rank: %d Training type: %d"
1185551587,3,ERROR,partition_error.c,"read address region error %u at DPA 0x%08X_%08X"
1185341373,2,ERROR,wear_level_move.c,"AitPolled_WriteReverseMap Failed on Backup Entry Address 0x%08X_0x%08X: "
1184721323,0,ERROR,i2c_bus_manager.c,"FW attempted to issue an I2C bus request with a NULL request routine."
1183513841,0,ERROR,command_features.c,"Host Side DDRT Link Training Failure detected- Link unstable!"
1183222713,0,DEBUG,address_scrub.c,"DMA Callback"
1182241303,3,ERROR,die_error_emulator.c,"DieErrorEmulator: VDM adjust value resulted in underflow or overflow. Base VDM value 0x%04x Adjustment value 0x%04x Sign %d"
1180042065,0,WARNING,overwrite_dimm.c,"Overwrite DIMM Error Found"
1179817332,0,WARNING,debug_log_data.c,"Failed to get handle from Media Interface"
1178992188,1,DEBUG,wear_level_move.c,"Transition FBE State Machine : %d"
1178867077,1,ERROR,hal_pmic_vendor_bwv.c,"UNKNOWN IDT PMIC Stepping - Product Stepping: [0x%X]"
1178425186,0,ERROR,core_dump.c,"***** CoreDump Start *****"
1178054707,0,INFO,ddrt_sense_amp_calibration.c,"Training Complete.  Channel reset"
1174897460,1,ERROR,barlow_creek_pmic_init_reason.c,"Failed to retrieve Fault Code %d."
1174267908,0,DEBUG,memory_info.c,"Output Payload was NULL"
1174038694,0,INFO,ddrt_restore.c,"Ddrt_Restore -> Starting Timer"
1171700684,0,INFO,command_log.c,"Get Long Operation Status"
1171182154,1,ERROR,die_error_emulator.c,"Die error emulator not supported on 3DXP device: 0x%08x"
1169663369,0,ERROR,command_software_triggers.c,"Unsafe shutdown software trigger is injected"
1168899302,2,ERROR,write_count_histogram.c,"Max write count (%d) < min write count (%d)"
1167611650,1,DEBUG,high_priority_message_handlers.c,"High Priority Power Fail task handler: pwrMgmtStatus = 0x%08x"
1165808557,1,ERROR,sxp_device_access.c,"3DXP Devices do not have Persistent ID fused on rank[%d]. Cannot apply desired device mode."
1163338821,1,ERROR,kechika_river_pmic_driver.c,"PMIC Error returned while updating rail %d"
1162692414,1,ERROR,hardware_wear_level_move_engine.c,"WLM HW Stop request typed: %d is invalid."
1162313468,2,ERROR,kechika_river_pmic_driver.c,"PMIC Returned invalid Product ID. Expected: 0x%X, Received: 0x%X"
1158536710,0,WARNING,fw_img_auth.c,"Tried to do a customer debug FW update with a perPartID that did not match this DIMM"
1157535348,0,ERROR,enqueue_media_request.c,"Media request is being enqueued."
1154765574,0,WARNING,dfx.c,"Mismatching module build arch and firmware build arch"
1154491545,0,ERROR,power.c,"PMIC Rail D got svid fuse value 0x0"
1150934788,0,WARNING,command_features.c,"Clear History can only be executed on Bios Mailbox"
1150573327,1,ERROR,command_inject_error.c,"Wrong event notification: %d"
1146548684,0,ERROR,kechika_river_pmic_driver.c,"Couldn't read the current rail settings, skipping PMIC Rail Init"
1146029036,0,ERROR,kechika_river_pmic_driver.c,"Cap self test setup failed."
114163442,2,ERROR,sxp_trims.c,"Unrecognized media on Rank: %d, Die: %d"
1137406230,0,DEBUG,dfx.c,"Upload via large payload complete"
1137015802,1,ERROR,media_manager_engine.c,"WLM Threshold in PW_WCCTRL had an unexpected value: %d. Re-initializing WLM threshold"
1134661846,1,ERROR,write_count_histogram.c,"Step size is invalid (%d)"
1133272645,0,WARNING,task_media_interface.c,"Attempted to complete a DMA when there is no active DMA."
1132866168,0,DEBUG,power_state.c,"Surprise Reset Start"
1132734733,0,ERROR,update_firmware.c,"Failed to hash and commit image body to SPI"
1131053893,3,WARNING,core_wear_level_move.c,"FBL tail pointer and FBL Head point to each other. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
1130945063,0,DEBUG,command_features.c,"Get Features: Optional Config"
1129225464,3,ERROR,sxp_scheduler.c,"read SXP_REG_ADDR_MSR_11 failed! value = 0x%x, die = %d, rank = %d \n"
1126775253,1,ERROR,dma_polled.c,"DMA Polled complete with SRAM error at AHB index %d!"
1126273052,0,INFO,command_inject_error.c,"Mailbox command completed"
1126117891,0,ERROR,overwrite_dimm.c,"AIT Read failed"
1125916917,4,DEBUG,sxp_rx_dqs_training.c,"Advanced_RxDqs Rising_Mid_Falling%d: %d_%d_%d"
1125895465,0,ERROR,dma_polled.c,"Dma polled timed out during operation"
1122517478,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrioCmdEn: 0x%x"
1122174021,0,INFO,error_logging.c,"Creating new thermal entry"
1121808003,1,ERROR,log_pli_io_trig.c,"MSC_FNVIO_INIT_CONTROL_1: 0x%x"
1120214895,1,ERROR,ras.c,"fault data is not valid! PC_LOG_WCTL_NO_CMD_2: 0x%X"
1117907078,2,DEBUG,refresh.c,"Starting Refresh from Address 0x%08X to 0x%08X"
1117010607,1,ERROR,security_md.c,"Security md checksum failed on copy: %d"
1116654146,4,ERROR,ddrt_sense_amp_calibration.c,"[0-71]SENSE AMP CAL TRANSITION VALUES FAILURE SEEN AT 1's     [0-31] = 0x%x | [32-63] = 0x%x | [64-95] = 0x%x | [96-127] = 0x%x"
1115972789,1,ERROR,reg_protect.c,"Unaligned write request detected (%08X)"
1114428393,0,ERROR,log_ddrt_training_start.c,"DDRT training started."
1113723173,1,DEBUG,task_error_handler.c,"0x%08X: logging UECC fault"
1113506694,2,ERROR,sxp_trim_bundle.c,"Could not populate AdReset value 0x%02x to 0x%04x."
1111462089,5,ERROR,main.c,"MPU exception: Instruction Pointer(eip) = 0x%x, Stack Pointer(esp) = 0x%x, Fault Permission = 0x%x, Fault Address = 0x%x, eflags = 0x%x"
1111366682,2,WARNING,get_fconfig.c,"DFX Get Fconfig incorrect transfer type: 0x%X expecting: 0x%X"
1110552140,0,WARNING,task_security.c,"Unable to Unlock Unit: Encryption Disabled"
1110510980,1,ERROR,nlog_notify_ddrt_normal_mode.c,"MSC_PLL_CTRL: 0x%x"
1109406242,0,ERROR,fw_init.c,"Failed to load soft fuses"
1109113381,4,WARNING,command_features.c,"Invalid set power management params. Values do not meet granularity requirements"" AveragePowerLimit = %d; mBBAveragePowerTimeConstant = %d; mBBEnable = %d; mBBMaxPowerLimit = %d"
1108647219,1,ERROR,nlog_region_lock.c,"D_TWO_LM_BASE_ADDR_L: 0x%08x"
1107788112,0,ERROR,thermal_manager.c,"Powering off DIMM: Critical Temperature"
1106818012,3,ERROR,core_dump.c,"OutputPayload QWORD[%d]: 0x%08x_%08x"
1105920520,1,ERROR,log_vdm_for_wlm.c,"CHN_FWCMD4: 0x%x"
1105597746,0,ERROR,key_management.c,"Failed to AES key unwrap Salt with KEK - security enable base key"
1105420668,1,ERROR,log_vdm_for_wlm.c,"FreeBlockExpansionState: %d"
1103389373,0,WARNING,security_interface.c,"EAU security request timed out"
110303729,1,ERROR,log_power_event_end.c,"PowerEvent: 0x%x"
1102157398,0,DEBUG,command_features.c,"PCD Get Data DDRT"
1101602905,0,DEBUG,task_security.c,"SECURITY_SHA256DMA"
1100421019,0,DEBUG,command_features.c,"SS: Set S3 Resume Passphrase"
1099887548,1,ERROR,power_state.c,"Warm Reset: Unexpected Power State event [0x%x] detected."
1099333091,0,INFO,core_wear_level_move.c,"FBE: AIT line of address contains SMD or CB or FSD"
1098648422,1,ERROR,nlog_set_ddrt_io_init_info.c,"D_FW_STATUS_H: 0x%x"
1094481665,1,ERROR,nlog_notify_ddrt_normal_mode.c,"ddrtDaDdrtTrainingMr5: 0x%x"
1093642572,0,WARNING,dfx.c,"Mismatching module build config and firmware build config"
1093464163,1,ERROR,wear_level_move.c,"FreeBlockExpansion_Dispatch unexpected AIT get line msg:%x"
1092859231,0,WARNING,commands.c,"Invalid Mailbox SubOpcode"
1091781706,1,WARNING,get_fconfig.c,"DFX Get Single Fconfig not found token: 0x%X"
1091358307,0,WARNING,dfx.c,"Module ID or Module Size do NOT match with previous chunk"
1090464703,0,DEBUG,command_features.c,"SS: Security Secure Erase"
1090052376,0,INFO,ddrt_training.c,"DdrtTraining_StartTraining!"
1089783659,0,ERROR,ltec.c,"Missed LTEC update. LTEC normal mode update requested prior to completing previous update request."
1087194040,1,ERROR,sxp_commands.c,"Unexpected FGPK SXP Reg Read Latency value of 0x%X."
1085869318,3,INFO,error_logging.c,"Start Address for Log %d : 0x%08X_%08X"
1085289527,0,WARNING,health_manager.c,"Spare Blocks <= 1%"
1084632657,0,ERROR,ltec.c,"LTEC normal mode update missed due to I2C bus error."
1076834890,0,WARNING,dfx.c,"Chunk index was not received incrementally"
1075666012,0,ERROR,command_inject_error.c,"Error Injection is enabled"
1075492359,0,ERROR,log_ait_move_complete.c,"AIT NM2 table move completed!"
1073851156,1,WARNING,viral.c,"Data path Error: %d"
1073304267,0,DEBUG,buffers.c,"Queue not empty, someone is waiting for a buffer"
1071996169,1,WARNING,task_error_handler.c,"unexpected fault type 0x%02X"
1069747988,0,WARNING,sxp_commands.c,"SXP WriteReg REQ bit still set after delay!"
1066836322,0,ERROR,host_interrupt.c,"HostInterrupt AbortInFlight - Aborting Pending"
106664969,2,ERROR,chn_no_cmd.c,"Chn no cmd with no WLM for DPA 0x%08x_%08x deallocating WDB entry"
1065104594,0,ERROR,command_fw_update.c,"Cannot update FW because image sync failed"
1063523521,0,INFO,write_disturb_refresh.c,"Resuming Write Disturb Refresh"
1061775673,0,WARNING,command_features.c,"Get Features: Invalid Mailbox SubOpcode"
1060800086,1,ERROR,power_budgeting_engine_imf.c,"Invalid time constant %d Sec requested. Power budgeting engine applies the value but does not store in FW state."
1058583810,1,ERROR,write_count_histogram.c,"Invalid Transfer Type %d"
1055927188,2,ERROR,ddrt_training.c,"Clock alignment failure detected- applying workaround. gIsColdBoot = %d caf_delay = 0x%x"
105581917,0,ERROR,fw_init.c,"WDB was not flushed on the previous boot cycle (WRITE_DATA_FLUSH_COMPLETE=0)"
1055719248,0,WARNING,command_features.c,"No Address Range Scrub in Progress and no enable sent"
1054654192,1,ERROR,read_write_pmic.c,"After sending I2C request EM_CTRL: 0x%08x"
1053040302,0,DEBUG,command_features.c,"SS: Get Security State"
1052957330,0,ERROR,power_event_at_image_sync.c,"POWER_EVENT_AT_IMAGE_SYNC function has been removed"
1050208323,1,ERROR,log_power_event_start.c,"PowerEvent: 0x%x"
1048482382,1,ERROR,format_device.c,"Cmd Format Device, security MD rebuild failed. %d"
1047383201,0,ERROR,fw_init.c,"Watch dog timer event in previous boot detected!"
1042207320,1,DEBUG,spi.c,"Sending %d read commands to SPI Flash"
1041688659,0,INFO,security_interface.c,"Security_GetSecurityRequest: RequestQueue has work ready to process"
1039440610,4,ERROR,algo_write_leveling.c,"SXP Fine WrLvl failed due to invalid strobe duty cycle. Rank[%d] Byte[%d] Rising Edge[%d] Falling Edge[%d]"
1037758928,0,ERROR,core_wear_level_move.c,"Wear Level Move operation has fatally failed, request has been dropped!"
1037079042,3,WARNING,wear_level_move.c,"FBL head pointer not in valid range. Head: 0x%x, Tail: 0x%x, BBHead: 0x%x"
1036759035,0,ERROR,throttling_engine.c,"Invalid DIMM rank type detected."
1035379349,0,ERROR,wear_level_move.c,"FBE AIT DMA Line Callback DMA Failure"
1034996827,0,WARNING,task_media_interface.c,"Attempted to complete a DMA when there is no active DMA."
1032728052,1,ERROR,kechika_river_pmic_driver.c,"PLI Cap Value is Low. Self Test Time : %d"
1030429712,0,DEBUG,command_features.c,"Get Admin Features: FW Debug Log Level"
102839861,0,INFO,fw_init.c,"Loaded Fw State, now dirtying saved state"
1027843499,1,ERROR,nlog_region_lock.c,"D_PM_BASE_ADDR_L: 0x%08x"
1027498004,1,ERROR,sxp_commands.c,"Unexpected FGPK SXP Read Latency value of 0x%X."
102499321,0,DEBUG,wear_level_move.c,"AIT Update Callback"
1022721873,0,DEBUG,power_state.c,"Warm Reset Exit Clock Enable"
1022634540,0,ERROR,backside_training.c,"Writing Training report to SPI failed"
102175488,0,DEBUG,command_pmon.c,"Get Features: PMON Registers"
1021156039,1,ERROR,get_ait_info.c,"A_LVLNM1_BASE_DPA: 0x%x"
1021085370,4,ERROR,task_error_handler.c,"AIT Scrub Start! FaultData DPA 0x%08X_%08X; PDA 0x%08X_%08X"
1020494162,4,STATUS,fw_init_profiler.c,"ROM init completed @ 0x%08X (%d us). FW init completed @ 0x%08X after %d us."
1019619637,2,ERROR,write_count_histogram.c,"Received more than maximum supported steps. Number of steps: supported = %d, requested = %d"
1019345122,0,ERROR,security_interface.c,"Couldn't queue HMAC security request"
1019121753,8,ERROR,core_dump.c," - EAX: 0x%08x | EBX: 0x%08x | ECX: 0x%08x | EDX: 0x%08x | ESI: 0x%08x | ESP: 0x0%08x | EBP: 0x%08x | EIP: 0%08x"
1017505357,4,INFO,ddrt_scheduler.c,"DDRT MRC Revision %d Build Date: %d/%d/%d"
1017022219,2,ERROR,wear_level_move.c,"AitPolled_WriteReverseMap Failed on Backup Entry Address 0x%08X_0x%08X: "
101618542,0,ERROR,barlow_creek_pmic_init_reason.c,"Fail to erase fault code."
1015374166,0,ERROR,platform_config_data.c,"Internal Device Error: Handle was NULL"
1014071958,1,ERROR,die_error_emulator.c,"sxp_reg library returned with status = %d"
1013609801,0,ERROR,energy_meter.c,"Energy meter failed to reset"
1013571479,0,ERROR,high_priority_message_handlers.c,"Warm reset entry is detected in PC6 transition flow"
1011812704,0,INFO,core_wear_level_move.c,"Invalid address value"
1011194301,0,ERROR,short_stroke.c,"Short Stroke Fconfig values are invalid, Going DIMM Fatal"
1008838300,4,WARNING,command_features.c,"Invalid set power management params. Values do not meet minimum, maximum or granularity requirements."" AveragePowerLimit = %d; averagePowerTimeConstant = %d; turboModeState = %d; turboPowerLimit = %d"
1008353993,1,ERROR,hal_pmic_vendor.c,"Unrecognized PMIC vendor - Vendor ID: [0x%x]"
1006990039,1,ERROR,hal_pmic_rail.c,"Rail 0x%x is not a dynamic rail."
1005678386,0,ERROR,ddrt_training.c,"Ddrt_XoverCalibration failed"
1004328781,0,ERROR,dfx.c,"Injection module upload failed!"
1002412571,1,ERROR,platform_config_data.c,"PCD Partition Invalid [%x]"
1001181892,0,ERROR,wear_level_move.c,"Wear Level Move operation has fatally failed, request has been dropped!"
