================================================================================
            Intel(R) Server Platform BIOS Release Notes
================================================================================

INTEL(R) Server Boards and Systems
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

================================================================================
DATE : December 16 2020
TO : Multi-Core Intel(R) Xeon(R) Processor-Based Server Platform customers
SUBJECT : BIOS Release notes
================================================================================
                           LEGAL INFORMATION
================================================================================

Information in this document is provided in connection with Intel Products
and for the purpose of supporting Intel developed server boards and systems.
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation 
may have patents or pending patent applications, trademarks, copyrights, or
other intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any such
patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (C) 2021 Intel Corporation.

================================================================================
                                                      ABOUT THIS RELEASE
================================================================================
Build Stamp : SE5C620.86B.02.01.0013
Build Date : Dec 15 2020
================================================================================
                                                      Supported Platforms
================================================================================
        S2600WFR Family
        S2600BPR Family
        S2600STR Family

================================================================================
                                                      BIOS COMPONENTS/CONTENTS
================================================================================
Processors supported:
	1st and 2nd Generation Intel(R) Xeon(R) Processor Scalable families

Microcode versions:
        CPUID           Version              Status
        0x50654        0x02006a08     (1st Generation Intel(R) Xeon(R) Scalable H0,M0,U0)
        0x50656        0x04003003     (2nd Generation Intel(R) Xeon(R) Scalable B0,L0,R0)
        0x50657        0x05003003     (2nd Generation Intel(R) Xeon(R) Scalable B1,L1,R1)

SATAAHCI: 
        v2.00i
VROCSATAEfi: 
        v6.3.0.1005
VROCSATALegacy: 
        v6.3.0.1005
VROCsSATAEfi: 
        v6.3.0.1005
VROCsSATALegacy: 
        v6.3.0.1005
VROC NVMe UEFI drivers: 
        v6.3.0.1005
ESRT2 UEFI drivers: 
        05140000
NVMDIMMDriver: 
        v01.00.00.3506
NVMDIMMHii:
        v01.00.00.3506
AspeedVideo: 
        1.09
ASTVBIOS: 
        1.09
BIOSACM: 
        Production,v1.7.41_LBG
SINIT: 
        Production,v1.7.49_LBG
PDR: 
        V1.0
S2600WFR_WFT_WFS FPKSI:
        4.10
S2600WFR_WFQ_WF0 FPKSI:
        4.10
S2600BPR FPKSI:
        4.10
S2600STR FPKSI:
        4.10
ME: 
        04.01.04.423
HfiPcieGen3:
        v1.9.2.0.0
Security Revision:
        0006

================================================================================
                                  INSTALLATION NOTES
================================================================================

WARNING:  It is very important to follow these instructions as they are written.
Failure to update using the proper procedure may cause damage to your system.

Firmware Update Tools: iFlash32_V14_1_Build14

User can update BIOS flash image via the next method...
    
    UEFI iFlash32
    1.  Copy the entire contents of the zip file to the root of a USB flash drive
    2.  Boot to uEFI Shell, then change the Shell to the mapped device (USB flash drive)
        Example: Shell> fs0: (or fs1:)
    3.  Run updBIOS.nsh, updME.nsh, updFD.nsh and reset the system after each region upgrade
    4.  Reboot the system after the last upgrade is completed
    5.  Do *NOT* interrupt the BIOS POST during the first and second boot

================================================================================
			     BIOS RECOVERY INSTRUCTIONS
================================================================================

The Recovery process can be initiated by setting the recovery jumper (called BIOS Recovery Boot Jumper)
Details regarding the jumper ID and location can be obtained from the Board TPS.

BIOS starts the recovery process by first loading and booting to the recovery image from backup BIOS region.
This process takes place before any video or console is available. Once the system boots to the recovery image use the following steps to perform the BIOS recovery:

   1.  The BIOS POST screen will appear displaying the progress and it automatically
       boots to the uEFI SHELL
   2.  Follow any of the next two methods for recovery process.
   
   Note: Recover mode will clean up all user previous changed BIOS settings including ITK saved settings 
   
BIOS update under recovery mode as below two methods:

The USB flash drive is necessary for the primary BIOS upgrade and must contain the following files 
under its root directory:
   1.  uEFI iFlash32.efi (including iflash32_temp.efi and ipmi.efi )
   2.  *.CAP( the released BIOS capsule which version you expect to update)
   3.  UpdBIOS.nsh (update accordingly to use proper *.CAP file)

  A Method: Install USB media after recovery boot to shell, you need to follow below steps
   1. Under Shell, type "map -r" to map all disc
   2. Change the Shell to mapped device file system
      Example: Shell> fs0: (or fs1:)
   3. Execute the UpdBIOS.nsh script for BIOS update, wait for BIOS update complete
   4. Power OFF the system, and revert the recovery jumper position to "normal operation".
   5. Power ON the system. 
   6. Do *NOT* interrupt the BIOS POST during the first boot.
  
  B Method: Install USB media prior to recovery boot
    It will boot automatically into EFI Shell to invoke the Startup.nsh script and start the flash update application.
    IFlash32.efi requires the supporting BIOS Capsule image file (*.CAP). After the update is complete, there will be a message displayed stating that the "BIOS has been updated successfully" indicating the recovery process is finished. 
    The user should then power off the system and revert the recovery jumper back to normal operation and restart the system by performing a power cycle.

Note:
    The Startup.nsh file includes parameters to upgrade not only the BIOS, but the ME, FD, BMC, FRUSDR and DCPMM

================================================================================
                                 IMPORTANT NOTICE
================================================================================
1. Package C-State only works well with Xeon Scalable Family H0 parts, for other Xeon Scalable Family stepping, C6 non-retention is hardcode from BIOS side.
2. BIOS R00.01.0001 does not support online downgrade to any Dxxx or Xxxx BIOS.
3. BIOS R00.01.0001 removed Xeon Scalable Family A1 microcode(m1350651_8000002B) and Xeon Scalable Family B0 microcode(m9750652_80000035).
4. Removed 'UpdateNvram' support for iflash32 tool for security reason of SRA bios.
5. Security revision upgrade to v0002 on BIOS R00.01.0002 will prevent BIOS downgrade via normal mode to R00.01.0001, user can use BIOS recovery mode for BIOS downgrade. Although Intel doesn't recommend downgrading firmware
6. One new production key is integrated onto R0004 BIOS, which will correct an OEM string. 
7. Security revision upgrade to 0004 on BIOS R0009 will prevent BIOS downgrade via normal mode to previous version that with lower security revision, user can use BIOS recovery mode for BIOS downgrade.
8. System will prevent downgrading ME from 04.00.04.288 to 04.00.04.235 or older version, if system BIOS version is R0009. This is an expected behavior.
9. Security revision upgrade to 0005 on BIOS R0010 will prevent BIOS downgrade via normal mode to previous version that with lower security revision, user can use BIOS recovery mode for BIOS downgrade.
10. Security revision upgrade to 0006 on BIOS R0014 will prevent BIOS downgrade via normal mode to previous version that with lower security revision, user can use BIOS recovery mode for BIOS downgrade.
11. R02.01.0009 added KCS Policy Control feature, must combine with BMC which version is equal to or greater than 2.22.59c3b83a. 
12. Starting from BIOS R02.01.0009, when KCS Policy Control Mode is configured as "Deny ALL" on BMC EWS, BIOS cannot be upgraded/downgraded as expected behavior.
13. Due to integrate FPKSI v4.10 into R02.01.0010, need offline flash BIOS binary or use LanConf/nvmupdate to online update the NVM image.         
================================================================================
                                                      KNOWN ISSUES/WORKAROUND
================================================================================
1. [2103629100] When Flash FSUP from R008 with AEP configure, the system will hang at POST code 32 if reboot system after complete FSUP flash script (only happen 1st time reboot).
   Workaround: After FSUP update successfully, do a power cycle using command “Syscfg /gpc” or “Ipmitool –H xxxxxx –U xxxx –P xxxxxx –I lanplus raw 0x30 0x53”
2. [2103636701] Intel Server system S2600SP The help notes for enable complex password is incorrect in the BIOS setup when set password complexity to "Medium" or "High" in EWS
3. 
================================================================================
                                            
                                                       CHANGE LIST
================================================================================	
                                                        02.01.0013
================================================================================
[Non-HSD]-[Fixed] SKX6S. Using a Mix of Vendors' 2666 MHz DDR4 DIMMs May Cause Correctable Errors or a System Hang
RP release Reference code version: CP_PURLEY_0602_D02.
[Hsd-ES]:[14012848534] PurleyPlatPkg/MeUpdate: Remove Do/While Wait Loop after ME Update
[Hsd-ES]:[22011661315] PurleyPcPkg/PlatformSetupVariableSyncLib: Leaky bucket interval not triggering when expected
[Hsd-ES]:[1508438639] Type 190 offset 05h(slot number) show incorrect value 00 with add-in NIC card installed
[Hsd-ES]:[2103635658] After trigger invalid Intel Optane(TM) DC Persistent Memory Configuration Dimm configuration error, all boot entries are bootable when press F6 to Boot Manager
[Hsd-ES]:[2103635506] There is no "Intel Optane(TM) DC Persistent Memory Configuration" option when enter BIOS setup screen
[Hsd-ES]:[1508450103] PurleyPcPkg/Platform: Message "Intel (R) Optane(TM) PMem invalid Configuration f" will show during post screen with invalid config
[Hsd-ES]:[1508380589] PurleyPlatPkg/Library: Official Intel Optane(TM) DC Persistent Memory Configuration branding naming and usage update
[Hsd-ES]:[2103636919] the host interface will auto enabled after press F10 to save in BIOS setup
[Hsd-ES]:[2103636916] boot in BIOS setup->server management->BMC LAN Configuration will pop a warning messages when disable host interface in EWS
[Hsd-ES]:[1508380589] change the name "DCPMM" Update to "Intel(R) Optane(TM) PMem".(Main->memory configuration; Advanced->memory Configuration->DIMM information)
[Hsd-ES]:[CCB3178] - Enable Advanced MemTest
		Adavnced->memory Configuration->MemTest->Auto/Disabled/Enabled, Auto is defalut setting;
	     	Adavnced->memory Configuration->MemTest Loops, 1 is defalut setting;
		 Adavnced->memory Configuration->Adv MemTest Options, 0 is defalut settings;
		 Adavnced->memory Configuration->Adv MemTest Reset Failure Tracking List ->Disabled/Enabled.Disabled is defalut settings;
		 Adavnced->memory Configuration->Adv MemTest Conditions->Disabled/Auto/Manual. Auto is default settings)
[Hsd-ES]:[CCB3158] Integrate BMC features developed by InSyde,add below settings at BIOS setting UI
         	(Server Management->BMC LAN Configuration->HI BMC LAN configuration
		 Server Management->BMC LAN Configuration->HI Host LAN configuration)
[Hsd-ES]:[1508332492]  change System time default value from 2015/01/01 to 2020/01/01(main->System Data)
[Hsd-ES]:[1508383190] CpPcPlatPkg/SmiVariable: Memory overlap in VariableInterface SMI
[Hsd-ES]:[CCB3275] Enable NIC 190 and Storage(NVMe) 194 SMBIOS Table
[Hsd-ES]:[1507934020] Hide BMC and SDR version info under KCS Deny All mode
[Hsd-ES]:[1508375971] PurleyPcPkg/BuildImage.bat: (Patch 2)CAPSULE_ME.cap and CAPSULE_FD.cap are not available for IP Clean Build after IPU2020.2 Integration
[Hsd-ES]:[NA] PurleyPCPkg/StitchingPkg: Sync the RSTE drivers and VMDVROC version to v6.3.0.1005
[Hsd-ES]:[NA] PurleyPCPkg/StitchingPkg: Integrate Microcode 02006a08 for 1st Generation Intel(R) Xeon(R) Scalable H0
[Hsd-ES]:[NA] PurleyPCPkg/StitchingPkg: Integrate Microcode 05003003 for 2nd Generation Intel(R) Xeon(R) Scalable B1
[Hsd-ES]:[NA] PurleyPCPkg/StitchingPkg: Integrate SPS E5_04_01_04_423_0 to Trunk
[Hsd-ES]:[NA] PurleyPCPkg/StitchingPkg: Integrate Microcode 04003003 for 2nd Generation Intel(R) Xeon(R) Scalable B0
[Hsd-ES]:[NA] PurleyPCPkg/StitchingPkg: Integrate IntelDCPersistentMemoryDriver v01.00.00.3506 to Trunk
[Hsd-ES]:[NA] PurleyPCPkg/StitchingPkg: Integrate SINIT 1.7.49 PW
[Hsd-ES]:[NA] PurleyPCPkg/StitchingPkg: Integrate ACM 1.7.41 PW to purley trunk
[Hsd-ES]:[2103633362] PurleySktPkg/Include: Fix Build Error Caused by HSD 2103633362 (WHEA ID # 47/23 and Correctable error show when inject uncorrectable non-fatal error via wheahct)
[Hsd-ES]:[5388637] PurleySktPkg\ProcMemInit: Fixed Memtest issues with NVDIMM-N restore flow
[Hsd-ES]:[5388638] PurleySktPkg\ProcMemInit: Added Refresh Watermarks control to Memtest step
[Hsd-ES]:[5388628, 1508197968] PurleySktPkg/MemRas: ADC first strike meet ECC +1 with 1DPC 1RX4
[Hsd-ES]:[1508244875] PurleySktPkg/ProcMemErrReporting: Continuously Inject second strike CE directly cause RankVLS(reverse), and cause cor_err_cnt beyond threshold.
[Hsd-ES]:[14012345009] PurleySktPkg/MemDecode: SUT cannot boot into OS after enable "Mirror TAD0".
[Hsd-ES]:[18012748461] [ME] Platform code should not verify HECI interface
[Hsd-ES]:[5388371] FW-UEFI-Vuln-2019-132 Unsecure write to SMRAM because of missing buffer validation
[Hsd-ES]:[5388631] PurleySktPkg/ProcMemInit: PPR flow is triggered for several failing rows within the failed Rank0
[Hsd-ES]:[5388626, 14012151686, 1508197968] [RAS]: mSystemMemoryMap->Socket[Socket].ChannelInfo is still  pointing to boot time memory and  used in runtime code
[Hsd-ES]:[5388607] PurleySktPkg\ProcMemInit: Updated Advanced Memtest vendor content
[Hsd-ES]:[5388625] CpRcPkg/AdvMemTestLib: [AdvMemTest] Rank1 shows all DQs got failures in MemTestScram retry path
[Hsd-ES]:[5388624] CpRcPkg/AdvMemTestLib: [AdvMemTest] System reboot unexpectedly upon "N1: UpdateRowFailures: New failure occured in previously masked range"
[Hsd-ES]:[5388623] IPU 2020.2 PIV_IPU_PatrolScrubDowngrade_Enable_Logging_Signaling_UCE_EMCAGen1_L - UCE error is injected by CScripts but is no logged in Serial output or OS either
[Hsd-ES]:[5388449] ProcMemInit/Chip: UCE in ADDDC due to incorrect sparing of unmapped DRAM memory.
[Hsd-ES]:[5388621] CpRcPkg/AdvMemTestLib: CpRcPkg/AdvMemTestLib: Bug Fixes for AdvMemtest
[Hsd-ES]:[5388525, 5388620, 1508101191, 1508188532, 1508129395] 1st Generation Intel(R) Xeon(R) Scalable[RAS] Tc3b met SMI dead lock issue after strike 3 to overflow with ADDDC enable and SDDC plus one disable.
[Hsd-ES]:[5388617] PurleySktPkg/ProcMemInit: [CMD Vref TF] Skip MA 13,14, 15, 16 for DDRT DIMMs only in 2DPC config in the late cmd clock and skip teh same in RMT
[Hsd-ES]:[5388608] PurleySktPkg/Library/ProcMemInit/Chip/Mem: 3rd Generation Intel(R) Xeon(R) Scalable BIOS incorrectly logs WDB flush failed on cold reset
[Hsd-ES]:[5388604] AdvacentMemTest row failure bit 18 being reported as part of C[2:0]
[Hsd-ES]:[5388601]CpRcPkg/AdvMemTestLib: Restore refresh after MemTest
[Hsd-ES]:[5388592] CpRcPkg\AdvMemTestLib: Resolved Advanced Memtest failure in TestType 16 after PPR repair and retry
[Hsd-ES]:[5388587] SDC on running CAP+ Memicals
[Hsd-ES]:[5388431] CpRcPkg\AdvMemTestLib: Added Advanced Memtest support for DRAM vendor-specific algorithms
[Hsd-ES]:[5388492] [RAS] : Change the BIOS help text for Patrol Scrub knob
[Hsd-ES]:[5388583] Basetool: Fix GCC build Target failures in PreFl
[Hsd-ES]:[5388533,5388548,5388529,5388528,5388527,5388514,5388532] [RAS] SMI generation being disabled during ADDDC spare copy..
[Hsd-ES]:[5388577] ServerPlatformPkg/TPM: add platform hierarchy configuration
[Hsd-ES]:[5388552] PurleyPlatPkg/WheaErrorInj: Patrol Scrub APEI EINJ memory-uncorrectable-non-fatal (0x10) and TRIGGER=1 fails to work with serial printing disabled (ordering/delay related issues)
[Hsd-ES]:[5388573] Restore "Bank XOR" setup option to prevent memory bandwidth degradation in Linux.
[Hsd-ES]:[5388575] unsafe shutdown being logged by Intel Optane(TM) DC Persistent Memory Configuration when a warm reboot is followed be a cold boot initiated by mrc error handling
[Hsd-ES]:[5388545]] ServerSiliconPkg/MemTurnaroundTimingLib: Rank Switch Fix: Equation Check for DDR-T Turnarounds
[Hsd-ES]:[5388557] [RAS] Add BIOS setup opton to enable/disable patrolscrub UC downgrade signaling to Corrected
[Hsd-ES]:[5388574] PurleyPlatPkg: Rank Switch Configuration : Set Default to RCVEN_AVE
[Hsd-ES]:[538855] [RAS] Remove the patrol scrub option added to pc package header files.
[Hsd-ES]:[5388570] PurleyPlatPkg: Rename Rank Switch setup knob
[Hsd-ES]:[5388569] Purley/PurleyRpPkg: Update PurleyR IPClean tools in release folder per BDBA analysis (Phase 3)
[Hsd-ES]:[5388566] [RAS] UCE Error detected by patrol scrub is should be logged as uncorrected error
[Hsd-ES]:[5388567] Resolve microcode revision checking issue in BIOS
[Hsd-ES]:[5388522] Patrol Scrubber needs to be turned OFF with ADR flow (CCB follow up)
[Hsd-ES]:[5388555] Intel Optane(TM) DC Persistent Memory Configuration Media error caused by illegal access issue
[Hsd-ES]:[5388554] PurleySktPkg/MemDecode: Wrong TAD programming when rank 0 is disabled.
[Hsd-ES]:[5388484] ServerCommonPkg/LogoLib: FW-UEFI-Vuln-2019-179 Use of unsafe deprecated function ConvertBmpToGopBlt
[Hsd-ES]:[5388395]CLONE from skylake_server: Intel Optane(TM) DC Persistent Memory Configuration - Define 1018 namespaces leads to reboot loop"
[Hsd-ES]:[5388486] Package/Module:FW-UEFI-Vuln-2019-183 SMM accessing memory outside of SMRAM and not validating the memory
[Hsd-ES]:[5388407] Package/Module: Update PurleyR IPClean tools in release folder
[Hsd-ES]:[14010619471,5388537] PurleyPlaPkg: add TXT event log
[Hsd-ES]:[5388546] Rank Switch Fix: Rcven Ave part2 performance issue when RMT enabled
[Hsd-ES]:[5388485] Package/Module: Out of Bounds memory writes
[Hsd-ES]:[5388544] PurleySktPkg\ProcMemInit: Added "Refresh Watermarks" option for Row Hammer migation
[Hsd-ES]:[5388539] Linux cannot load acpi-frequency driver when X2APIC and VT-d are enabled
[Hsd-ES]:[5388534] PurleyPlatPkg/ProcessorErrorHandler: IPU [SKXH0 602.D02] UCE Error detected by patrol scrub is logged as corrected error(Expectation: Signaling as CE while logging as UCE)
[Hsd-ES]:[5388489]PurleyPlatPkg/Me: ME BIOS: Unable to Retrieve Hardware Information
[Hsd-ES]:[5388440] bios changes required for purley/purleyr to enhance p2p perf
[Hsd-ES]:[5388520] PurleySktPkg/Dxe/CrystalRidge: Fixing potential security issue with
[Hsd-ES]:[5388492] [RAS] : Revise BIOS knob PatrolScrub: Enable. Disable, Enable at End Of POST
[Hsd-ES]:[5388535] CpRcPkg\BaseMemoryCoreLib: Added MRC improvements to the "Rank Switch Fix"
[Hsd-ES]:[5388525] [RAS]:DXE Assert when per-rank CECC counters artificially set to threshold
[Hsd-ES]:[5388531] PurleyPlatPkg/OemProcMemInitLib: Missing NFIT type 6 (Flush Hint Address) table for Intel Optane(TM) DC Persistent Memory Configuration DIMM
[Hsd-ES]:[5388515] CpRcPkg\BaseMemoryCoreLib: Added MRC options for "Rank Switch Fix"
[Hsd-ES]:[5388513] PurleySktPkg/ProcMemErrReporting: For the UCE PPR log, fix the code for incorrect Rank when the Dimm is on slot1
[Hsd-ES]:[5388501] CpRcPkg\AdvMemTestLib: Fixed false failures and hang conditions in Advanced Memtest
[Hsd-ES]:[5388473] kernel panic observed when executing DCU test with eMCA Gen2 enabled
[Hsd-ES]:[2103633735] PurleyPcPkg/Ipmi/GenericIpmi: In BMC force update mode,the KCS mode of the BIOS setup still show allow all mode in the restricted/deny all mode
[Hsd-ES]:[22011363805] CpPcRestrictedPkg\Include: ADDDC threshold, when set to 500d (1F4h), is triggering after 244d (F4h)
[Hsd-ES]:[1508195797] PurleyPcPkg/SmbiosDataUpdateDxe: Type 190 NIC Firmware version is incorrect
[Hsd-ES]:[CCB3141] Some BIOS settings, when modified by ITK, don't take effect until the user manually intervenes
[Hsd-ES]:[1508203382]  PurleyPcPkg/Uba/UbaMain: SMBIOS type 41 video device bus number is incorrect
[Hsd-ES]:[2103633770] CpPcRestrictedPkg/SetupBmcCfg: Pop up warning message when user password cannnot meet complex requirements
[Hsd-ES]:[2103633158] PurleyPcPkg/Uba: STP PCIE Retimer NVME SSD can NOT be detected correctly after AC off/on cycle
[Hsd-ES]:[2103634038] PurleyPlatPkg/XmlCliRestricted/XmlCliCommon: BIOS Setup-->Main page has setting “POST errors Pause” but EWS BIOS Configurations Main page do not have it
[Hsd-ES]:[2103633809] CpPcRestrictedPkg/Library/CommonSetupLib/: "<"and">"symbol display as"?"in EWS->BIOS Configurations->Integrated IO Configuration.
[Hsd-ES]:[CCB3157] Memory SMBIOS record Asset Tag to show memory manufacturer date from SPD
[Hsd-ES]:[1508192389] PurleyPcPkg/Uba/UbaMain: SMBIOS type 8 internal reference designator string of RAID KEY mismatch with the motherboard
[Hsd-ES]:[1508192256]  PurleyPcPkg/Uba/UbaMain: SMBIOS type 8 internal reference designator string of M2 PCIE sSATA ports mismatch with the motherboard
[Hsd-ES]:[2103626923] PurleyPcPkg/Uba: Fix SMBIOS type9 “Current Usage” information is incorrect when only one CPU connect.

================================================================================
                                    02.01.0012
================================================================================
Rename BIOS ID from 0X.02.0256 to R02.01.0012
HSD-ES: 2207406475 Intel Server System S2600WF Vulnerable SMI handler UsbRt pointed to HwSmiHandler
HSD-ES: [NA] Integrate Microcode 02006906 for 1st Generation Intel(R) Xeon(R) Scalable H0
HSD-ES: [NA] Integrate Microcode 05002f01 for 2nd Generation Intel(R) Xeon(R) Scalable B1
HSD-ES: [NA] Integrate Microcode 04002f01 for 2nd Generation Intel(R) Xeon(R) Scalable B0
HSD-ES: 1507959901 Change Mailbox register to SIO scratch pad register 0x20
HSD-ES: CCB3115 Change the default vaule of NVM Performance Setting
HSD-ES: 1507879137 CCB3027 Enable PPR Type in BIOS setup knobs
HSD-ES: [NA] Integrate SPS E5_04_01_04_381_0 to Trunk
HSD-ES: CCB3015 Add PCIe port option ROM control in UEFI mode.
HSD-ES: 2103630638 Handling au-reboot after injecting 2nd ADDDC error for standard RAS
Merge remote-tracking branch 'remotes/origin/PurleyRefresh_PC_20Q2_QSBR' into Purley-R_DSG_BIOS_Production_Trunk
Hsd-ES: 1507892509 Update BIOS OOB update&config SEL
HSD-ES: 1507864848 Replace BIOS RAID Option "Intel(R) RSTe" to "Intel VROC" for sSATA
HSD-ES: 1507927108 Update SMBIOS Type 17 AssetTag on S2600WF.
HSD-ES: [NA] Integrate Microcode 04002f00 for 2nd Generation Intel(R) Xeon(R) Scalable B0
HSD-ES: 2103630333 Modified the EWS BIOS configuration "Reset Static Boot Order" value from 0x0 to 0x1 will cause SUT reboot continuously
HSD-ES: 1507924351 Fix incorrect processor info in setup.
HSD-ES: [NA] Sync the RSTE drivers and VMDVROC version to v6.2.0.1034
HSD-ES: [NA] Integrate SINIT 1.7.48 PW
HSD-ES: [NA] Integrate SPS E5_04_01_04_381_0 to Trunk
HSD-ES: [NA] Integrate Microcode 05002f00 for 2nd Generation Intel(R) Xeon(R) Scalable B1
HSD-ES: 1507659391 Fix to SMBIOS Type 197 offset 6 and offset 7
HSD-ES: 1507894757 Some knobs still can be modify and some Sub_Menu knobs can't be read with user password entering
HSD-ES: [NA] Integrate Microcode 02006901 for 1st Generation Intel(R) Xeon(R) Scalable H0
HSD-ES: [NA] Integrate IntelDCPersistentMemoryDriver v01.00.00.3497 to Trunk
HSD-ES: [NA] Integrate ACM 1.7.40 PW to purley trunk
HSD-ES: 2103630341 The Multi-Rank Sparing value of EWS is not match with BIOS setup menu.
HSD-ES: 5388518 Fix CMOS Corruption
HSD-ES: 5388517 SYSTEM_CONFIGURATION structure MUST NOT have changes in the middle of the structure
HSD-ES: 5388476 Request to add new profile for 2LM performance improvement
HSD-ES: 5388463 Fixed incorrect bank address reported by Advanced Memtest
HSD-ES: 5388474 Fatal event (PCC=1) with eMCA Gen2 enable causes the system to not boot
HSD-ES: 5388088 3rd Generation Intel(R) Xeon(R) Scalable code enabling in IP clean tree
HSD-ES: 5388498 Fixed Soft PPR flow
HSD-ES: 5388490 The MBP buffers must be cleared before exiting functions
HSD-ES: 5388493 ME Corrected the media table length
HSD-ES: 5388487 Need Panic and Watermark change setup option for MRC
HSD-ES: 5388458 ADDDC SMI handler's writes to non-32 bit aligned registers failing on 2nd Generation Intel(R) Xeon(R) Scalable"
HSD-ES: 5388429 CE and UC Error Injection Shows Wrong DIMM Location in AD-WB or 2LM Provisioning
HSD-ES: 5388482 Fix Surprise reset and Multi Socket Bug
HSD-ES: 5388488 Fixed Memtest failures during the PPR flow
HSD-ES: 5388472 2nd Generation Intel(R) Xeon(R) Scalable BIOS sets nonfailed_cs to non-existent rank in 3-rank config
HSD-ES: 5388483 Enabled the DDR scrambler prior to Legacy Memtest
HSD-ES: 5388470 Remove the TRFC1_VAL tRFC override for SPD_16Gb DIMMs introduced by sighting 5387664
HSD-ES: 5388479 PBF should not affect HWPInterrupt and EPPEnable settings
HSD-ES: 5355343 UCE in ADDDC due to incorrect sparing of unmapped DRAM memory.
HSD-ES: 5388454 prevent nested machine check, demote P.S UC to signal corrected
HSD-ES: 5388456 IO resource overlap between PNP0C02 and IPI0001 devices
HSD-ES: 5388467,5388468 Update PPR RAS code to fix the DRAM Mask reporting for x8 DIMMS and also reporting multiple entries for same address
HSD-ES: 5388443 CPU SystemSemaphore0 Will Not Release Semaphore And Appears Stuck
HSD-ES: 5388471 Added Receive Enable Average feature
HSD-ES: 5388441 AppDirect in CPU SKU memory cap exceeded boots with Non-Functional DCPMMs
HSD-ES: 5388464 [RAS] EINJ code is causing to have SDC under mirror mode
HSD-ES: 5388435 Fixed TOC/TOU vulnerability
HSD-ES: 5388452  Fixed Advanced Memtest failure where DQ mask is all 0xFFs
HSD-ES: 5388399 Extend the Direct Update Flow (HMRFPO) to support partial Update via SMI handler
HSD-ES: 5388390 ME Update system reset when using OFU build 14.1 Build 21 with WW18 BKC
HSD-ES: 2103626444 SUT will reset after udpate BIOS/FD/ME via OFU in Linux
HSD-ES: 5388459 DCPMM-64GB SKU - fail to boot in AD mode (2-2-2)
HSD-ES: 5388457 illegal access error seen when upgrading from BKC16 to 26 @ DPA 0x1040
HSD-ES: 5388430 [DCPMM] [AD/WB] NM UC error causes AD-WB NM flush hang
HSD-ES: 5388455 RCVEN training result offset
HSD-ES: 5388451 Bug fixes for Advanced Memtest with PPR
HSD-ES: 5388428 update for memory corruption below 1MB on S3 resume
HSD-ES: 5388444 Add CTLE functionality for Nanya DRAM based DIMMS
HSD-ES: 5388438 Fix CE PPR Error flow
HSD-ES: 5388391 Added Advanced Memtest feature with Post Package Repair
HSD-ES: 5388439 ServerSiliconPkg/PeiPchIinitLib Incorrect Flexible IO Adapter (FIA) used to map Pcie port clocking
HSD-ES: 5388396 Added memory RAS support for UCE->PPR flow
================================================================================
                                  02.01.0011
================================================================================
Rename BIOS ID from 0X.02.0225 to R02.01.0011
HSD-ES: NA, Fix ISS sync between BIOS and BMC
HSD-ES: 1507819944, Fix password mismatched bug
HSD-ES: 14010920676, RAID module RMS3HC080 and Software RAID RSTe can't work together in legacy mode
HSD-ES: 16010688351, Replace BIOS RAID Option "Intel(R) RSTe" to "Intel VROC"
HSD-ES: 2103626900, Fix incorrect behavior after injecting PCIe CE/UCE on Port C
HSD-ES: 1507176793, Hardware P States disable function invalid when set "Hardware P States disable +Active PBF enable" in BIOS.
HSD-ES: 1507588040, Fix Incorrect RMRR of Raid Card (RMS3HC080) in DMAR
HSD-ES: 1507243669, Fix Incorrect Console Redirection Display of 100*31
HSD-ES: 2103626914, Add 3 invalid DCPMM config and change "promotewarning" to false by default.
HSD-ES: NA, Fix PC IssCapable cannot be changed back to 0
HSD-ES: Change copyright to 2020.

================================================================================
                                  02.01.0010
================================================================================
Renamed BIOS ID from 0X.02.0141 to R02.01.0010
HSD-ES: NA, PCPkg/StitchingPkg: Integrate Fpksi v4.10_80001A7A_WFT_WFS/v4.10_80001A76_BNP/v4.10_80001A78_STP/v4.10_80001A79_WFQ_WFO.
RP relese Reference code version: CP_PURLEY_0596_D08.                                                      
HSD-ES: 1507430586, CCB#2762 SMBIOS region shall include additional structure (type 210) for Intel Speed Select Configuration.
HSD-ES: HSD-ES Fix incorrect PCIe Slot Number in SMBIOS type 192
HSD-ES: 1609246698, Change "Enforced Password Support" to disable after clearing admin PWD
HSD-ES: 1507430586, Adjust some information of SMBIOS Type210.
HSD-ES: 1507492512, CCB#2707: Customer ask for a way/tool to change SMBIOS Type0- BIOS Vendor String from Intel to customer's
HSD-ES: 2103627193, Some of SMBIOS T197 info is incorrect.
HSD-ES: 2103626917, Fix incorrect port index in SMBIOS type 190
HSD-ES: 1507520209, Fixed incorrect description of "AtomicOp Egress Blocked Mask"
HSD-ES: 2103626884, FRB2 triggered on the early video phase.
HSD-ES: 2103629389, Send BIOS ID to BMC in RSD module
HSD-ES: 2103629034, Fix ISS cannot be changed in BIOS setup in "DenyAll Mode"
HSD-ES: 5388392, System hangs when injecting poison when in ADWB.
HSD-ES: 5388403, S3 DDRT ERID/Rd error during S3 resume.
HSD-ES: 5388406, S3 AEP Dimms & other devices get reset during S3 resume.
HSD-ES: 5388405, S3 Hang with CatErr - DDR4 UNC / Petrol scrub unc during S3 transition restoration.
HSD-ES: FIV1187, PCPkg/StitchingPkg:Integrate Intel DC Persistent Memory Driver v01.00.00.3475 to Trunk.
HSD-ES: NA PCPkg/StitchingPkg: Integrate SPS E5_04_01_04_339_0 to Trunk.
HSD-ES: 5388394, Combo RC failing to training LRDIMMs.
HSD-ES: 5388416, [Power Management] BIOS knob "TCC Activation Offset" Not Functional.
HSD-ES: 5388413, TxLRDIMMDqCentering should only run for 2933 and above.
HSD-ES: 5388414, TrainDramRxEq and ModifiedTrainCTLE need to run for 2933 and above only.
HSD-ES: 5388377, MCA recovery reports wrong failed DIMM location on FC29.
HSD-ES: 5388420, CK Stop exit potentially can cause DRAM read ECC errors with IDT Gen 2.5 C2 Data Buffer.
HSD-ES: 5388384, SktPkg Override CpuMpDxe: Make PpinCtl feature to follow the flow.
HSD-ES: NA, PcPkg/RasPkg: Report MEM UCE inside MESEG region.
HSD-ES: NA, PCPkg/StitchingPkg: Integrate Microcode 02000065 for 1st Generation Intel(R) Xeon(R) Scalable H0.
HSD-ES: NA, PcPkg/Uba: When OCP card is installed, there are two type41 records for 000:3d:00.0.
HSD-ES: NA, PCPkg/StitchingPkg: Integrate Microcode 0400002c for 2nd Generation Intel(R) Xeon(R) Scalable B0.
HSD-ES: NA, PCPkg/StitchingPkg: Integrate Microcode 0500002c for 2nd Generation Intel(R) Xeon(R) Scalable B1.
HSD-ES: 5388272, Package/Module: Update for new ucode.
HSD-ES: 1507473345, PlatPkg/Rsa: Skip adding SMBIOS type 210 when ISS is not supported.
HSD-ES: NA, PCPkg/StitchingPkg: Integrate ACM 1.7.32 PW to trunk.
HSD-ES: NA, PCPkg/StitchingPkg: Integrate SINIT 1.7.45 PW.
HSD-ES: NA, PCPkg/StitchingPkg: Integrate SPS E5_04_01_04_339_0 to Trunk.
================================================================================
                                   02.01.0009
================================================================================
HSD-ES: 2103626250, SUT will hang on black screen when use NVMe SSD then install windows chipset driver
HSD-ES: 5388345, 6 sec time window from MB3 (EKV entering normal mode) to iMC entering normal mode - SCS
HSD-ES: CCB2763, [BIOS/BMC Q3'19] Single reboot to update BIOS, FD, ME & BMC: Current design requries 3 reboots to update FD,  BIOS and ME. 
HSD-ES: 5388220, CCB 136637 OS Mgmt: Intel(R) Optane(TM) DC Persistent Memory fallback to SMBus when DDRT training fails to allow log collection & firmware upgrade
HSD-ES: 5388361, CCB 136533 Intel(R) Optane(TM) DC Persistent Memory SW RAS: BIOS Driven "BACKGROUND" ARS thread - critical for proper Windows/Azure error handling behavior (phase 2)
HSD-ES: 5388220, CCB 136637 OS Mgmt: Intel(R) Optane(TM) DC Persistent Memory fallback to SMBus when DDRT training fails to allow log collection & firmware upgrade
HSD-ES: 5388223, CCB 136654 Clear PCD0 corruption without overwrite DIMM
HSD-ES: 5388342, MCA Recovery Test Issue with 6133 CPU
HSD-ES: 5387495, CCB 136533 Intel(R) Optane(TM) DC Persistent Memory SW RAS: BIOS Driven "BACKGROUND" ARS thread - critical for proper Windows/Azure error handling behavior
HSD-ES: 5388325, Short ARS - Allows errors to be returned even user requested no notification.
HSD-ES: 5388097, Save S3 boot script for IOAPIC   There was an issue with missing some PCIE graphic cards after S3 resume.
HSD-ES: 2103626817, The KTI Prefetch item help text is different BIOS spec. The prefetch letter p in KTI prefetch should be capitalized.
HSD-ES: 5388323, User CAPS State for WS in support of CCB 136665
HSD-ES: 5388342, IRPPERRSV CSR maps protocol parity errors to correctable
HSD-ES: 5388338, CLX64L - Enabling CLTT w/PECI results in both CLTT mode and CLTT w/PECI
HSD-ES: 5388350, [IPS 1409117089][AMI] x2APIc broken
HSD-ES: 5388309, Platform\DxeSmm\BiosGuard: Vuln-2019-012 -- Unregister IO trap once triggered
HSD-ES: 5388326, Incorrect DIMM location reported when disabling CMCI-SMI Morphing in 2LM
HSD-ES: 5388356, PCU machine check (MSCOD = 0x68) observed when memory channel fails to train
HSD-ES: 5388337, Against the DIMM rule with 2DPC RDIMM (SR is in DIMM0, DR is in DIMM 1), this channel will be disabled as design, but the system will hang when booting Windows server 2012 R2
HSD-ES: 5388340, Need final resolution for FW-UEFI-Vuln-2019-012 BIOSGuard issue
HSD-ES: 5388389, [2nd Generation Intel(R) Xeon(R) Processor Scalable family] SST-BF Frequency Table in BIOS needs minor adjustment 
HSD-ES: 5388264, Add software timeout and issue cold reset
HSD-ES: 5388324, Intel(R) Optane(TM) DC Persistent Memory BIOS - ARS Error Inject updates
HSD-ES: 1507355635, CpPcRestrictedPkg/Ipmi: User configuration page is  hidden  after setting BMC KCS to Restricted Mode
HSD-ES: 5388313, Intel(R) Optane(TM) DC Persistent Memory DIMM's showing ECR_WDATA_PE (data path poisoned) without error media log created (or WDB UE)
HSD-ES: 5388339, Firmware Test Suite failures with NVDIMM _NBS & _NCH methods
HSD-ES: 1507354875, OOB update caused system be in reboot loop under restricted/Deny all mode
HSD-ES: 1607594883, FRB-2 triggered on option ROMS under Deny All mode.
HSD-ES: 1507337951, Released BIOS bug with Intel(R) Optane(TM) DC Persistent Memory in description instead of Optane DCPMM.
HSD-ES: 1407979768, BMC KCS Policy Control Modes Implementation.
HSD-ES: 1806951266, XmlCliDxe Assert on reboot after creating max number of namespaces in UEFI CLI.
HSD-ES: FIV10506, PC Stitching Update RSTeSataLeagcy version to 6.1.0.1017 for RP
HSD-ES: OSS_0011668, OSS_0011668_Integrate SPS E5_04_01_04_323_0 to Trunk
HSD-ES: 2103627012, "Password is set successfully" message show up when press "F10" to save the config after create BMC user account.
HSD-ES: 2103625822, Revert"Intel(R) Optane(TM) DC Persistent Memory 55785.1 -  Invalid Configuration - Mixed NVDIMMs and DCPMMs, Step2 - Intermittent POST 0x32 hang and IERR logging."
HSD-ES: 1607211313, Race conditions in VariableInterface() allow arbitrary writes inside of SMRAM
HSD-ES: 2103626532, Complex Password setting will change to default setting (disable) after reset SUT
HSD-ES: 1507212924, Onboard VGA Always On knob is grey out and display output from add-in video card
HSD-ES: 1507223712, "DCPMM Invalid Configuration found" after running UEFI NVRAM variables without any DCPMM installed.
HSD-ES: 1507140808, Vulnberabilities CVE-2019-6260 as BMC didn't disable superIO
HSD-ES: 2103626444, SUT will reset after udpate BIOS/FD/ME via OFU in Linux
HSD-ES: 2103626509, System cannot boot to recovery mode with some memory population
HSD-ES: 2103626021, SUT will halt at 0x99 probably when Intel(R) Optane(TM) DC Persistent Memory set to 2LM MM mode
HSD-ES: 1507136963, S2600WFR FRUSDR/SYSCFG utility stall for quite a long time when dumping FRU content or bios/bmc setting under uefishell with USB31000SA installed.
HSD-ES: 1607277367, Operands in a bitwise operation have different size KW issue
HSD-ES: 2103626208, It can enroll CA cert via Setup UI after login as user.
HSD-ES: 1507072526, ServerAmiRestrictedPkg : FW-UEFI-Vuln-2019-009 UsbRt SMM callout code execution Server Board S2600ST
HSD-ES: 2103625317, [S2600STR]  RAID option ROM have no display background color and only display character in SOL session.
HSD-ES: 2103626238, Stop bits should be "0" according to new ACPI SPCR spec.
HSD-ES: 1507136963, [S2600WF0R] FRUSDR/SYSCFG utility stall for quite a long time when dumping FRU content or bios/bmc setting under uefishell with USB31000SA installed.
HSD-ES: 2103625234, There are some issue when SUT boot with invalid DCPMM config
HSD-ES: 1507036525, There are 7 PSIRT BIOS security issues reported on R15 code base.
HSD-ES: 1507173389, SMBIOS type 16/ type 19 show incorrent info.
HSD-ES: 1507175341, RSD Type 194 info is incorrect.
HSD-ES: 2007797829, BMC Web Console doesn't show CPU and DIMM information.
HSD-ES: 1507175309, RSD Type 193 info is incorrect
HSD-ES: 2103625822, [Intel(R) Optane(TM) DC Persistent Memory] 55785.1 - Invalid Configuration - Mixed NVDIMMs and DCPMMs, Step2 - Intermittent POST 0x32 hang and IERR logging.
HSD-ES: 2103624920, BIOS / ME / FD image still can be updated via OOB feature when the mismatch type is selected
HSD-ES: 2103626488, S2600BPR Configure out Intel(R) Optane(TM) DC Persistent Memory for CFG1 2-1-1(Intel(R) Optane(TM) DC Persistent Memory 256G x 4, and 128GB DIMM x12), appeared 0XFA fatal error after power on Fatal error is thrown when high memory is used with the SKU which does not supports.
HSD-ES: 11581, Integrate Microcode 03000012 for 2nd Generation Intel(R) Xeon(R) Processor Scalable family A0 from PC-1st Generation Intel(R) Xeon(R) Processor Scalable family
HSD-ES: 1507170024, [S2600WF] ipmi set bootdev bios/disk sometimes doesn't work
HSD-ES: 11544, PC Stitching Sync Intel(R) Optane(TM) DC Persistent Memory UEFI driver v01.00.00.3458 from RP
HSD-ES: 1607116940, Add BIOS options to change different PCIe Uncorrectable Error Severity mapping
HSD-ES: 1507072526, FW-UEFI-Vuln-2019-009 UsbRt SMM callout code execution Server Board S2600ST
HSD-ES: 1507146548, CCB#2591-Q2'19 To add [Onboard VGA Always On] to support GPGPU usage
HSD-ES: 1607184056, Resolve BMC network problem from LAN disabling under BIOS and MAC address problem
HSD-ES: 2103624263, S2600ST Q3'18 SFUP test failed with SUSE12.3 OS that show critical issue for ME in BMC web
HSD-ES: 1607202054, [2nd Generation Intel(R) Xeon(R) Processor Scalable family] SST-BF identification of High Priority cores broken in VMWare ESXi
HSD-ES: 2103626179, The SUT will halt at early video with some memory config.
HSD-ES: 2207272621, S2600WF: PCI device slot id is not unique
HSD-ES: no_sighting, Integrate microcode 2nd Generation Intel(R) Xeon(R) Processor Scalable family A0 mb750655_03000012 to Trunk
HSD-ES: 5388296, Incorrect DIMM location reported when PS finds UCE
HSD-ES: 5388329, [2nd Generation Intel(R) Xeon(R) Processor Scalable family] SST-BF identification of High Priority cores broken in VMWare ESXi
HSD-ES: 5388209, DXE_ASSERT - Protocol 'gEfiVariableWriteArchProtocolGuid' is not available
HSD-ES: 5347308, Post code hang d5 after enable BIOS Gard option in BIOS setup
HSD-ES: 5388298, [2nd Generation Intel(R) Xeon(R) Processor Scalable family] Dimm re-training and ADR enable results in loosing DIMM data
HSD-ES: 1607113667, CCB-2570-Complex BMC Password
HSD-ES: 1506985873, S2600BP BdsUpdateHook driver is loaded on S9200WK.
HSD-ES: 1607042642, IIO config help string override by SDP.
HSD-ES: 5388322, BIOS hangs at "Pipe Exit starting..." message during S3 flow in 2DPC system configuration  
HSD-ES: FIV11501, Integrate true version of NMPTU binary for SPS E5_04.01.04.296.0 to Trunk
HSD-ES: 1607085596, Restrict Update Nvram support for DC requirement
HSD-ES: 1607201873, Sync the Setup options value with respect to refresh and non-refresh project trunks
HSD-ES: 1507108474, BIOS post fail with S2600BPS SKU in Riser solt2 M.2 NVME
HSD-ES: 1607172379, CCB-2659: [Q2'19 BIOS]Support for Priority Based Frequency
HSD-ES: 11482&11483, Integrate Microcode 04000024 for 2nd Generation Intel(R) Xeon(R) Processor Scalable family B0 and 05000024 for 2nd Generation Intel(R) Xeon(R) Processor Scalable family B1
HSD-ES: 1507095678, On 1 CPU system SMBIOS type 9 Current Usage value for CPU 2 - PCIE slot don't follow SMBIOS SPEC.
HSD-ES:  2103625234, There are some issue when SUT boot with invalid DCPMM config
HSD-ES: 5388283, Dynamic loops accessing one element beyond boundary (MAX_TT_ROW) due to <= operator in DimmTT
HSD-ES: 5388046, [2nd Generation Intel(R) Xeon(R) Processor Scalable family] System getting stuck at postcode FF during AC cycling"
HSD-ES: 5388139, BMC version is changing to NA in bios setup menu after flashing IFWI/ loading any config file
HSD-ES: 5388153, When running MRC cycling with Intel(R) Optane(TM) DC Persistent Memory, each boot results in surprise clock stop.
HSD-ES: 5388031, BIOS hang at "Config TDP Level 2..." after enable "Opportunistic SR" with full memory configuration
HSD-ES: 5388222, [2nd Generation Intel(R) Xeon(R) Processor Scalable family] Speed Select Base Config P1 frequency is lost and not available to discover when CPU is in a different ISS config than base
HSD-ES: 5388195, MRC: Limit EKVCMD Vref high side boundary to 63
HSD-ES: 5388301, ASSERT_EFI_ERROR 451 while running MLC at high temp
HSD-ES: 5388286, [2nd Generation Intel(R) Xeon(R) Processor Scalable family B0] Add datecode check for CTLE for Samsung C-die and D-die
HSD-ES: 5388285, [2nd Generation Intel(R) Xeon(R) Processor Scalable family B0] Fatal error during DRAM Rx Eq training on Samsung 8Gb based DIMMs
HSD-ES: 5388261, SMBIOS Type 19 for UMA should expose LMMIO gap.
HSD-ES: 5388266, Intel BIOS Guard implementation IO TRAP SMI call-out
HSD-ES: 5388288, Surprise clock stop after S3 reset
HSD-ES: 5388239, DXE_ASSERT when flushing ADWB memory
HSD-ES: 5388281, Incorrect DIMM location reported in ADWB or 2LM when injecting CE or UCE
HSD-ES: 5388290, Fixed counter RDPMC failures
HSD-ES: 5388101, Add PPR
HSD-ES: 5388231, CPU string is not matched between BIOS and DCL SPEC
HSD-ES: 5388284, The current BIOS implemenation is not following the POR validation matrix
HSD-ES: 5388260, Intel MRC change broken customrefreshrate setting to 2x refresh.
HSD-ES: 5388217, Fix size check for ADDDC Ranks
HSD-ES: 5387999, Unnecessary HECI resets causing SPS failures
HSD-ES: 1606927743, to reduce the build time for PurleyPcPkg
HSD-ES: 5388108, [2nd Generation Intel(R) Xeon(R) Processor Scalable family AP] Observing Package cstate & Core cstate value of PKG-C1 to be greater than 90% instead of PKG-C6 values.
HSD-ES: 5388209, DXE_ASSERT - Protocol 'gEfiVariableWriteArchProtocolGuid' is not available
HSD-ES: 5388237, Intel(R) Optane(TM) DC Persistent Memory FIS version as part of input structure fed to 'Identify DIMM' Intel(R) Optane(TM) DC Persistent Memory command is wrong.
HSD-ES: 5388229, The starting/initial values for CLK signals seems exist problem on BIOS
HSD-ES: 5388274, Mixed Mode Intel(R) Optane(TM) DC Persistent Memory is not throwing out an unsupported warning message
HSD-ES: 5388271, PCD Error Handling - BIOS runs into infinite loop on invalid signature
HSD-ES: 5388254, LSS - All Intel(R) Optane(TM) DC Persistent Memorys Reports Dirty Shutdown After Same-Level BIOS Flash Following a Cold Reset
HSD-ES: 5388251, Implement workaround for CoreBo credit leak issue dropped from Intel(R) Xeon(R) Processor Scalable family code
HSD-ES: 5388178, BIOS don't follow FIS 1.14 to parsing BSR in serial debug msg
HSD-ES: 5388261, Fix for SMBIOS Type 19 missing if NUMA disabled
HSD-ES: 1507042968, Remove the lock feature of Power LED
HSD-ES: 5388198, L3 Cache Size  is incorrect in SMBIOS table type 7
HSD-ES: 5388190, [2nd Generation Intel(R) Xeon(R) Processor Scalable family - AP] Platform is not booting after changing the boot mode to power optimized in Bios setup menu.
HSD-ES: 5388252, DCPMM Protocol - do not switch to SMM for TSOD polling state retrieval
HSD-ES: 5388198, L3 Cache Size  is incorrect in SMBIOS table type 7
HSD-ES: 1507094928, Support RSD SMBIOS table 190 NIC
HSD-ES: 5388202, Update NvmCtlrGetPlatformInterpretedLss & NvmCtlrGetPlatformInterpretedUnlatchedDsc to return new dirty shutdown reasons from BSR
HSD-ES: 5388241, CCB 136659 Disable DDRT on 1st Generation Intel(R) Xeon(R) Processor Scalable family CPUs before Intel(R) Optane(TM) DC Persistent Memory goes to production
HSD-ES: 5388246, [2nd Generation Intel(R) Xeon(R) Processor Scalable family] CPC Error on windows after enabling Prioritized base frequency support
HSD-ES: 210362551, There is no "Direct To Core (D2C)"  and "Direct To UPI (D2K)" option on BIOS Setup.
HSD-ES: 5387873, SMBIOS Type 19/20 is not showing effective memory Size.
HSD-ES: 2007793994, BIOS displays 2934 MHz for Current memory Speed instead of 2933MHz.
HSD-ES: 1507073575, Patch 2 Die as One to get logic socket ID for 2nd Generation Intel(R) Xeon(R) Processor Scalable family AP
HSD-ES: 5388203, Intel(R) Optane(TM) DC Persistent Memory surprise warmreset detection does not work
HSD-ES: 5387983,[2nd Generation Intel(R) Xeon(R) Processor Scalable family AP] UEFI PXE Boot is not present in the DragonRock BIOS
HSD-ES: 5387156, Add support to report FRU information in Error Logs based on 2nd Generation Intel(R) Xeon(R) Processor Scalable family AP 2 dice in 1 Skt
HSD-ES: 5388125, BIOS BDAT crc incorrect
HSD-ES: 5388163, BIOS hangs during platform boot when get PCD for partition 0 (or 1) fails as a consequence of UCC (or poison)
HSD-ES: 5388216, RAS Clear Poison while ARS running
HSD-ES: 5388215, [2nd Generation Intel(R) Xeon(R) Processor Scalable family AP] Remove 2die as 1S Setup Option
HSD-ES: 1507099817, [S2600WF] BIOS does not have a memory setting for 2666 or 2933 memory 
RP relese Reference code version: CP_PURLEY_0581_D01.
This release is mapping to RP daily build:CP_PURLEY_0581_D05.
===============================================================================
                                R02.01.0008
================================================================================
Hsd-ES:1507112201, Default option for Resume on Power Loss changed to 'power on'
Hsd-ES:1607077352, Default option for Console Redirection changed to 'Serial Port A'
Disable "UpdateNvram" in BIOS so that UpdateNvram can't be used in flash utility like iflash32.
Hsd-ES:1507108474, BIOS post fail with S2600BPS SKU in Riser solt2 M.2 NVME
Hsd-ES:[no_sighting] OpenSSL version update to 1.1.0j.
Hsd-ES:2103625393, [S2600ST] TPM BitLocker (Boot order change) test result does NOT match expected result.
Remove [Hsd-ES]: 5387873, SMBIOS Type 19/20 is not showing effective memory Size.
RP relese Reference code version: CP_PURLEY_0573_D10.
This release is mapping to RP daily build:CP_PURLEY_0574_D07.
================================================================================
                                R00.01.0016
================================================================================
Rename BIOS ID from X0191 to R0016
HSD-ES:2103625314, The copyright should be Copyright (c) 2006-2019 instead of Copyright(c) 2006-2018.
HSD-ES:1506731732, [S2600BP][Q2] SEL error during AC cycling: IPMI Watchdog reports the watchdog initiated a hard reset. 
HSD-ES:2103624878, With AIC Card populated in RJ45 MB, return data “CB” when execute "Get AIC MAC address".
HSD-ES:2103624556, Setting IPv6 address will display unexpected messages after enable/disable it.
HSD-ES:1606884710, [Intel Xeon Scalable]System hang up when press F9/F10 to load BIOS default after delete ‘EM_Configuration’ value.
HSD-ES:1506131214, Q3'18 #CCB2343[Intel Xeon Scalable] Add BIOS options in ITK to change USB 2.0 ports equalization parameters.
HSD-ES:1504750181, SMBIOS type 9 segment group number should be all 0.
HSD-ES:2103624586, [S2600BP]OPROM and DOS screen cannot be redirected to remote terminal with CR 100x31 - Serial Port A Baud Rate 115.2K RTS-CTS mode.
HSD-ES:2103624653, SUT will halt on post code 0xD4 when injection MBE after reboot the system.
HSD-ES:1506980475, [server_bios][Intel Xeon Scalable]A coding error in IPMI KCS driver.
HSD-ES:2205485105, [PSAV] Flash illegal opcodes not Configured.
HSD-ES:1506766438, [OOB Firmware Update]OOB image update SEL sensor name and Description is unexpected while input wrong BIOS password.
HSD-ES:2103623988, [OOB BIOS CONFIGURATION]BIOS config cannot be updated via OOB method under Power on status.
HSD-ES:1506949739, [Intel Xeon Scalable][Add BIOS option [DMI-PCIe Port MPSWorkaround] to set PCIe max packet size to 128 bytes on DMI as PCIe slot port.
HSD-ES:1506875497, [Intel Xeon Scalable]System MAC address and IP is zero from Redfish.
HSD-ES:1506940429, Intel Xeon Scalable R15 BIOS CCB2343 port 12 implementation lacks of one ITK option [USB2.0 Per Port HS Transmitter Emphasis] compared to original CCB requirement. 
HSD-ES:1504750181, SMBIOS type 9 segment group number should be all 0.
HSD-ES:2103624203, Without AIC Card populated, return data contains onboard NIC info when execute  "Get AIC MAC address".
HSD-ES:1506861772, NVME UEFI driver should wait for  the correct timeout time as programmed in NVME card's timeout value from NVME spec.
HSD-ES:1504683590, Clone from HSD - Security VT - IIO UEFI FW shall delay PCI Bus Master Enable (PCICMD.BME) until end of POST to prevent DMA attacks on UEFI FW in RAM.
OSS_9231:[PC_Stitching]Integration for ME 4.0.4.393.0
HSD-ES:1506871190, syscfg /bldfs "" not working the same way an F9 in the BIOS setup does.
HSD-ES:2204077884, S2600WF server SUP R0013 hangs on first boot after memory configuration changed. 
HSD-ES:2103624158, OS CERT - Win2019- Check SMBIOS Table Specific Requirements test failed.
OSS_9371:[PC_Stitching]:Update RSTeSataEfi version to 5.5.0.1028
OSS_7213:Integration add Xeon Scalable B1 01000146
OSS_7215:Integration add Xeon Scalable H0 02000050
OSS_7021:Integration add BIOS ACM 1.3.9
OSS_7022:Integration add BIOS SINIT 1.3.6
HSD-ES:2103622487, 1st boot to DVD drive w/ ESXi6.7 disc will show "Boot failed" msg under uEFI mode.
HSD-ES:1504400810, Some information incomplete display at the bottom of BIOS setup main page by sol in linux.
HSD-ES:1505083118, Q2'18 #CCB2398 [Intel Xeon Scalable BIOS] Allow all SMBIOS extensions as defined by RSD extensions to be supported by default.
HSD-ES:1506657447, PC RAS - NMI was triggered for Memory uncorrectable error.
HSD-ES:2103623845, There are two WHEA ID 22 event after inject MBE on windows.
HSD-ES:1506755655, [OOB BIOS Configuration]EWS show some variables when SUT without install related device.mismatch bios setup that can't find related variables
HSD-ES:1506744997, [OOB BIOS Configuration]Some variables can find in BIOS setup but can't find in EWS
HSD-ES:1506757895, [OOB Firmware Update] The sensor name format about BIOS image update  SEL  is unexpected
HSD-ES:1506731999, [OOB]there is no warning message in sel log when update corrupt BIOS via OOB FW update
HSD-ES:1506780000, [Intel Xeon Scalable] There is a coding style issue with CL528438 ----[1504579741] Q3'17 #CCB 2030: [Intel Xeon Scalable BIOS/Azure Stack] Enable/disable individual NIC ports.
HSD-ES:2103623558, [Intel Xeon Scalable] 0x8461 SEL log not generate when remove power cord to terminate backup bios update.       
================================================================================
                                 R00.01.0015
================================================================================
Rename BIOS ID from X0168 to R0015
HSD-ES:1504683593, Clone from HSD - Security VT - PCH UEFI FW shall delay PCI Bus Master Enable (PCICMD.BME) until end of POST to prevent DMA attacks on UEFI FW in RAM.
HSD-ES:1506731732, [S2600BP] SEL error during AC cycling: IPMI Watchdog reports the watchdog initiated a hard reset.
HSD-ES:2103623411, There is no SEL log generate when flash BIOS and ME version which same as SUT version.
HSD-ES:1506125764, Q3'18 #CCB2446 BIOS:  Intel Xeon Scalable Post -SRA feature: OOB Update and Config.
HSD-ES:1504788000, [PC Production] Sync Xeon Scalable Production code to PC Production.(5387193:Need Updated BIOS for External Use to Resolve P2P Issue)
HSD-ES:1506754163, FW-UEFI-Vuln-2018-031 - Dynamic loops accessing one element beyond boundary due to <= operator.
FIV_00008379[PC Stitching]Update ESRTIISataEFi version to 05140000.
5387405:PSIRT-FW-UEFI-Vuln-2018-040 SvSmmHandler SMI call-out. 
HSD-ES:1506132901, [S2600BP]MTT CPU1/MTT CPU2 sensors show no reading when run AC cycles and can't recovery within 300s[Only path for this issue,not a final solution].
HSD-ES:1506132509, [S2600BP]SUT hang post screen when run DC cycles.
HSD-ES:1506119814, [S2600BP]HSTI is absent on Windows Server 2016.
HSD-ES:2103623155, SUT will hang up on 0x9D after installed NIC card-X550 and enable RSD.
HSD-ES:2103623142, Update BIOS X0155 SEL LOG BIOS ID is wrong,it show 20.01.0155.
HSD-ES:2007015469, DIMM LED(chX) turns off after another correctable error is injected to a DIMM in different Channel(chY)-V01.
HSD-ES:2204466754, RSD 2.2-SMBIOS Type 199 had zeros value for port 3 and 4 for PCIe Cable ERROR Data.
HSD-ES:2205038517, Random Machine Check failure QPI Phy init abort during reboot reported on S2600ST.	
HSD-ES:2007360181, After CE injection,fault DIMM LED remains asserted despite follow up reset shows healthy memory subsystem-V02.			
HSD-ES:1506438632, Q3'18 CCB2437 [Intel Xeon Scalable BIOS]SOL function terminal type need to support more terminal types the same as console redirection types
HSD-ES:1506131214, Q3'18 #CCB2343[Intel Xeon Scalable] Add BIOS options in ITK to change USB 2.0 ports equalization parameters
HSD-ES:1506435385, Add Factory BIOS flag and .Factory string to SMBIOS Type 0
HSD-ES:1506129880, Q3'18 #CCB2443 [Intel Xeon Scalable BIOS]UPI latency performance parameters which impact bandwidth and latency to be exposed in setup/ITK/syscfg
HSD-ES:2202762181, [S2600BP] Warning SEL during AC Cycling: BMC FW Health reports SSB Temp has failed and may not be providing a valid reading
OSS_0008351/OSS_0008352:Integration BIOS ACM to 1.3.7 and SINIT to 1.3.4
HSD-ES:2103622995, [S2600ST]VMD enable in BIOS is mismatch with motherboard NVME SSD
HSD-ES:1506129887, Q3'18 #CCB2415 [Intel Xeon Scalable BIOS]Extend option value range for Memory Correctable  Error Threshold
HSD-ES:1506395072, ME update failed for X0148 online update to 0D.01.0008
================================================================================
                                  R00.01.0014
================================================================================
Rename BIOS ID from X0149 to R0014.
HSD-ES:1605354891, TPM Update fail on S2600ST and S2600WF
OSS_0008036:       Update Microcode 0x4d for Xeon Scalable H0 and 0x144 for Xeon Scalable B1  
                   Reference code version: 20180612_CP_PURLEY_PRODUCTION_155_R08 
                   [PC Stitching] Update OPA UEFI driver to v1.6.0.0.0 
HSD-ES:1506124820, CCB2334 [PSIRT Factory BMC & BIOS] enabling one-time software update to any version
OSS_0007838,       [PC Stitching]Update ME SPS version to 340
HSD-ES:2103621945, [S2600BP] Windows2016 cannot be installed with SATA port5+port7 RSTe RAID0
HSD-ES:1506125508, Other PCI device's SsidSvid is 0xFFFFFFFF and is different from NIC Controller on SFP+ S2600BP board
HSD-ES:1506122324, Higher security ID from 1.05 to 1.06 because HECI PRT and Backup BIOS PRT patch
HSD-ES:1504762466, BIOS Change for #CCB 2083[Syscfg tool]Add option to configure fan pwm offset in syscfg
HSD-ES:2202640819, System will not boot to IPV4 PXE if UEFI Network Stack disabled for IPV6 PXE in BIOS
HSD-ES:1504784817, CCB2267[BMC+BIOS]Need mechanism for BMC to return MAC addresses for add-in card on demand
HSD-ES:2103622021, Toshiba THNSN5128GPU7 M.2 PCIe SSD can't detect successful under Win2016 OS.
HSD-ES:1504707008, CCB2222 [BIOS] Add Infineon FW update capability support in BIOS and UEFI application
HSD-ES:2007351694, BSOD after warm reboot if HT is enabled with Windows Server 2016 version 17663 and 17666
HSD-ES:2103621261, [S2600WF]SMBIOS Type 8 NIC number does not match motherboard number 
HSD-ES:1504713715, [CCB#2284][S2600WF&S2600BP]Fix system will hang with POST code 0x94 when one riser slot of HOST connects two WRG JBOD nodes with 32 RSSDs
HSD-ES:1406736015, BIOS does not return Type 199 records
HSD-ES:1504707003, CCB1822 Support Relax Ordering and No Snoop in BIOS setup and ITK
HSD-ES:1504749247, [S2600WF]bios_wp protection has not been enabled
HSD-ES:1504749852, CCB2249 Add SMBIOS OEM String modification capability in ITK
HSD-ES:1504771459, After clear CMOS, EWS does not display about CMOS log when boot to BIOS setup
HSD_ES:2103620812, MMIO size set to Auto/1G can't boot to BIOS with NIC Card-XL710 in Legacy mode 
HSD-ES:1504762466, BIOS Change for #CCB 2083 [Syscfg tool]Add option to configure fan pwm offset in syscfg
HSD-ES:2103616363, Inject Memory Address Parity error and no error event occurred in SEL accordingly
HSD-ES:1504630755, Change "CPU Power and Performance Policy" from "Balanced Performance" to "Performance" on the custom BIOS capsule by ITK tool, related items "C1E" can not be changed automatically.
HSD-ES:1504788000, CL541242  5386244: BaseTraceHubInitLibNull references non-existing SkylakeSiPkg
HSD-ES:1504788000, CL547293  5386319: Xeon Scalable 2933 mc transient error
HSD-ES:1504788000, CL556508  5386005: BIOS NTB PPD Option Setup is Reversed
HSD-ES:1504788000, CL558559  5386307: Some validated DIMMs have not been included in the DimmWT4 table
HSD-ES:1504788000, CL558628  5385969: Advanced Memory Test failed at MT_CPGC_READ_WRITE   
HSD-ES:1504788000, CL570837  5386628: HECI_MBAR can be reallocated by ring-0 anywhere in the address map (BIOS vulnerability)
HSD-ES:1504788000, CL569535  5386412: 2 SKT DEBUG build ASSERTs with a Security Violation
HSD-ES:1504788000, CL566239  5386475: System hangs after error injection during DIMM Address Translation
HSD-ES:1504788000, CL571328  5386488: 2006702382: NVDIMM not in memory map when NUMA is disabled
HSD-ES:1504788000, CL576560  5386813: Enable MSR_VIRTUAL_MSR_LLC_PREFETCH reconfiguration on Xeon Scalable B-step
HSD-ES:1504788000, CL579507  5386817: Add device IDs for QS/PRQ S LBG SKU
OSS_0006624:       Integration BIOS ACM to 1.3.6 and SINIT to 1.3.3
OSS_0007339:       [PC Stitching] Update ME SPS version to 333
HSD-ES:2202565747, BIOS POST messaging shows no errors when in fact a DIMM is mapped out
HSD-ES:1504788000, CL575833 5386751: Function RemovePsfAccess () is not called with SPS FW binary
HSD-ES:1504788000, CL582692 5386573: IioEarlyInit.c:IioPciePortEWL() swaps link_width and link_speed in EWL
HSD-ES:1504788000, CL558927 5386052: [220586227] Early SEC RC is not properly programming the HPET due to coding bug, causing rogue write to memory [IPS 220586227]
HSD-ES:1504788000, CL 553223 + CL556549 5386074: ACPI table will miss some core with some specific bit mask processor
HSD-ES:1504790255, Clone from 5386949 FW-UEFI-Vuln-2018-008 - "PSIRT-BIOS-2018-008 Additional protection for DCI enable"
HSD-ES:2103617388, When hotplug NVMe HDDs the RSTe GUI location couldn't match actual HDDs location
HSD-ES:1505084878, XL710 show the same boot order name in Boot management
HSD-ES:1505083003, CCB 2161 [BIOS]Support more memory vendor DIMMs -- Apacer,ATP,Hyundai,Innodisk,intelimem,V Color
HSD-ES:1505083055, CCB 2401 [BIOS] BIOS support for WFC, WFD, WFS cluster systems
HSD-ES:2103619811, [S2600BP] Boot manager still show pcie device if disable it on PCIe Port Oprom Control. -->Fix CL552580 side effect
HSD-ES:2103620496, NIC Port Mapping between Chassis and Windows Server OS are inverted on S2600BP SFP+, RJ45 and S2600WFT
OSS_0006929:       [PC Stitching] Update RSTE Drivers to v5.4.0.1039
HSD-ES:2103621959, EWS and SEL viewer shown incorrect ME version when online update ME version
HSD-ES:1504784817, CCB2267 [BMC+BIOS]Need mechanism for BMC to return MAC addresses for add-in card on demand
HSD-ES:1505330637, Add two APIs in fast video ppi and protocol
HSD-ES:2103620418, [S2600WF] After downgrade FD and ME, SUT will halt with beep code 1-5-1-2 when reboot
================================================================================
                                  R00.01.0013
================================================================================
Rename BIOS ID from X0117 to R0013.
Microcode 0x140 update for B1
===============================================================================
                                  R00.01.R0012
================================================================================
Rename BIOS ID from X0115 to R0012.
Microcode 0x43 and 0x13f update to address Intel-SA-00088 

================================================================================
                                  R00.01.R0011
================================================================================
Rename BIOS ID from X0114 to R0011.
HSD-ES: 1504685331,[PC Stitching] Sync Microcode 0x3c for Xeon Scalable Family H0 from RP
HSD-ES: 1604595333,[PC Stitching] Sync Xeon Scalable Family B1 Production Patch 0x13e from RP
HSD-ES: 1504705784,[PC Stitching] Integrate the OPA UEFI driver v1.6.0.0.0 from RP
HSD-ES: 1504651973,The SerialA Console continues to work while the VGA screen appears hung after enable serial port A enable and input "reconnect -r" in efi shell, update Aspeed GOP to v1.07
HSD-ES: 1504634146, [PC Production] Sync Rp code to PC Production

================================================================================
                                  R00.01.R0010
================================================================================
Rename BIOS ID from X0108 to R0010.
HSD-ES: 1504694350,Higher security ID from 04 to 05 because Microcode 3c include security patch
HSD-ES: 1504686401,Integration BIOS ACM to 1.3.4
HSD-ES: 2103617388,When hotplug NVMe HDDs the RSTe GUI location couldn't match actual HDDs location.
HSD-ES: 1504626593,[S2600BP]Some variables cannot load default when it was deleted after SUT reset
HSD-ES: 1504680515,[CCB 2076]  Allow user to change serial communications setting values independent of Console Redirection and Serial Over LAN state
HSD-ES: 2103619487,[S2600BT] System boot no hotkey string displayed on POST diagnostic screen with change System Boot Timeout value to 30 and unplug the proper markerfile (payloadsig.txt) USB Key devices.
HSD-ES: 2103619922,[S2600WF] Smbios Type 8 doesn't list table of CPU1 PCIe_SSD port connector on WFQ
HSD-ES: 2103617706,[Retimer]The system HDD5~7 carrier LED no display on first power on.
HSD-ES: 1504654004,Request to modify PCH SATA Tx De-emph and Rx CTLE setting
HSD-ES: 1504659011,Integrate latest v2.021R8153 EFI driver
HSD-ES: 1504653444,ITK modified Bifurcation settings for Riser slots will revert back to factory default value after pressing f9
HSD-ES: 2103619811,[S2600BP] Boot manager still show pcie device if disable it on PCIe Port Oprom Control.
HSD-ES: 2006676137,BIOS F2 menu doesn't show drive's OPROM under re-timer AIC in slot 4 when populating slot 2 with RSP3WD080
HSD-ES: 2103619292,C1E help text character display abnormal under console redirection
HSD-ES: 2006677577,,Unable to locate/fault/rebuild instructions to NVME drive  from EFI tool and OS for drives  under retimer AIC 
HSD-ES: 2006669546,,RAID module RMS3HC080 and Software RAID RSTe can't work together on a S2600WF system
HSD-ES: 1504605915,,#CCB 2049:To add ITK option to change MMIO High base to support various PCIe cards and Some OS compatibility issue
HSD-ES: 1504599337,,CCB#1896: iSCSI Boot Options Support for RSD 2.2 Spec.
HSD-ES: 1504595731,,RSD [S2600WF]: Provide SMBIOS table type 192 for RSD 2.2 Spec.
HSD-ES: 2103619444,,[S2600WF] Lan Device will disappear if only enable one NIC port after two NIC ports both are disabled.
HSD-ES: 2103619177,,[S2600WFQ] Boot time becomes very slowly, almost 6 times after flash FTPM Enabled Capsule file
HSD-ES: 1604527341,,[HaT] 3rd party code (OPROMs) can fake their TPM measurement
HSD-ES: 1504630755,,#CCB 2145:  Expose BIOS option [CPU Power and Performance Policy] to ITK and Syscfg
HSD-ES: 1504620840,,[S2600BP] CHIPSEC test find all PRx set to 0 after enable security.
HSD-ES: 2103619456,,[S2600BP] the Current Usage of SMBIOS Type 9 - System Slots are all In use even no PCIe Device attached with -F CPU
HSD-ES: 1504634146,,[PC Production] Sync Rp code to PC Production
HSD-ES: 1504599259,,CCB#1896(S2600WF):   Provide SMBIOS table type 197 for RSD 2.2 Spec.
HSD-ES: 1504599267,,CCB#1896:(S2600BP):  Provide SMBIOS table type 200 for RSD 2.2 Spec.
HSD-ES: 2103619114,,[S2600WF] Modify Legacy Boot Order "EFI Shell" item via ITK do not take effect, shell always in the Bottom.
HSD-ES: 1504591223,,Iflash32 utility can't get ITK modified custom BIOS revision string correctly. 
HSD-ES: 2006663518,,S2600ST QAT SKU PCH PCIE Uplink margin failed on Silver Build 3(PCH=QN1L B2)
HSD-ES: 1504595731,,RSD [S2600WF]: Provide SMBIOS table type 192 for RSD 2.2 Spec.
HSD-ES: 2103617706,,[Retimer]The system HDD5~7 carrier LED no display on first power on.
HSD-ES: 1504581583,,Rp RAS code sync  CL528211  5386077: Mirrorfailover should happen when mirrorfailover=1 and (mccmdvld=1 or errortype[4]=1)
HSD-ES: 2103619464,,[S2600WF] Add one Switch/Retimer card, RAID controller still shows in EFI shell via PCI command after disable VMD
HSD-ES: 1504591221,,RSD SMBIOS table was overwritten by OOB RSD SMBIOS table 
HSD-ES: 1504593557,,RSD: [S2600BP]Current link speed always is 0x40 in RSD SMBIOS type 190.
HSD-ES: 1504591388,,CCB#1896: Provide SMBIOS table type 199 for RSD 2.2 Spec.

================================================================================
                                   R00.01.0009
================================================================================
Rename BIOS ID from X0084 to R0009.
HSD-ES: 2103619332, , [S2600WF] NIC configuration page not show OCP controller and MAC info or show wrong when install OCP X527-DA2 on S2600WFT SKU or X527-DA4 on S2600WFQ SKU.
HSD-ES: 2103619390, , [S2600BP] Set "NIC1 Port1/2" to Disabled cannot be saved under legacy mode with S2600BP NIC X550.
HSD-ES: 1504599235, , [PC Stitching] Sync Microcode 0x30 for Xeon Scalable Family H0 from RP.
HSD-ES: 2103619297, , [S2600BP] ME status shows "Not ready" and ME revision shows "Unknown" after SPS FW downgrade from 04.00.04.285 to 04.00.03.235.
HSD-ES: 1504615636, , [PC Stitching] Sync Microcode 0x32 for Xeon Scalable Family H0 from RP.
Update BIOS security version to 0004.
HSD-ES: 2103619238, , [S2600WF] PXE function still work whether press F12 or selected from boot manager when disable NIC control.
Check in SPS FW 04.00.04.288 on critical security issue 

================================================================================           
                                   R00.01.0007
===============================================================================
HSD-ES: 220788736, ,S2600WF system goes into continuous restart loop after SUP update process on H48104-701 board with SUP x0060 installed and two embedded NIC ports disabled
HSD-ES: 1504597970, ,Fix issue- Array OCPDID Index Out of Bounds.

================================================================================
                                   R00.01.0006
================================================================================
HSD-ES: 1504579741, , CCB 2030:  Enable/disable individual embedded only NIC ports
HSD-ES: 1504582533/1504582491,  CCB 2022: Support storage and networking SMBIOS extensions for RSD2.2 on S2600WF
HSD-ES: 1504589353, , [PC Stitching] Sync Microcode 0x2e for Xeon Scalable Family H0 from RP 
HSD-ES: 1504581907/1504580980/1504573931/1504563070, , CCB 1896: Provide SMBIOS table type 197 for RSD 2.2 Spec.
HSD-ES: 2103618468, , [S2600BP] Current Active Processor Cores do not show the corresponding number when Active Processor Cores changed with Quad core QMRN CPU
HSD-ES: 2103618733, , [S2600WF] SMBIOS Type 16 of maximum capacity value of 0x90000000, is not represented in the Extended Maximum Capacity field.
HSD-ES: 1504580965, , RsaReadyToBoot should run before AssertPostGpio in ReadToBootEvent
HSD-ES: 220680356, , X722 NVM v3.49 BIOS integration
HSD-ES: 2103618637, , [S2600BP] SKU SFP+/1G: UUT show "Nmi activated - system halted" during POST when PCIE riser 2 x8 slot 2 installed a NIC/RAID card
HSD-ES: 1504580069, , [PC Stitching] Sync Xeon Scalable Family B1 Production Patch 0x13b from RP 
HSD-ES: 1504580058, , [PC Stitching] Sync Microcode 0x2c for Xeon Scalable Family H0 from RP
HSD-ES: 1504580414, , XPT Prefetch BIOS knob remove from PCSD BIOS. (XPT on Xeon Scalable Family Server is no longer POR)
HSD-ES: 1504579991, , S2600WF IFT config dat support class 3
HSD-ES: 2006669546, , RAID module RMS3HC080 and Software RAID RSTe can't work together on a S2600WF system
HSD-ES: 2103618307, , System Boot Timeout function not working if enable Power On Password
HSD-ES: 2103614644, , [S2600WF] "HDD Rebuild in progress" events were occurred during DC cycling
HSD-ES: 1504559251, , [PC-Stitching]Update ME SPS version to MR 235
HSD-ES: 2103618046, , After injecting MBIST error at rank sparing mode, memory size shows wrong.
HSD-ES: 1504567201, , RP production code sync up
HSD-ES: 2103618268, , [S2600WF] When Add-in M6000 in riser 1 slot1, SUT cannot boot normally on S2600WFQ
HSD-ES: 1504567160, , [S2600WF]Hard code the variable value of  Processor MSR Lock Control
HSD-ES: 2103617172, , [S2600BP]UEFI Mode,Boot order value doesn't follow ITKs' with FDD device.
HSD-ES: 2103618243, , [S2600ST] An new item "Diagnostic Messages" which should be invisible in BIOS setup.
HSD-ES: 2103618185, , [S2600WF] The memory info will show 'Empty/NO DIMM' in SMBIOS Type 17 if populate 1R DIMM on CPU1 Channel A and B and build Rank Sparing mode.
HSD-ES: 1504551789, , [PC Stitching] Sync Xeon Scalable Family B1 Production Patch 0x13a from RP 
HSD-ES: 1504551442, , [PC Stitching] Sync Microcode 0x29 for Xeon Scalable Family H0 from RP
HSD-ES: 1504549582, , Integration BIOS ACM to 1.3.3
HSD-ES: 1504543699, , [PC Stitching] Sync Xeon Scalable Family B1 Production Patch 0x139 from RP

================================================================================
                                    R00.01.0005
================================================================================
HSD-ES: 2103617864, ,[S2600WF] BIOS will not keep boot order after remove boot device.
HSD-ES: 220203024, , [S2600WF Retimer] VMD menus do not match system state  (for example 3 slot riser + 4P/8P switch + VROC key + VMD enabled does not enable VROC OpROM in some cases)
HSD-ES: 1504525281, , The uncore frequency cannot fix at the max frequency when UFS is disabled on S2600WF
HSD-ES: 1504539977, , #CCB 1974:  Remove BIOS WA which requested in SW CCB1958# and move to HW solution for S2600BP Full QAT
                      Enable all QAT EP in BIOS,  Enable PCIE x4 link from CPU to PCH.
HSD-ES: 1504536397, , Syscfg_V14.1.16: The boot order is different between press F9 and key command “syscfg /bldfs “ ” " to load default on Legacy mode.
HSD-ES: 1504396363, , BIOS should include production key when secure boot enabled.
HSD-ES: 1504411203, , CCB#1751[Xeon Scalable Family BIOS]Need to port Customer work from S2600V3/V4 BIOS to Xeon Scalable Family BIOS for Customer on S2600ST

================================================================================           
                                   R00.01.0004
================================================================================
Rename BIOS ID from X0029 to R0004.
HSD-ES: 2006649895, , FRB2 Asserted during system boot when 7 QLogic PCI cards are inserted on the system.
HSD-ES: 1504396363, , BIOS should include production key when secure boot enabled.
HSD-ES: 2006650537, , [S2600BP]DMI Information for the network device is not correct. "enp" as oppose to "eno".
HSD-ES: 1504403422, , Update ME FW to the new version.
HSD-ES: 1504531663, , [PC Stitching] Sync Microcode 0x26 for Xeon Scalable Family H0 from RP.
HSD-ES: 1504521876, , [S2600BP]NVMe U.2 SSD can't be detected or link speed/width downgrade during reboot cycling.
HSD-ES: 2103617966, , [S2600WF] The warning message is incorrect when set Admin/User PWD the same.
HSD-ES: 1504521041, , [S2600BP]Syscfg_V14_1:Command:syscfg /bldfs  "" and F9 load different Bios default Boot Order.

================================================================================
                                   R00.01.0003
================================================================================
Rename BIOS ID from X0021 to R0003.
HSD-ES: 1504527306, , Integration BIOS ACM & SINIT to 1.3.2.
HSD-ES: 1604381641, , [Intel(R) Optane(TM) DC Persistent Memory S2600WF] Can't update ME version with Debug BIOS.
HSD-ES: 1504527236, , CCB 1958: S2600BP RJ45-L SKU need disable Uplinkx4 and QAT2 for PCH power consumption reduction.
HSD-ES: 2006650537, , [S2600BP]DMI Information for the network device is not correct. "enp" as oppose to "eno".
HSD-ES: 2103617705, , The system SATA HDDs will Warning on BMC web.
HSD-ES: 1504526567, , [PC-Stitching] Sync Xeon Scalable Family B1 Production Patch 0x138 from RP.

================================================================================
                                   R00.01.0002
================================================================================
Rename BIOS ID from X0014 to R0002.
HSD-ES: 2006650537, [S2600BP]DMI Information for the network device is not correct. "enp" as oppose to "eno"
HSD-ES: 220203024,  3 slot riser + 4P/8P switch + VROC key + VMD enabled does not enable VROC OpROM in some cases
HSD-ES: 2103616560, VMware 6.5 Passthrough of RMSP3AD160F doesn't work with S2600WF 2U BIOS SE5C620.86B.01.00.0448
HSD-ES: 2103617774, [S2600BP] Package C1 always >90% whatever Package C-state with BIOS X0008
HSD-ES: 1504403422, Update ME FW to the new version
HSD-ES: 2103617693, [S2600BP]UUT cannot boot to EFI Shell automatically in recovery mode.
HSD-ES: 2103617718, [S2600BP] Windows OS eventview not report whea eventID 23 after SBE is sucessfully injected with BIOS X0008.
HSD-ES: 2103616570, [S2600WF]SUT can not boot to Win2016 with FAB2 Switch card.
HSD-ES: 2103617732, [S2600BP] SFP+ SKU socket0 1a,1c always show x8 whatever CPU1 IOU1 setting.
HSD-ES: 2103617198, [S2600BP]Can not build raid if pcie ssd connect VMD Port CPU1 1C/1D & VMD Port CPU2 3A/3B.
HSD-ES: 2103617682, [S2600BP]Riser_Slot_X Bifurcation's help text is incorrect in BIOS X0007 and BIOS Setup Degin v1.04
HSD-ES: 1504521158, Optimize slot3 VMD option display.
HSD-ES: 1504452197, #CCB 1900 [S2600WF BIOS] Enable Symmetric QAT Support in BIOS for hardware CCB 1893
HSD-ES: 1504521139, [S2600WF] and [S2600BP] short team solution for 10Gbe MAC address need BIOS sent it to BMC FW
HSD-ES: 1504437936, [SDLS4]REACT-2017-1-OpenSSL upgrade for security vulnerability
HSD-ES: 1504520668, GPIO need to be locked on all of platform
HSD-ES: 1504403422, Update ME FW to the new version
HSD-ES: 2103617416, [S2600WF] Pause key will not suspend the FRB2 timer during post process, thus system will reboot after 6 min.
HSD-ES: 1504515553, Integration BIOS ACM to 1.3.1
HSD-ES: 2103617458, [S2600BP] Amber LED have keep blinking  once boot into OS.(when disabled VMD)
HSD-ES: 1504452197, #CCB 1900 [S2600WF BIOS] Enable Symmetric QAT Support in BIOS for hardware CCB 1893
HSD-ES: 2103616570, [S2600WF]SUT can not boot to Win2016 with FAB2 Switch card.
HSD-ES: 2103617398, [S2600ST] SMBIOS type 20 "Memory Device Handle" and "Memory Array Mapped Address Handle" not align with type17 and type 19.
HSD-ES: 1504513467, [PC Stitching] Sync Microcode 0x22 for Xeon Scalable Family H0 from RP
HSD-ES: 2103615650, [Cert] HLK USB 3.0 Exposed Port System Test will be fail

================================================================================
                                   R00.01.0001
================================================================================
Rename BIOS ID from X0005 to R0001.
HSD-ES: 1405802398, SDP: UEFI PXE is failing with message "PXE-E16: No Offer received." on S2600WF.
HSD-ES: 1504506169, Open all setup options, except [CPU Power and Performance Policy] under Power and Performance page to Syscfg.
HSD-ES: 2103617250, PCIe SSD cann't be detected by Redhat 7.3  on 6Port 3408 or 6Port 3008 after plug out/in.
HSD-ES: 2103617276, [S2600ST] The first digit of BMC build number in "BIOS post information" isn't printed if it's 0.
HSD-ES: 1504483939, Error: 'ascii' codec can't encode character in this title!
HSD-ES: 1504396268, Unsigned capsule should be copied to root folder.
HSD-ES: 1504502129, Integration BIOS ACM to 1.3.0
HSD-ES: 1504502257, Error: 'ascii' codec can't encode character in this title!
HSD-ES: 1504501726, Disable Sddc Plus one
HSD-ES: 1504502155, [PC-Stitching] Support BIOS ID in the  IFWIingredientTable.htm
HSD-ES: 220194030,  [S2600BP] With BIOS D503 tftp during WDS UEFI PXEBOOT fails, Legacy still works
HSD-ES: 2103617198, [S2600BP] Can not build raid if pcie ssd connect VMD Port CPU1 1C/1D & VMD Port CPU2 3A/3B.
HSD-ES: 1209680381, [S2600BP] CPU slow down when power dropped from 1 PSU
HSD-ES: 2006635112, Function keys F6, F9, F10 and F12 not working when using serial connection
HSD-ES: 220187579,  S2600WFQ NVM v3.38 BIOS integration.
HSD-ES: 1504480516, #CCB 1925 [ BIOS] Change boot order so UEFI is same as legacy
HSD-ES: 2103615650, [Cert] HLK USB 3.0 Exposed Port System Test will be fail
HSD-ES: 1504396363, BIOS should include production key when secure boot enabled.
HSD-ES: 220187598,  S2600ST NVM v3.38 BIOS integration.
HSD-ES: 220187591,  S2600BP NVM v3.38 BIOS integration
HSD-ES: 1504403422, Update ME FW to the new version
HSD-ES: 1504495288, [PC Stitching] Integrate the Microcode 0x1e for Xeon Scalable Family H0 from RP
HSD-ES: 2006616153, BIOS update to include the Omni-path Gen1 Fabric AOC Platform Config Files
HSD-ES: 1504489067, SINIT ACM 1.2.1 update.
HSD-ES: 1504495428, Microcode version is not correct in BIOS capsule file
HSD-ES: 1504495368, [PC Stitching] Integrate the OPA UEFI driver v1.4.0.0.0 from RP
HSD-ES: 2103614736, [S2600BP NVDIMM] NVDIMM marked as "?" in windows 2016 Device Manager.
HSD-ES: 1504396262, Remove 'UpdateNvram' support for iflash32 tool for security reason of SRA bios
HSD-ES: 1504396357, Public key should be included in BootBlock of BIOS
HSD-ES: 2103616884, [S2600WF] The root port description is incorrect in VMD page when 3 slot riser installed.
HSD-ES: 2103616467, [MIC-S2600WF] WHLK USB Exposed System Test Fail.
HSD-ES: 2103616983, [S2600BP] Load file URI address string is not fully on boot option description when boot into HTTPv6 server.
HSD-ES: 1504492558, [S2600BP]Disabled boot type still show in boot manager menu(F6), not match with display devices in Boot order or Boot Manager .
HSD-ES: 2103616521, [S2600BP] SUT cannot boot normally after do recovery boot once with primary BIOS D0485 and backup BIOS D0478
HSD-ES: 220131068,  Serial Over Lan funtion not working correctly - (1) When SOl is enabled - Splash screen stays enabled which masks the console data.
HSD-ES: 1504493464, [PC-Stitching] Removing Xeon Scalable Family A1/B0 Microcode support from trunk
HSD-ES: 1504429786, #CCB 1863 [ Common]BIOS should support the Demoted Warm Reset (DWR) flow and setting of the 'Debug Enable' MSR bit
HSD-ES: 2103616882, Error: 'ascii' codec can't encode character in this title!
HSD-ES: 1504429786, #CCB 1863 [ Common]BIOS should support the Demoted Warm Reset (DWR) flow and setting of the 'Debug Enable' MSR bit
HSD-ES: 1504480516, #CCB 1925 [ BIOS] Change boot order so UEFI is same as legacy
HSD-ES: 1504483939, Error: 'ascii' codec can't encode character in this title!
HSD-ES: 1504492558, [S2600BP]Disabled boot type still show in boot manager menu(F6), not match with display devices in Boot order or Boot Manager .
HSD-ES: 1504493464, [PC-Stitching] Removing Xeon Scalable Family A1/B0 Microcode support from trunk
HSD-ES: 1504495288, [PC Stitching] Integrate the Microcode 0x1e for Xeon Scalable Family H0 from RP
HSD-ES: 1504495368, [PC Stitching] Integrate the OPA UEFI driver v1.4.0.0.0 from RP
HSD-ES: 2006616153, BIOS update to include the  Omni-path Gen1 Fabric AOC Platform Config Files
HSD-ES: 2103614736, [S2600BP NVDIMM] NVDIMM marked as "?" in windows 2016 Device Manager.
HSD-ES: 2103616467, [MIC-S2600WF] WHLK USB Exposed System Test Fail.
HSD-ES: 2103616521, [S2600BP] SUT cannot boot normally after do recovery boot once with primary BIOS D0485 and backup BIOS D0478
HSD-ES: 2103616882, Error: 'ascii' codec can't encode character in this title!
HSD-ES: 2103616884, [S2600WF] The root port description is incorrect in VMD page when 3 slot riser installed.
HSD-ES: 2103616983, [S2600BP] Load file URI address string is not fully on boot option description when boot into HTTPv6 server.
HSD-ES: 1504489067, SINIT ACM 1.2.1 update.
HSD-ES: 1504495428, Microcode version is not correct in BIOS capsule file.
HSD-ES: 1504396262, Remove 'UpdateNvram' support for iflash32 tool for security reason of SRA bios.
HSD-ES: 1504396357, Public key should be included in BootBlock of BIOS.
HSD-ES: 1504396268, Unsigned capsule should be copied to root folder.
HSD-ES: 1504403422, Update ME FW to the new version.
HSD-ES: 220131068,  Serial Over Lan funtion not working correctly - (1) When SOl is enabled - Splash screen stays enabled which masks the console data.
HSD-ES: 1504399927, The PCIe port name in PCIe port Oprom control is not same to circuit diagram.
HSD-ES: 2103616317, SMBIOS Type 8 and Type 41 are incorrect.
