===============================================================================
        Intel(R) Server Platform Integrated BMC Firmware Release Notes
===============================================================================


INTEL(R) Server Boards and Systems 
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA


===============================================================================
DATE:       19 March 2022


TO:         Intel(R) Server Board S2600XX


SUBJECT:    Integrated BMC(R) firmware 2.88 release notes

===============================================================================
                               LEGAL INFORMATION
===============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.


Intel is a registered trademark of Intel Corporation.


*Other names and brands are the property of their respective owners.


Copyright (c) 2022 Intel Corporation.


A portion of this firmware is open source code.
The OSS source code that the customer is entitled to per OSS license has been
posted on the Intel support website at the following link:

https://downloadcenter.intel.com/download/26968/BMC-Source-Code-for-Intel-62X-Series-Server-Boards-and-Systems


This open source code falls under the GPL 2.0 license, please see the license
at the following link:

http://www.opensource.org/licenses/gpl-2.0.php


===============================================================================
                            ABOUT THIS RELEASE PACKAGE
===============================================================================
Source file: Purley_2.88.6999d21a.bin
Built from git revision: 6999d21a06b2ac81cdaae535b3c6c744f473ef29

REVISION INFORMATION RETURNED BY GET DEVICE ID COMMAND:
Operational mode:   2.88.6999d21a

Device ID:          0x22
Manufacturer ID:    0x000157

SHA1 checksum:
    Purley_2.88.6999d21a.bin: 8188639639343a92ec2ae4df2dc5b83d6da79133

JAVA Certificate:
from:    Wed Jan 19 08:00:00 CST 2022 UTC/GMT+08:00
until:   Fri Jan 20 07:59:59 CST 2023 UTC/GMT+08:00

Redfish Specification: DSP0266 v1.7
Redfish Schemas:       DSP8010 v2019.1

Embedded firmware files for the following components:
Power Supplies
    1100ADU00201 00: 54.1.1
    1100ADU00201 01: 54.1.1
    1100ADU00201 02: 54.1.1
    1100ADU00201 03: 54.1.1
    1100ADU00201 04: 54.1.1
    1100ADU00201 05: 54.1.1
    1100ADU00201 S3: 54.1.1
    DPS-1200TB A 00: 77.39.4
    DPS-1200TB A 02: 89.40.6
    DPS-750AB32A S0: 33.3.3
    DPS-750XB A  S4: 100.39.5
    DPS-900AB-5 E 00: 13.13.0
    DPS-900AB-5 E S3: 12.12.0
    PSSF132202A  00: 23.5.0
    PSSF132202A  01: 23.5.0
    PSSF132202A  03: 25.5.0
    PSSF132202A  S3: 23.5.0
    PSSF162202A  00: 75.9.0
    PSSF162202A  01: 75.9.0
    PSSF162202A  02: 75.9.0
    PSSF162202A  03: 75.9.0
    PSSF162202A  04: 75.9.0
    PSSF162202A  05: 78.9.0
    PSSF162202A  06: 78.9.0
    PSSF162202A  07: 78.9.0
    PSSF162202A  08: 78.9.0
    PSSF162202A  09: 78.9.0
    PSSF162202A  11: 78.9.0
    PSSF162202A  11: 78.9.0
    PSSF162205A  00: 18.4.0
    PSSF162205A  01: 18.4.0
    PSSF162205A  02: 18.4.0
    PSSF212201A  00: 12.3.0
    PSSF212201A  01: 14.3.0
    PSSF212201A  S3: 12.3.0
    PSSF222201A  S4: 33.0.0

Hot Swap Backplane
    V1 HSBP: 1.22
    V1 HSBP: 1.33
    V2 HSBP: 2.08
    V2 HSBP: 2.09

Firmware Update Tools: FWPIAUPD_v14_1_Build19

* NOTE  The PSSF222201A 00A or newer identifies itself as a PSSF222201A S4 internally.
Please use that firmware version when referencing that PSU.

*** IMPORTANT *** 

    WARNING: Starting from BMC v2.86, BMC does not allow upload .key files and only accepts .pem 
    file for SSL certificate. 
            
    If uploaded SSL Certificate or Key files fail to format checking, BMC will remove the invalid
    format file before starting BMC EWS and re-generate a self-signed certificate to ensure the
    BMC EWS can boot up successfully. Please consult TA-1176 for more details
    
    WARNING: Starting from BMC v2.88,  Purley platfomrs only support SSL certificate which is equal to or longer
    than 2048 bit.

    WARNING: A security issue was fixed in Purley platforms. BMC credential is 
    required to access files in internal virtual media from BMC v2.88.
    
    Issue:[Internal Virtual Media] Files in internal virtual media are accessible 
    without BMC credential 

    WARNING: Starting from BMC v2.88, EWS Active Directory should allow
    domain name and user name longer than 16 characters.

    The AD Setting will be cleared after downgrade to v2.86 or lower BMC versions if the Domain Name
    is equal to or longer than 32 characters.

*** IMPORTANT *** 
Downgrading below 1.43.660a4315 is not supported due to a security revision change. 

-------------------------------------------------------------------------------

===============================================================================
                         IMPORTANT INSTALLATION NOTES
===============================================================================
The following update process must be followed to ensure a trouble free updating
of your baseboard.  The order is important to minimize any issues for status
checking as different components are initialized.
1.  BMC firmware
2.  BIOS/Manageability Engine (ME) firmware (as directed in BIOS Release Notes)
3.  FRU/SDR package specific to the baseboard.
4.  NIC EEPROM

===============================================================================
                            INSTALLATION PROCEDURE
===============================================================================
There are two supported ways to update the BMC firmware.
You may opt to use the Web GUI or the UEFI shell method.

Web GUI update
1. Unzip the package onto your system
2. Log into the BMC web GUI
3. Navigate to Configuration, then Firmware Update
4. Click browse, and direct the browser to the location of Purley_2.88.6999d21a.bin
5. Click upload.  Progress and status will be shown as the update progresses


UEFI update
1.  Unzip package and load onto a flash drive
2.  Boot to UEFI shell, and navigate to the folder where this package lives
3.  Run fwUpdateBMC.nsh and follow the prompts

===============================================================================
                     FIRMWARE UPGRADE/DOWNGRADE PROCEDURES
===============================================================================
Upgrade of BMC FW from version 2.88 to later versions
will be documented in the release notes for those versions.

Reverting to a lower version of firmware may have unexpected side effects,
including but not limited to user settings reset to defaults, and will always
result in the loss of functionality which was present in the higher version
but was not implemented in the lower version.
We do not guarantee that any downgrade will operate without side-effects.

Downgrading below 1.43.660a4315 is not supported due to a security revision change.

===============================================================================
                        KNOWN ISSUES/WORKAROUNDS/REQUIREMENTS
===============================================================================

    WARNING: This release disables RMCP authentication by default.  ipmitool uses
    RMCP by default, so it will fail to authenticate.  Add the '-I lanplus' parameter
    to all ipmitool commands to use RMCP+ instead.

    WARNING: This release has the BMC PCIe bridge disabled.  This will cause the
    majority of operating systems to fail at boot as they stall during video
    driver initialization
    
    WARNING: When using IPMI to establish a SOL session using KONSOLE:
    A. The "Delete" input cannot be captured when pressing "Backspace" 
       Workaround: Modify the "Backspace" key to "0x08" in the KONSOLE profile keyboard settings.
    B. Resizing a KONSOLE window with an active SOL session can cause the content to overlap 
       Workaround: None. Recommend using the Java SOL Viewer instead of KONSOLE
       
    WARNING: Redfish API POST requests using a browser extension or plugin will fail if the extension manipulates the 
    HTTP(S) Origin header. This affects REST clients which are implemented as browser (chrome, Firefox) plugins or extensions 
    such as the older versions of Postman. It is recommended to use Postman version 6.0 or later.For security purposes, the 
    BMC Redfish API requires that if a HTTP Origin header is present, the host portion of the Origin header must match the 
    HTTP Host header. Some browser based REST clients alter the Origin header preventing their use with the BMC.


    Steps to recover a failing Operating System:

    Linux variants (one of the below):
        A. Ensure the "modprobe.blacklist=ast" parameter is set in your boot loader (grub) 
        B. Ensure you are using a kernel version V4.10 or newer
		For Red Hat* Enterprise Linux* v7.3, please refer to the included "RHEL73_InstallationGuide_Rev1.00.pdf"
		For SUSE* Linux* Enterprise Server v12 SP1 or SP2, please refer to the included "SLES12_InstallationGuide_Rev1.00.pdf"

    Windows variants:
        Boot to safe mode, and load aspeed video driver v1.03 or greater and reboot
		For Windows* Server 2016, please refer to the included "WinSrv16_InstallationGuide_Rev1.00.pdf"

    Redfish API:
        Redfish API POST requests using a browser extension or plugin will fail if the
        extension manipulates the HTTP(S) Origin header. This affects REST clients which
        are implemented as browser (chrome, Firefox) plugins or extensions such as the
        older versions of Postman. It is recommended to use Postman version 6.0 or later.

        For security purposes, the BMC Redfish API requires that if a HTTP Origin header
        is present, the host portion of the Origin header must match the HTTP Host header.
        Some browser based REST clients alter the Origin header preventing their use with
        the BMC.

    WARNING: Starting from BMC v2.21, When KCS control mode is put in restricted and deny all mode,
    BMC EWS CPU and DIMM page displays blank or last  DC on configuration information.

    WARNING: IPMIUtil can not support user password length larger than 16 bytes.

    WARNING: When KCS policy control mode is configured as "Deny All", BMC and FRUSDR cannot be
    upgraded/downgraded as expected behavior.
    KCS Policy control mode is "Allow all" by default on all BIOS from version R02.01.0009 and older

    WARNING: Starting from BMC 2.22.59c3b83a, when KCS Policy Control Mode is configured as "Deny ALL" on BMC EWS, BMC and FRUSDR cannot be upgraded/downgraded as expected behavior. Updates can still be performed via Redfish or BMC EWS

    	Cipher Suite 3 is disabled by default since BMC firmware 1.90 and only keep Cipher Suite 17 opened by default.
	Due to this the extra parameter "-C 17" is required for ipmitool to work via LAN.
	The Cipher Suite 17 was first introduced in ipmitool 1.8.18 on Oct 8th 2016, 
	you have to update ipmitool to this version or newer one, earlier versions of ipmitool don’t have Cipher 17 support
	ipmitool is not working well when running in high load network. We recommend to add extra timeout by using “-N 5”. 
	Default is 1 second for RMCP+, which is not enough. –N 5 will set 5 second as timeout.
	So the command will look like:
	ipmitool –I lanplus –H ip –U user –P password –C 17 –N 5 command
	Please refer to the included "TA-1143_Extra_parameters_needed_for_ipmitool.pdf"

    WARNING: Starting from BMC 2.48.ce3e3bd2 implements new security rules about password complexity, please consult TA-1161 for more details

    

===============================================================================
                                
===============================================================================
				DEFECTS SOLVED
===============================================================================
v2.88.6999d21a -(Release version)
===============================================================================
    Upgrade kernel to 4.9.294
    CCB3457:[BIOS & BMC]Bypass BIOS admin password when FORCE_EFI_BOOT or SILENT_FORCE_EFI_BOOT is detected
    CCB3458:[BMC]Active Directory should allow domain name and user name longer than 16 characters
    CCB3459:When updating BMC and BIOS, browser should limit search to .bin and .cap files respectively
    1507285344 - Upgrade libxml2 from v2.9.8 to v2.9.9
    2103650029 - Purley][S2600WF] the response is wrong for IPMI command Get DIMM Information (DIMM assert slot).
    2103649750 - [S2600ST] After mounting a virtual media via iKVM and selecting the Device again, it  will pop up a message "Exist an effective Connect from others ".
    16015595685 -[Utilities] [SDPTool-4.0.0] [Purley] - Stress failure on IVM
    2103648087 - [S2600ST] The device mount function on iKVM console menu Virtual Media > virtual storage can't be released.
    15010737507 -[Purley][S2600BP] BMC doesn't check the ISO/IMG header when mount virtual media via WebISO
    2103649160 - [Purley][ S2600WF / S9200WK ] The SEL has no description about  "SPS FW Health" on EWS.
    2103648972 - [Purley][S9200WK]  the response is wrong for IPMI command Get DIMM Information (DIMM assert slot).
    2103643376 - [S2600ST] [internal virtual media]After mount a internal VM in redfish and turn off iKVM,the mounted internal VM will be automatically unmounted in OS
    15010705608 -[S2600ST] [Redfish]After mounting the ISO through redfish and then reset BMC, the EWS and redfish will hang up.
    2103647672 - [Purley][S2600WF] Run DC/AC cycling with SP3RT040X16SPP Retimer card, port 1~3 connected nvme drives will be lost(drive LED is off). Fail rate 178/200
    15010697059 -[Purley][S2600BP] Session will reach to the maximum if repeat login and then logout the BMC EWS Web
    15010705258 -[S2600ST] [Redfish]When uploading a compressed file with Spaces or & in the file name via redfish, it only displays a file link in the OEM list.
    15010704983 -[S2600ST] [Redfish]When a zip or gz file containing a folder is uploaded via redfish,the timestamp of some files are displayed as 1935.
    2103648673 - [S2600ST] The policy suspend timers can't be disabled when change the Policy Suspend Timers from "Yes" to "No".
    2103648677 - [S2600ST] The ISO/IMA file can't be mounted in the Virtual Media > virtual storage > Device 2/Device 3 after mounting a folder in Device 1.
    2103648687 - [S2600ST] When select media type to ISO/IMG/IMA in virtual media over HTML5,all ISO/IMG/IMA files can't be displayed in the "ISO.IMG.IMA File" search mode.
    2103648682 - [S2600ST] Chinese and English EWS help information does not match.
    2103648097 - [S2600ST] After AC off SUT,the HTML5 KVM session doesn't give any prompts of disconnection.
    2103647974 - [S2600ST] The LAN channel1/2 are missing in the EWS->IPv4 Network Settings when power off SUT.
    15010550057 -[Purley]Unnecessary prompt pops up when upload 2048-bits certificate
    16015511567 -[SDPTool][Purley][Internal Virtual Media] Files in internal virtual media are accessible without BMC credential
    2103648046 - [Purley] [S9200WK] The EWS "NIC Information" and "Storage Information" can't detect any device with BMC 2.88.
    2103647923 - [S2600ST] The client IPv6 address is not displayed on the EWS->Current Users page when login the EWS with a dynamic BMC IPv6 address.
    1509875853 - [Purley][ Internal Virtual Media] Upload an encrypted file via Internal Virtual Media, the response is successful but no file can be accessed under OS
    2103644460 - [S2600ST] The warning dialog box have some English words and missing a double quotation mark in Chinese EWS when upload a new SSL certificate
    2103647768 - [Purley][S2600WF / S9200WK ] The BMC force update is failure with BMC 2.88.
    2103647740 - [Purley][S2600WF] the FTF FSC function test fail with BMC 2.88.
    22014214787 -MDR SendMsgBlock redundacy fail
    14012941881 -[S2600BP] : PSU on 3 Compute Module system chassis is reporting 0% current out and PS status indicating "Power Supply AC lost"
    15010173897 -[Purley][S2600BP] The complex password is abnormal with high level. (username: testuser2 / Password: 4rfv$RFVB)
    15010183182 -[Purley][ Internal Virtual Media] Update BIOS via EWS/Redfish, the mounted image will be automatically unmounted to BMC
    22014000969 -Incorrect BMC password logged in SEL; incorrect BMC user not logged in SEL
    14014263553 -NVMe drive information on HSBP3/Drive2 appears duplicated with HSBP3/Drive1 on BMC Web console
    2103644569 - Redfish: Use Postman tool to mount an "empty" txt file, it shows an extra string in the content of the mounted file
    15010201274 -[Purley][Point release][CCB3478/3457] Cannot set Bypass BIOS password flag by ipmitool via LAN1/2
    2103643169 - [Purley][S2600WF / S9200WK ]The Java Cert validity period is not match the release note for BMC v2.86
    1509724299 - [Purley][S2600ST] Sometimes the web  login event log is not logged in log file when login out EWS and login again.
    1509724203 - [Purley][S2600ST] The client IP address displays the abnormal address "#011 "privilege": #011 "4"".
    2103642881 - [S2600ST] The date and time is synchronized with the secondary NTP server when both the primary and secondary NTP server are configured
    1509725178 - [Purley][S2600WF / S9200WK ]The SOL log view is no display after running "ls -lR" command.
    2103643384 - [S2600ST][internal virtual media]The Oem list can only display 20 file links
    2103643380 - [S2600ST][internal virtual media]Failed to download files from the internal VM to OS
    2103643416 - Login to EWS with LDAP or AD users, there shows a new added "CPLD Update" option in the "Configuration" menu
    2103643309 - [S2600ST] SUT will fail to connect to the SSH console after change default port number to other port
    2103643393 - [S2600ST] it pops up an empty dialog box when replace a new certificate with 512 bits or 1024 bits in Chinese EWS
    2103643315 - [S2600ST] The SSH console is still active when disable SOL SSH in EWS
    2103642310 - [S2600ST] There is no link to channel 4 in redfish after enable HOST interface
    2103642381 - [S2600ST] The boot order can't be changed via redfish
    1508380544 - [SOW] BMC doesn't check the ISO image header when via HTML5 mount ISO image
    1509357645 - [Purley][S2600BP] User can't use Redfish to replace/upload a new certificate instead of current one
    1509357868 - [Purley][S2600BP]User can not use EWS to replace/upload a new certificate instead of current one
    1509411390 - [Purley][S2600ST] KVM "mouse mode setting" screen in ews shows exceptions
    1509439269 - [PURLEY] [BMC]lost dynamic IP after online update BMC 2.83
    1509442200 - [BMC][purley]mixed  up in get nvme information command
    1509464162 - #CCB 3402: [Purley][S2600BP] The file of size larger than 33M cannot be uploaded to the newly image created via Redfish internal interface
    1509486843 - #CCB 3402: [Purley][S2600BP] Unmount image is successful while the image is not mounted
    2103641466 - [Purley][ S2600WF / S9200WK ]The UI for "anonymous" user is abnormal and can't be modified in EWS
    2103641472 - [S2600ST]  The Mount type is missing NFS in web ISO help page
    2103641482 - [S2600ST] Alert events cannot all be selected when click "Check All" button in EWS->Configuration->Alerts page
    2103641549 - [S2600ST] There is an extra character '<' in the Date&Time help page in the Chinese EWS
    2103641607 - [S2600ST] There is a unknow item in EWS->Miscellaneous->Power Statistics
    2103641618 - [S2600ST] there is missing size limitation definition for Virtual Media Over HTML5 help page in EWS
    2103641755 - [Purley] [S9200WK] Open EWS -> Miscellaneous -> Power Statistics, it will pop-up a caution about NM initialization have problem. (BMC 2.83)
    2103641774 - [S2600ST]  KVM cannot open Via JRE due to JAVA certificate expired.
    2103641816 - [S2600ST] The NTP server IP can't be set successfully when NTP server IP is xxx.xxx.xxx.1~9 in EWS
    2103642274 - [S2600ST] Alert events cannot all be cleared when click "Clear All" button in EWS->Configuration->Alerts page page
    2103642310 - [S2600ST] There is no link to channel 4 in redfish after enable HOST interface
    2103642388 - [S2600ST] The EWS can't be opened when online update BMC from 2.48(upload new certificate) to 2.83
    1509261003 - [S2600BP][L9][Showstopper]Exit Air Temp (#0x2E) CRITICAL event: Exit Air Temp reports the sensor is high, critical, and going higher state.
    1509352602 - [Purley][S2600BP] ISO image mount via Redfish fail.
    1509363546 - [Purley][S2600BP]User can not use Redfish to upload CA certificate success
    1509118656 - [Purley][S2600ST] Get event log abnormal in EWS after updating BIOS
    14012450677 -[S2600WF] system reboots by interacting with OS Watchdog
    1507285344 - Upgrade libxml2 from v2.9.8 to v2.9.9
    1509247112 - [PURLEY][BMC][IPS 00615607]redfish alerting has power on/off backwards
    16013122517 -SDPTool [DEV] - SDR Upload issue
    16012935938 -[Purley][S2600BP]When BMC is running factory image, try to update BMC, BMC backup image instead of  primary image will  be updated.
    1509122866 - [Purley] [S2600WF] Can’t mount Virtual Media via Redfish.
    2103639108 - [Purley][ S2600WF ]It reports PSU1 FAN fail in SEL after AC cycle with BMC 2.48.f831fbb5.
    2103636406 - [Purley][ S2600WF ]The settings is no function for "BootSourceOverrideMode" in Redfish.
    22012657916 -jQuery vulnerability affecting Wolf Pass
    22012633532 -BMC EWS  iKVM over HTML5 disconnects, when Date or Time is selected and keypad '+' [scan code 79] is press
    2103635937 - Purley][ S2600WF ][900W DC] The PSU FW isn't match the BMC release note
    2103636054 - [Purley][ S2600WF ][900W DC] The blackbox data shows “This feature is not supported by any power supplies in the system” in the BMC debug log file.
    2103639150 - [Purley] S9200WK  Some MemoryLocation info show "null" when check it by Redfish
    1508892684 - [Purley][S2600BP] the warning message is incorrect while adding the same user name in EWS.
    1508871269 - User can set the same username as the password when user sets username separately which mismatch Password Complexity rule



===============================================================================
v2.86.2da97d3f -(Release version)
===============================================================================
    Upgrade kernel to 4.9.282
    CCB3388: Add one additional type to CCB 3245 to log AMT and PPR to SEL
    CCB3389: Need SEL for runtime PPR request
    CCB3402: Internal Virtual Media Image with file upload/download
    CCB3403: Redfish and EWS Virtual Media IMG & ISO support over NFS/SAMBA/Local
    CCB3245: Log AMT and PPR results in SEL
    15010010055 - [Purley][Internal Tool]cannot decrypt BMC debug log
    1509762682 - [S9200WK]The ca signed of the 4096-bit SSL certificate error when viewed in Redfish after successfully uploaded via EWS
    2103643101 - [S2600WF]There are 3 more AIC risers' FRU info in EWS after BMC update to version 2.86.2da97d3f
    1509732850 - [S2600ST]Restore BMC with checking "Keep User and LAN configuration",IPV4 Network Settings has abnormal behavior.
    1509732551 - [S2600ST]The primary port is changed when restore BMC with checking "Keep User and LAN configuration"
    1509675014 - [S2600ST]When set SMTP authentication Method to "Authentication after STARTTLS" or "Authentication over TLS/SSL session", the email alert function is failed.
    1509673621 - [S2600ST]The "PercentComplete" always is 60 when simple update BMC via redfish.
    2103642161 - [S2600ST]The“Advanced System Management Key”item in EWS shouldn’t be displayed in Purely project
    1509732255 - [S2600ST]There are four channel options in EWS->VLAN Settings->LAN Channel.
    1509724643 - [S2600WF/S9200WK]The mounted samba img file via Web ISO can't be opened or auto-detected by SUT OS.
    1509417498 - #CCB 3402: [S2600BP] With three virtual media devices mounted by HTML5,  mounting the new image created by internal interface via Redfish, the response is 200 OK and with no error info
    2103642152 - [S2600WF/S9200WK] The DIMM location is incorrect for "Mem err Sensor" SEL in EWS.
    2103642154 - [S2600WF/S9200WK] Change KVM(Secure) port value, open KVM /HTML5 KVM session and it will be disconnected automatically soon.
    2209858616 - Rapid power cycling on Wolf Pass Purley leaves power supply in status of 0x0980
    2103637171 - EWS: Occasionally after we login to the EWS, it will show a information "You don’t have privilege to perform this action." later
    2103637124 - S2600ST [Redfish]The static IPv6 address can't be set via redfish.
    1508593254 - [BMC EWS]some changes for BMC EWS - Intel LOGO, DCPMM to PMem
    2103637984 - [Purley] S9200WK After enable LAN failover with LAN1(primary channel)+ LAN3, the link status is down when remove LAN1 cable.
    1508659554 - When set Bonding between 3 LAN channels with Primary port = LAN1, the link status of channel1 is "DOWN" after removing the channel1 cable.
    1508664747 - [Purley]Complex password setting mismatch between BMC EWS and BIOS SETUP after updating SUP R0012 to R0013
    2103637125 - S2600ST The channel4 ip address can't be ping successfully when set bonding with Primary port as LAN1
    2103637217 - [Purley][ S2600WF ]The prompt info is incorrect when try to mount 4th vMedia device via vmviewer.
    2103637103 - [Purley][ S2600WF ]There is no Connection information in Connection Status History (Virtual Storage) when mount vmviewer vMedia.
    2103637104 - [Purley][ S2600WF ]There is no Disconnection information in Connection Status History (Virtual Storage) when un-mount vmviewer vMedia.
    2103636977 - [Purley][ S2600WF ] Web ISO settings can't be saved in EWS with BMC 2.48d.
    2103636978 - [Purley][ S2600WF ] There is no login failure prompt when Callback user try to login EWS with BMC 2.48d.
    2103636911 - [Purley][ S2600WF ] The Date&Time Help document content is not match the Date&Time setting page in EWS.
    2103636814 - [Purley] S9200WK  There is "Channel-2" in the IPv4/IPv6 Network settings when LAN Failover enabled.
    2103636789 - [Purley][ S2600WF ][SOW] There isn't "Save" option in EWS (Active Directory) Help information when login with Chinese language
    2103636787 - [Purley][ S2600WF ] The "HTTPS" is changed to "HTTP" in EWS (Security Settings) when login with Chinese language.
    1508442467 - [Design optimize] Consider to optimize the NTP date and time display in EWS
    2103636788 - [Purley][ S2600WF ] There isn't "Port Settings" option in EWS (Security Settings) Help information when login with Chinese language.

===============================================================================
v2.48.ce3e3bd2 -(Release version)
===============================================================================
    CCB3158: Integrate BMC features developed by InSyde
    CCB3275: Storage/Networking as SMBIOS extensions and displayed in BMC via Redfish/EWS
    CCB3059: 900 W DC Power Supply
    CCB3156: Add NTP and World Clock to BMC
    CCB3209: Option to retain user info and IP settings after firmware factory reset
    CCB2448: [BIOS+BMC]Speed Select support in S2600WF via RSD FW Extensions Spec
    CCB3109: BIOS Settings should persist in BMC after BMC reset
    5354047: Using a Mix of Vendors' 2666 MHz DDR4 DIMMs May Cause Correctable Errors or a System Hang
    2103636075 - [S2600ST]New users created before enabling host interface cannot log on to channel 4's EWS.
    2103636299 - [S2600ST]the deleted user network privilege still exist in channel 4 when delete a user via channel 3
    2103636301 - [S2600ST]The new user 's network privilege is invaild in channel4 when create a new user in channel3 with same ID
    2103637120 - [S2600ST]The update message is shown as "BIOS" when update ME FW via redfish
    2103637174 - Embedded Web Server: There is a type error in the help document of the "Security Settings" option
    2103637181 - Embedded Web Server: There is a type error in the "Miscellaneous" ---> "NM Configuration" option
    2103637119 - [S2600ST]There is a warning messages when click on the BIOS Configurations page immediately after logging in to the EWS.
    2103636933 - [S2600ST]The KVM delete button on the current users page in the EWS is invalid
    2103636982 - [S2600ST]The "+-" button of the KVM number bar on the Current Users page in the EWS is invalid
    2103636945 - [S2600ST]The information of the channel3/4 are lost in EWS when SUT have 4 NIC port in BIOS NIC Configuration
    1508422943 - [SOW] The display of WebUI host interface(IPV4 page) is not beautiful enough
    2103635503 - [S2600ST]The contents of the help page for the NIC/Storage information are not displayed correctly.
    2103635530 - [S2600ST]The warning messages is not displayed correctly when restore BMC with checking "Keep User and LAN configuration".
    2103635541 - [S2600ST]SDR version will roll back to factory shipping version "D2.48" after restore BMC with checking "Keep User and LAN configuration"
    2103635552 - User can add duplicate AD group name with different network privilege via EWS.
    2103635560 - The Network Privilege of the role group show "Reserved" in "Active Directory Settings" page when add a "No Access" role group in Active Directory.
    2103635568 - [S2600ST]The theme display abnoramlly for the storage information page in EWS
    2103635708 - [S2600ST]The drop-down menu for the role group privileges of AD in the Chinese EWS is shown in English.
    2103635717 - [S2600ST]When enable NTP server and set primary NTP server, the warning message is empty or "undefined" in the chinese EWS.
    2103635730 - [S2600ST]The type for web console show as "N/A" in the "system"->"Current Users" page
    2103635740 - [S2600ST] the "vMedia Usable" is shown "NO" in the "System" ->"Current Users" page when mount USB device or 'ISO image' as virtual storage in the KVM session
    2103635746 - [S2600ST]the "vMedia Usable" still show "Yes" in the "System" ->"Current Users" page when pull out all  the HTML5 virtual medias
    2103635748 - [S2600ST]The number of event entries in the "Sensor Specific Events"/"BIOS Generated Events" event category is incorrect
    2103635803 - [S2600ST][Redfish]When use POST method to create the 6th subscription,the "code" and "message" info in the response are not displayed correctly.
    2103635845 - [S2600ST][Redfish]When plug out the dedicated LAN cable,the "SpeedMbps" is shown "4294967295" in redfish
    2103635849 - [S2600ST][Redfish]There are two links to the ethernet interface of channel3 in redfish
    2103635865 - [S2600ST][Redfish]The response messages display abnormally when use post method to update BMC/BIOS/ME/debug FW via redfish
    2103635922 - [S2600ST][Redfish]The BMC/BIOS/ME FW can't be downgraded in BMC v2.48b via redfish.
    2103635924 - [S2600ST]It pops up a warning message when check "Enable HOST Interface".
    2103635996 - Embedded Web Server: The title bar of "NIC Information" and "Storage Information" still show English when the Web browser set to Chinese language
    2103636002 - Embedded Web Server: There is a typo error on the “System Information --- Storage Information” menu
    2103636004 - Embedded Web Server: The help documentation of the “NIC Information” and “Storage Information” shows the “DIMM information” help documentation
    2103636005 - Embedded Web Server: When mount a media to SUT, on the “Current User” option, the “vMedia Usable” option still shows “No” string.
    2103636083 - [S2600ST]The HI BMC IP can't be modified when enable LAN failover and set the primary LAN channel to channel-1.
    2103636295 - [S2600ST][Redfish]The behavior of user with different privilege in Redfish doesn't same with EWS.
    2103636303 - [S2600ST][Redfish]The "EndTime" of simple update FW is displayed as "1970-01-01T00:00+00:00" when simple update FW via redfish.
    2103636306 - [S2600ST][Redfish]The "Messages" of simple update FW is empty when simple update FW via redfish
    2103636461 - Enable the complex password and set the password complexity to "Low", it still can use the "qw12!@" string to the user password
    2103636476 - Embedded Web Server: The "Enforce Password History" value does not match with its help documentation
    2103636525 - [STPS2600STThere is a spelling error "interfac" in warning messages when check "enable Host Interface" in Chinese EWS->configuration->IPv4 network or IPv6 network
    2103636530 - [S2600ST]The "Virtual Media over HTML5" function failed when change HTTPS port to login the EWS
    2103636533 - [S2600ST]debug console will pop some error messages when click "IPv4 Network"/"IPv6 Network"/"Web ISO" page in the EWS
    2103636537 - [S2600ST]The primary port can't be modified when issue ipmitool command again to change the primary port.
    2103636691 - [S2600ST]The example password should not allowed in the help page for high complex password
    2103636724 - Embedded Web Server: It can not mount the media through the device 1, device 2, device 3 and device 4 options concurrently
    2207974933 - WebISO feature saves remote system credentials in plain text
    2103628332 - OFU Utility: When use Gold 6248 2.5GHz CPU, update both BIOS and BMC, it always generate the “Exit Air Temp” UNC and UC event log
    2103633732 - [S2600ST]The KVM session of the shared IPv6 NIC will be closed automatically after press F10 to save the BIOS setup.
    2103633363 - Embedded Web Server: Occasionally when you login the EWS with correct username and password, the browser will kick you out of the EWS immediately
    2103633665 - [S2600ST]It keeps repeating update when update the ME FW via OOB under deny all mode.
    1508134722 - [Redfish]It keeps repeating update when update the ME/BIOS FW via Redfish under deny all mode.
    2103633628 - [S2600ST]The SUT will hang up or reboot automitacally after not connectting to the WEB ISO server.
    1508103258 - BMC Debug log smbios type0 stores wrong BIOS version information

===============================================================================
v2.48.89b32e0d -(Release version)
===============================================================================
    2103633517 - [S2600ST]The debug console will print "TRACENOW: PIA_GetModuleRecord:801: -NO PIA record for module 0x79 121" info.
    2103633467 - On-line update the BMC_2.47.7d70c8d3, it can not show the correctly version string in BIOS UI or by "cmdtool 20 18 01" get device id command
    2103632933 - It can not update the BMC twice with BMC_2.45.15da7ca0 version
    2103633043 - [S2600ST] The sidebar font on the BIOS configurations page will be grayed out after logout and login the EWS
    2103633229 - [S2600ST]There aren't the SDR version info in the event logs of FW update status after updating FRUSDR.
    2103633232 - [S2600SST]Sometimes online update BMC v2.46 failed.
    2103633335 - There is a type error in the EWS ---> Configuration ---> "KVM & Media" menu
    2103633350 - EWS: The option menu in the EWS --> BIOS_Configuration page show the "Grey" color
    2103633284 - [S2600ST]The OEM EWS version infomations are not shown in the event log of OEM EWS FW update status.
    2103633142 - [S2600ST]After change any of the options in the Security settings and save them, the web will automatically refresh and skip to the system page.
    1507327283 - The primary LAN channel of Enable LAN failover doesn't work
    2103632922 - Update the BMC_2.45.15da7ca0, the "PSOC" and "HDD Status" sensors show "Not Available" in the EWS
    2103633039 - [S2600ST] The Chinese Web console is empty on the BMC v2.45
    2103633122 - It returns the "0x82: Unknown" response information when execute the raw command "raw 0x30 0x67 0x01"
    1507962138 - Add FD update support in Redfish
    1507916073 - EWS BIOS Configuration OOB Test: There is no content for the "System Event Log" option	      
    CCB2434i: Implement 0xD5 return code when user requests power on and system is already on

===============================================================================
v2.42.d0b788a4 -(Release version)
===============================================================================
    1507662630 - Redfish - The action to update BIOS via Redfish fail in Purley_2.34.c46c1f89
    2103631429 - When enable the LAN Failover and bond all the 3 channels, then it can not ping through the BMC
    1307167502 - RedFish POST action - when appying Power Off to already Powered Off system BMC responds with inproper status code and message
    1507238116 - Occur Redfish Schema Errors using DMTF test
    1507685098 - Redfish - The status code return 200 OK when the number of simultaneous subscriptions exceeding the limit of the implementation
    1809282007 - POST with FW Update action and empty payload returns incorrect return Status Code
    2103630325 - There are many code descriptions missing under the EWS->System Diagnostics->Post codes
    2103630330 - When change Legacy VGA Socket to 0x02(CPU Socket 2) in the EWS, the SUT will always reboot automatically.
    14010728205 - System restarts when FAN_TACH is 0 RPM on customer's chassis environment
    1507683048 - Redfish - When creating a new user successfully, the status code should return 201 Created, while actually return 200 OK
    2103630752 - Redfish - Get an error of use DELETE method  to send the request 4th times with below link "https://SUT IP/redfish/v1/EventService/Subscriptions/{ID}"
    1506731715 - BIOS Configuration - Some variable show in EWS BIOS configuration but can’t map it in BIOS setup menu.
    1507465888 - The EWS shows Exit air temperature unknwon
    1809195649 - RedFish Patch action - Indicator LED "Lit" request response is invalid
    1809203869 - RedFish Patch action -changing BootSourceOverrideTarget on ComputerSystem response is invalid
===============================================================================
v2.37.1f190479 -(Release version)
===============================================================================
    1809195649 - RedFish Patch action - Indicator LED "Lit" request response is invalid
    1809203869 - RedFish Patch action -changing BootSourceOverrideTarget on ComputerSystem response is invalid
    2103630337 - S2600ST System Boot Timeout Value is not match BIOS setup menu
    1507662630 - Redfish The action to update BIOS via Redfish fails
    1507662518 - Redfish The action to update BMC via Redfish raises “500 Internal Server Error” 
    1507325042 - Redfish S2600BP The value of attribute "Legacy USB support", "Port 60/64 Emulation", "Make USB Devices Non-Bootable" can be modified when they are grayed out in BIOS and EWS
    2103629456 - S2600ST doesn't show primary BMC LAN’s MAC/IP infos in EWS->IPv4/6 network after setting the primary LAN channel to channel 2 or 3.
    1507313235 - Redfish S2600BP The value of attribute "Force Password Support" can be modified without setting administrator password
    1809209424 - RedFish POST action - when appying Power On to already Powered On system BMC responds with inproper status code and message
    1507623138 - Purley BMC SSH-SOL port 66 security vulnerability --- request to replace weaker  algorithms with stronger ones
    1507429379 - The BIOS SDR in the frusdr package doesn't align with BIOS EPS
    1507609800 - Redfish In BMC 2.28 and later (2.29-2.32), log messages for FW update only show "OEM"
    1507313188 - Redfish Provide PATCH method, but all properties are read only
    2103629492 - S2600ST primary LAN channel of Enable LAN failover doesn't work on IPv6 network.
    1507517589 - Redfish The action to update the target image via Redfish raises “400 Bad Request”
    CCB2762: [BIOS/BMC Q3'19] BIOS requried support for PSME 2.4 including RSD 2.4 extensions
    CCB2880: BMC FW Cipher Suite Policy Control
    CCB2572: Mount local file folder by RKVM, only JAVA
    CCB2717: [BMC Q3'19] Support SSL upload via Redfish
    CCB2764: Periodic heartbeat for reporting health
    CCB2767: [BMC Q3'19] Redfish - Enable BMC LAN configuration
    CCB2768: [BMC Q4'19] Redfish - Download debug log
===============================================================================
v2.22.59c3b83a - (Release version)
===============================================================================
    1507299182 - The crash dump json file in the BMC debug log miss some part
    1607818386 - BMC login problem by ipmiutil and EWS if the password length is longer than 16 bytes
    1507285420 - Upgrade Curl from 7.64.0 to 7.65.1
    2103628329 - EWS: It can not send the SNMP alert packages to destination IP
    1507357494 - [Redfish]Unable to change property "BootSourceOverrideEnabled" from "Continuous" to "Disabled"
    1607346326 - [Redfish] Username or password length is abnormal when create or modify
    2208243530 - BMC Session ID hijacking flaw
    1507373053 - The latest BMC has no event log on EWS
    1607346326 - [Redfish] Username or password length is abnormal when create or modify
    1507343404 - [S2600WF][KCS]Cannot change BMC KCS mode in BMC force-update mode.
    CCB2546: [Redfish] Add additional eventing to Redfish support
    CCB2645: Support virtual media
    CCB2570: Complex BMC Password
    CCB2700: Point release to resolve BMC network problem from lan disabling under BIOS and MAC address problem
===============================================================================
v1.93.870cf4f0 - (Release version)
===============================================================================
    1504762562 - [S2600BP LCR] SEL Log has PS1/PS2/P1/P2/HDDs/Pwr Unit Redund Status Assert during DC cycle(appear once)
    1506985125 - BMC slow response and EWS can't login during DC/reset cycle test.
    1606875819 - Ipmitool command random lost function  during DC cycles test and sel log show redundant "bad user PWD"  information(EWS can be login).
    2103622412 - During the HSC FW update processing, execute the cmdtool 20 c0 38, it could not return response data until the update completed
    2103623745 - EWS BIOS Configuration OOB Test: When set the SerialOverLan option to enabled, the SUT will continuously reboot
    2103625073 - The "BIOS configurations" items not gray out when login with user privilege
    2103625221 - The System Macro key "PrntScrn" and "Alt+PrntScrn" have no function in iKVM over HTML5.
    2103625242 - Alert Email of EWS can't save via Chrome/Firefox/Safari
    1507016738 - [OOB BIOS Configuration]Some variables have the same value when we don't change the default "Select a BIOS Variable" in EWS.
    2103624478 - Description in HELP page isn't corresponding to the actual Chinese EWS page
    1507018625 - Fan 6 Present show unknown from EWS and disabled from ipmitool sensor list.
    2103625163 - RMCP cipher suite will be disable after offline BMC then online update BMC
    1507004031 - Security for missing or insecure "Content-Security-Policy"
    1506996790 - [S2600ST]No alert SMTP mail/SNMP trap received  after triggering the alert of "intel temp overheat shutdown"
    2103624840 - [S2600ST] Alerts and Alert mail  setting in EWS Configuration will be lost after click refresh button
    2103625101 - Alert Destination can't be saved via LAN3 in WFQ board
    2103625071 - The message display incorrect after enable syslog in Chinese EWS
    2103625044 - Copyright display incorrect in EWS
===============================================================================
v1.90.0cf6e935 - (Release version)
===============================================================================
    1506985125 - BMC slow response and EWS can't login during DC/reset cycle test.
    1507018625 - Fan 6 Present show unknown from EWS and disabled from ipmitool sensor list.
    1306124875 - [S2600BP and S2600ST] BMC EWS can not login.
    1504691171 - [S2600BP LCR]BIOS/System Management Software controller time are not synchronous with BMC time in EWS event log
    1506999387 - DNS setting can't be changed
    1606903509 - FRUSDR update via EWS failing on one system with AIC cards for BMC 1.88a (1.88.2d047b47)
    2103624411 - [S2600ST_OOB BIOS Configuration] BIOS Variable Value cannot be changed Via EWS OOB BIOS configuration
    2206618701 - login to EWS and observe the Configuration->SDR Configuration the Processed Tags Copyright (c) 2018 messages should be 2019
    2202811235 - [S2600BP] [Q4] BMC reports PSU AC input lost and later regained
    2103624862 - VLAN channel shows "Unknow" when login EWS with operator privilege.
    1506761317 - [S2600BP LCR]Sel log appear Power Unit Failure detected - Power supply failure detected - Asserted during AC cycles.
    1506956417 - FRB2 WDT handling on BMC FW(1): BMC does not respond to FRB2 mailbox bit in time.
    1506983635 - [S2600BP LCR]SUT can't auto power on during the DC cycling and  it cannot auto power on in the next cycle.
    1606876077 - FRB2 WDT handling on BMC FW (2): Disabled FRB2 WDT when received GPIO from BIOS.
    2103625010 - Connect the "PWRGD_PVDDQ_CPU0_ABC_R"  or "PWRGD_PVDDQ_CPU1_ABC_R" signal to the ground, it could not generate the 1-5-1-2 beep code
    2206474697 - S2600WF SUT,  with DDR4s in a 1DPC mirror, configuration, injecting a mirror failover, causes an incorrect DDR4 slot indication in the SEL log.
    2103624841 - Spell error in keyboard Macro when KVM over HTML5 in EWS.
    1506132909 - [S2600BP LCR]BB CPU1 VR Temp /BB CPU2 VR Temp sensors show no reading when run AC cycles and can't recovery within 300s
    1506132916 - [S2600BP LCR]Mem 1VRD Tem/Mem 2 VRD Temp sensors  show no reading when run AC cycles and can't recovery within 300s
    1506769587 - PS1 Curr Out %/PS2 Curr Out %/PS1 Temperature/PS2 Temperature/PS1 Input Power/PS2 Input Power no reading during  AC test and can't recovery within 300s.
    2206474488 - [BMC CTF]  BootFlagCmds BootSetOptions Buffer Overflow on the heap
    2206474502 - [BMC CTF]   memory corruption in Redfish parse URL
    2206474881 - [BMC CTF] Hidden NM configurations can be added that are not visible from WebUI list
    2103624450 - The login screen of EWS page shown abnormal with OEM customized image
    2103624715 - No warning message displayed after opening 5th EWS sessions.
    2103624749 - No warning message displayed after opening 5th EWS session.
    2206192060 - [PS - Scandium] Debuglog command fails with PS Script 2.09
===============================================================================
v1.74.ee39402a - (Release version)
===============================================================================
    1506764699 - OEM Get reading command isn't workable
    2205369358 - [S2600BP] Exit Air Temp SEL events seen during OS Install and AC Cycling
    1209275701 - PCIe register access from host can be remapped to any base address into BMC address space.
    2202523214 - SPS FW Command Filtering
    2205369288 - [S2600BP] OpenIPMI driver fails to detect BMC on startup
    1506759784 - [redfish]UpdateMe Error with biospack 0D010125
    2205425827 - Baseboard FRU information missing with Redfish Schema
    1506749803 - [iKVM over HTML5]Up and Down key can control HTML5 iKVM session menu and BIOS setup menu in the same time
    2103623408 - [S2600WF] The threshold info will disappear after change sensor owner.
    2205369358 - [S2600BP] Exit Air Temp SEL events seen during OS Install and AC Cycling
    1506755754 - [OOB BIOS Configuration]the actual value is different with the value you click to change after do change value steps
    1506745023 - [iKVM over HTML5]Virtual media will be terminated when refresh the session of Virtual Media over HTML5 by press "F5"
    2205467333 - [S2600WF]Control BMC Services command sometimes cannot disable BMC Services
    2103623431 - [S2600WF] The button of Launch KVM over HTML5 not gray out when use operator user.
    2103623444 - [S2600WF] PSU redundancy lost event not showing after remove power supply cable
    2103623437 - [S2600BT] PSU redundancy lost event Not showed after remove power supply cable
    1506731715 - [OOB BIOS Configuration]Some variable show in EWS BIOS configuration but can’t map it in BIOS setup menu.
    2204837267 - Redfish ComputerSystem node has invalid field
    1506745202 - [iKVM over HTML5]When changed the language from English to Chinese, there always some English characters in the session
    1209275701 - PCIe register access from host can be remapped to any base address into BMC address space.
    2202523214 - SPS FW Command Filtering
    2205369288 - [S2600BP][Q2] OpenIPMI driver fails to detect BMC on startup
    2205425827 - Baseboard FRU information missing with Redfish Schema
    2103623352 - S2600BP: Use BMC_1.71 or 1.72 and S2600BPS mainboard, after updating the FruSdr_1.37, some sensors in EWS shows "unavailable" or incorrect reading
    1506132921 - [S2600BP LCR]NVME 1 Therm Mgn sensor  show no reading when run AC/DC cycles and can't recovery within 300s
    1506745145 - [iKVM over HTML5]It will show "SecurityResult Failed(Retry after 30 sec or iKVM reset)" if we launch the 5th ikvm session
    2007464975 - [S2600ST] IPMI command to get fan speed not working on CPU fans
    2205369288 - [S2600BP][Q2] OpenIPMI driver fails to detect BMC on startup
    2103623344 - [S2600BT] EWS help page show 404 about Virtual Media over HTML5
    2205425827 - Baseboard FRU information missing with Redfish Schema
    1506731715 - [OOB BIOS Configuration]Some variable show in EWS BIOS configuration but can’t map it in BIOS setup menu.
    1506659800 - [HTML5 KVM] No error or warning message displayed when 5th HTML5 KVM is opened, but the session is blank.
    1506109146 - CCB1964(PSME 2.2 support in BMC 1.57) doesn't align with PSME restful API specification
    1506129772 - Q3'18 #CCB2447 [Intel Xeon Scalable BMC]HTML5 support
    1506659800 - [HTML5 KVM] No error or warning message displayed when 5th HTML5 KVM is opened, but the session is blank.
    1506706272 - [S2600BT]Access still be denied after unmounted USB disk from rKVM
    1506733454 - [S2600WF]Seneor report PWR Unit Redundancy lost with FCT SDR
    1506733968 - [redfish]URL spelling error ,bios settings
    1506745202 - [iKVM over HTML5]When changed the language from English to Chinese, there always some English characters in the session
    1606376899 - [HTML5 KVM] 'Options' and 'User List' menu are always greyed out in the HTML5 KVM
    1606376909 - [HTML5 KVM] 'Defined Macros' option disabled in Keyboard Macro menu, hence the user added keyboard macros in EWS->Configuration page also not getting reflected.
    1606376917 - [HTML5 Virtual Media] Java Virtual media supports 4 devices whereas HTML5 Virtual media supports only 3
    1606652628 - FRUSDR update via EWS fails with BMC 1.71
    2103623223 - [S2600BT] No "start" and "completed" in FW update event description
    2103623248 - The warning messages of "restore system defaults" doesn't match test case.
    2103623309 - [S2600BT] SDR parse failed after press "Parse" button in EWS SDR configuration page.
    2103623322 - On-Line Update the firmware (such as BMC or ME), the event log does not show the "update process" clearly
    2103623344 - [S2600BT] EWS help page show 404 about Virtual Media over HTML5
    2205425824 - Unable to enable SSH using Redfish Schema
    2204837759 - Redfish DMTF schema does not have a Bios/Settings XML field
    1504742896 - Q3'18 #CCB2202[BMC]Need log to track user/IP logins to BMC
    2202470727 - [S2600WF] PSOC on rear HSBP becoming corrupted
    2103623271 - Use Windows Client PC, mount a USB Flash then un-mount it later, the USB Flash could not be accessed on the Client PC

===============================================================================
v1.60.56383bef - (Release version)
===============================================================================
    1407264248 - [S2600BP] BMC is not reporting redundancy lost by clearing STATUS_INPUT flags from PSU
    1506122908 - [S2600WF]The AIC Product Name information returned is replaced by part MAC address of the third cards when the connected AIC Cards are greater than two.
    1506123447 - BMC User and Network setting will change to default after online update BMC to 1.59.ba077703&AC cycle
    1505567118 - [S2600BT]SSL/TLS use of weak RC4 cipher
    1505573379 - [S2600BT]Birthday attacks against TLS ciphers with 64bit block size vulnerability (Sweet32)
    1506114971 - [S2600ST] Chinese characters are not displayed properly in Event Log page while login Web in Chinese
    1506118999 - Q2'18 #CCB2434 [Intel Xeon Scalable BMC]Implement 0xD5 return code when user requests power on and system is already on
    1506119149 - Completion code for OEM get sensor reading(platform power consumption) isn't right when no ADM chipset is available.
    1506123447 - BMC User and Network setting will change to default after online update BMC to 1.59.ba077703&AC cycle
    2103620859 - [S2600BT] Media will be unmounted after boot into OS
    2103621752 - [S2600WF] Media will be unmounted after boot into OS
    2103622022 - [S2600BT] Event log page can't be read via IE browser
    2103622102 - [S2600WF] The Event Log shown abnormally on EWS after pressed NMI Button.
    2103622115 - EWS: Use firefox browser to check the system event log, all the information is unreadable code unless clearing the browser cache
    2103622127 - EWS: There is a unreadable character in the system event log
    2103622137 - EWS: When set the language to Chinese, the event log information show unreadable characters
    2103622142 - EWS: It could not establish the session to EWS after setting the https port to customized value
    2103622186 - [S2600BT] BMC can't stuck in Safe mode after execute 4 times BMC watchdog
    2103622241 - [S2600BT] HTTPS Port can't login from other values after HTTPS Port modify 8443
    2203123584 - Remote ipmitool chassis power off returns error when chassis is already off.
    2203745825 - [KVM/VM] Virtual Media redirection fails installing OS and console spews SSL errors
    1504766995 - [S2600BP LCR]Sensors are not correctly display in one cycle when run AC/DC cycle test
    2103622260 - [S2600BT] Enable Remote Debug function command response incorrect via BMC Shared LAN IP
    1506118927 - Q2'18 #CCB2427  [Intel Xeon Scalable BMC]Increase KVM timeout to 1+ minutes
    2103614048 - EWS User Enable is blank
    2103621847 - [S2600BT] EWS some information will be abnormal via IE browser
    2103621983 - [S2600ST] There is no display information for DIMM and FRU in system information while login Web by using IE
    2103622082 - [S2600WF] Event log page can't be read via IE browser
    2103622113 - IE: After updating the BMC_1.58.eafa53ef, it could not show the system event log in EWS
    2202696827 - BMC EWS GUI SEL Fails to Finish Loading
    2203669681 - BMC Web console fails to show FRU and Memory information after update to SUP x0135
    1506077858 - [S2600BP LCR]Event log “Sensor failure—HSBP temp -- Asserted” during AC/DC/linpack test
    1504651008 - Sometimes system will generate an abnormal event log about “Sensor failure—HSBP temp -- Asserted” and status LED show green blinking
    220857900 - [S2600BP] 17 of 3456 nodes  ( 9 of 864 system) failed EST for intermittent BMC FW Health unable to read HSBP Temp sensor
    2103620331 - [S2600BT]profile can't be shifted by the riser number
    1505815184 - RKVM can't launch if we have setup port forward from external IP address to internal address
    2103622022 - [S2600BT] Event log page can't be read via IE browser
    2103621764 - [S2600BT] Network configuration will be abnormal on EWS after stress VLAN ID test
    2103621770 - [S2600WF] Network configuration page can't worked on EWS after stress VLAN ID test
    2202676945 - Get Security Version Information returns 00 00, hence no way to know the security revision of the firmware.
    2202770366 - ReadSelfTest command response not as expected and the command missing in EPS
    2202843495 - [KVM/VM] Java pegs the CPUs on Linux when kvm/virtual media loses connection to the BMC
    2203284099 - [KVM] - The TLS ciphers used by KVM (port 5902) and USB (port 627) allow weak encryption algorithms and ciphers
    2103621726 - [VMviewer] The History will shown duplicate messages after mount image files via VMViewer.
    2103621885 - EWS: Use IE browser, it could show the baseboard serial number string
    2202676945 - Get Security Version Information returns 00 00, hence no way to know the security revision of the firmware.
    2202696827 - BMC EWS GUI SEL Fails to Finish Loading
    2202731630 - [EWS] Lower privilege user (operator, user) can update session timeout for all users
    2203103848 - [Redfish] Account Service with user privilege leaks user information
    1504745080 - [S2600BP LCR]PS1/PS2 Input Power/Curr Out %/Temperature sensors show no reading or disabled and need unplug/plug nodes to recovery during AC cycling
    2202314699 - RSD 2.2 -TPM setting by PSME via POST command is not implemented yet
    1504716901 - It takes more than 10 second to get MTT CPU1/2 sensor
    2103621780 - The name of menu bar is incorrect on KVM
    2202485388 - Redfish - Discrepancy in PATCH body for  BootSourceOverride Action
    2202039060 - MSM PS script 1.13. issue with "debuglog" command
    2103620859 - [S2600BT] Media will be unmounted after boot into OS
    2103621667 - [S2600BT] The login screen of EWS page shown abnormal with OEM customized image
    2103621528 - [S2600BT] The login screen of EWS page shown abnormal
    2103620331 - [S2600BT]profile can't be shifted by the riser number
    1504707042 - Q1'18 #CCB2201[Intel Xeon Scalable BMC]Need OpenLDAP support in BMC
    1504765942 - Setting IPv4 Network is abnormal via EWS
    2103621229 - [S2600WF] The Alerts Destination configuration can't save on EWS when SUT no install OCP card.
    2103621677 - [S2600BT] Setting IPv4 Network is abnormal via EWS
    2103621719 - [S2600BT] Alert Mail delivery failed via EWS settings
    2202534178 - [redfish] several properties are missing from /redfish/v1/Managers/BMC/EthernetInterfaces/1
    1504749848 - Q2'18 #CCB2257 Q2'18 [Intel Xeon Scalable]Add OEM command to provide global reset capability for Syscfg(Graceful shutdown, then automatically power on after powering off)
    2103621462 - [S2600BT] The SEL description is incorrect when trigger the FPGA CATERR.
    2103621525 - Failed in setting up SNMP alert destination with IPv6 address in the SUT's EWS
    2103621597 - [S2600BT] The SEL doesn't "Power off/down" event logged after DC Cycle.
    2103621603 - [S2600WF] User 1(Anonymous) can't be modify in EWS users page.
    2202039060 - MSM PS script 1.13. issue with "debuglog" command
    2202534178 - [redfish] several properties are missing from /redfish/v1/Managers/BMC/EthernetInterfaces/1
    2103621661 - [S2600BT] There are no thermal trip/IERR deasserted events logged on SEL
    2103621582 - [S2600WF] The sensor type of SMI timeout is not match with EPS 1.12
    2202525692 - [redfish] AssetTag is missing from Systems/{ID}
    1504743210 - EWS will auto login out after click "Clear Event log", and event log can't be cleared by EWS
    2103621502 - [S2600BT] EWS will be forced to logout when click Clear Event Log.
    2103621528 - [S2600BT] The login screen of EWS page shown abnormal
    2202565737 - BMC SEL Incorrectly Reports DIMM Slot with Failed DIMM in CPU2 Slot C1
    2006708660 - BB P1- P2 VR Temp issue during AC Cycling
    2103621270 - Unusual thermal critical events in JBOD BMC log during QRC (AC/DC/Warm reboot) cycling test
    2103621381 - [S2600BT] There are two OEM Sensors in EWS sensor type category
    2103621464 - [S2600BT] EWS will be forced to logout when use Operator and User privilege
    2201838395 - Redfish - Unable to set BootOverrideTarget to Pxe when the BootOverrideMode is UEFI.
    2202420277 - DIMM Enumeration in BMC GUI SEL Display for ECC Entry is 0-based
    2202468321 - KVM window can not be closed by clicking "trash can" symbol in the Web console
    2006679703 - Redfish:  ResetCycle command fails to send graceful restart.
    1504720141 - Fan values differ substantially before and after cold reset of the BMC under performance mode
    1504731495 - flash BMC will occur 'Error Finish BMC update transfer failed.' when online update BMC 1.48.da6db8b3 to BMC 1.48.da6db8b3
    220891332 - S2600WF BMC GUI Fails to display P4600 NVMe information
    1504707051 - Q1'18 #CCB2118 [Q1'18 Intel Xeon Scalable BMC] Need to support NVMe 1.2 VPD to correctly identify Cliffdate, Fultdondate and future drives
    1504711379 - [S2600BP LCR]HSBP_PSOC sensor shows no reading when run reboot test.(recovered later automatically)
    1504720124 - [S2600BP]BMC release-notes doesn't contain the new type PSU(PSSF222201A  04A)
    2006710682 - Chassis ID LED needs to be pressed twice to turn off when turned on in EWS
    1504706586 - [FTF]Get DIMM offset command returned unexpected completion code 0x01 during FSC AutoProfileFunc.tcl test
    1504707060 - Q1'18 #CCB1954 [Intel Xeon Scalable BMC] Remote debug over PECI
    1504718239 - Customize EWS image update failed
    2103620599 - EWS: Occasionally it shows "Exist an effective connect from others" or "Media has been unmounted from others" while mount or unmount the virtual device
    1504473313 - [FTF]Fan Boost value do not reach expected value  during running FSC BAT_FSC_Functional_004.tcl test
    1504696854 - Redfish URL redfish/v1/Managers/BMC/NICs NOT align with Redfish Spec
    1504696869 - Redfish API GET redfish/v1/Managers/BMC/ response should contain ServiceEntryPointUUID element
    1504699916 - 2130W PSU predictive failure on S2600BP from across customers and across sites
    1504706039 - Redfish API unable to read system network interfaces
    1504707049 - Q1'18 #CCB2140 [Intel Xeon Scalable BMC]Get CPU temperature displayed in degree Celsius after executing an “ipmitool sensor”
    2006709919 - IPMI OEM type record cannot use 0x20 on generator ID field
    2103620363 - The ME sensor should not be define in SDR 1.41 file.
    2103620840 - BMC debug console shows abnormal messages about "PcieSwitch_sensors_thread".
    2103620851 - [S2600BT] Failed to update configuration of NM by EWS.
    2201981916 - BMC firmware Update to 1.47.e54761ed clears the BMC LAN Settings
    1604603941 - [FTF]It will report a failure “Unable to program SDR record#52” during SDR and FSC FTF test.
    2103617028 - [S2600WF]Description in HELP page isn't corresponding to the actual EWS page
    2103620512 - [S2600BT] The Power Control shows incorrect in the KVM menu bar
    2103620737 - [S2600BT] The being setting NM policy of memory cannot delete by EWS
    2103619818 - [S2600BT] NM configuration Couldn't display the memory power policy in the EWS
    1504627444 - #CCB2006: [Cloned CCB 2003] [2nd Generation Intel(R) Xeon(R) Scalable]ERROR_N[1,0] connection request to BMC
    1604595437 - Several Redfish GET commands return errors
    2006689963 - VR-Watchdog - Voltage Fault issues running DC_Cycling
    2006709004 - [S2600BT] Wrong date in event logs with WW51 BKC
    2103617840 - [S2600BT] The time stamp in sellog is incorrect after offline flash BIOS , BMC , set clear CMOS jumper and remove battery.
    2103619526 - It generates some incorrect event logs in the AC cycle stress test
    2103619725 - The sensor reading of "System Airflow" sensor in slave node show 0 CFM.
    2103619818 - [S2600BT] NM configuration Couldn't display the memory power policy in the EWS
    2103619846 - [S2600WF] The VFP LED cannot be changed via SM signal command under MTM 1 or 2 mode.
    2201187649 - S2600WF LNET Router BMC sometimes reports Voltage Fault State - Asserted/Deasserted events during DC and OS cycling

===============================================================================
v1.43.91f76955 - (Point Release for JAVA certificate expiring)
===============================================================================
    1504745080 - [S2600BP]PS1/PS2 Input Power/Curr Out %/Temperature sensors show no reading or disabled and need unplug/plug nodes to recovery during AC cycling
    1505482466 - Point release to unblock customer line down due to Java certificate expiring. 

===============================================================================
v1.43.660a4315 - (Release version)
===============================================================================
    1504699916 - 2130W PSU predictive failure on S2600BP from across customers and across sites

===============================================================================
                                    CHANGES
===============================================================================
===============================================================================
v1.90.0cf6e935 - (Release version)
===============================================================================
    Add RMCP+ Cipher Suite3 Configuration in ews security configuration page. Cipher Suite 3 is disabled by default with this patch in the commit messge.
	
===============================================================================
v1.74.ee39402a - (Release version)
===============================================================================
    Update 750W DPS-750AB32A PSU fw image from 27 to 33.
    CCB2247: Q3'18 [Intel Xeon Scalable BMC]HTML5 support
    CCB2202: Q3'18 [BMC]Need log to track user/IP logins to BMC
    Q3'18 #CCB2496 provide robust method to indicate the Factory BMC and Webpost BMC at Factory BFT
    BIOS OOB updating feature.
    implement Pcie Switch Firmware update function for WRG JBOF2.
    EWS support for CCB2357.
       [CCB2357]: Provide capability to bond LAN interface for LAN failover and define which BMC channel will be primary.
    Upgrade kernel to 4.9.111.
    [CCB2357-phase 4]Provide capability to bond LAN interface for LAN failover and define which BMC channel will be primary.
     Redfish support of FW updating.

===============================================================================
v1.60.56383bef - (Release version)
===============================================================================
     Add new FW for HW rev S3 of 1100w PSU.
     [CCB 2434i]: Implement 0xD5 return code when user requests power on and system is already on
     [CCB2267] Provide interface to list MAC address of PCIe NIC card.
     Align Intel Xeon Scalable OEM Misc sub commands with Previous Generation
     Put TPM command under MTM2.
    Upgrade kernel from 4.9.79 to 4.9.98.
    CCB2201: Adding the OpenLDAP support with version 2.4.45
    Add the FW of 1600W 185mm PSU.
    [CCB 2257] add OEM command to gracefully power cycle the machine.
    Add factory build configuration.
    The new FW for 1300w PSU(Rev 0x17).
    Adds security enhancements
    Fixes RAF1000JSP CFM calculation with master node off
    CCB2166: Limits access to I2C Write commands with a special MTM Operator mode
    Adds security enhancements
    Enables Remote JTAG on S2600BT
    Redfish: Updates XML Metadata to version 2017.3
    Adds security enhancements
    Adds capability to get the number of CPU Error logs generated since last boot
    CCB2118: Adds support for new FRU VPD format in NVMe MI 1.2 drives
    Updates RAF1000JSP SDR
    Redfish: Implements OEM features for the Computer System schema
    Redfish: Adds ProcessorMetrics and MemoryMetrics data
    CCB2140: Adds sensor for absolute CPU temperature to S2600WF and S2600WFPFR
    Adds Remote Debug sensor support for WFFR
    Updates to kernel patch 4.9.78
    Adds remote JTAG authentication
    Adds security enhancements
    CCB1954: Adds PECI remote debug support
    Adds a second debug type for CPU logs
    CCB2140: Adds sensor for absolute CPU temperature to S2600BT, S2600BP, S2600ST, and S2600BP SFP+
    Adds security enhancements
    Upgrades to Linux Kernel 4.9
    Redfish: Enables RSD extension IPMI commands
    Updates PSSF222201A revision S4 firmware to 20180117 version
    Updates RAF1000JSP SDR for spreadsheet 0.95
    Increments BMC global security revision
    Redfish: Fixes Computer System PowerState reporting
    Adds Remote Debug sensor support for S2600BT
    Adds security enhancements
    Redfish: Includes NVMe Critical Warning data into Redfish drive health
    Adds SSD's Fault and rebuild status of PCIE Switch feature
    Updates voltage sensor config for RAF1000JSP
    Redfish: Updates XML to version 2017.2 (2 October 2017)
    Fixes timestamp issue for RAF1000JSP
    Restores factory defaults if an image is copied from another board
    Redfish: Implements the EthernetInterfaces for the BaseBoard NIC
    Fixes shared fan will not arise speed during BMC update for RAF1000JSP
    CCB2006: Adds WFFR BMC sensor and handler for CPU ERROR_N[0]
    Redfish: Implements remaining specified drive elements
    Redfish: Fixes Reset and Boot operations
    Updates SDR for RAF1000JSP
    Redfish: Improves Drive Schema to correctly report HSBP and slot
    Redfish: Implements HDD IndicatorLED status for Redfish

===============================================================================
v1.43.91f76955 - (Release version)
===============================================================================
    CCB2183: Changes immediate power off to power button override instead of PCH command
    Adds Fan Fault LED support for RAF1000JSP
    Adds support for UART break over SOL
    Adds option to print date/time timestamp on BMC serial logs
    Fixes an I2C master-slave switch bug
    Enables Redfish access for RAF1000JSP
    Removes ME SDR entry for RAF1000JSP

