=============================================================================
    Intel(R) Server Platform S2600WF FRU/SDR Update Release Notes
=============================================================================

INTEL(R) Server Boards and Systems 
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

=============================================================================

DATE:       December 10, 2021

TO:         Intel(R) Server Platform S2600WF customers

SUBJECT:    IBMC(R) FRU/SDR update package S2600WF_2.03 FRUSDR release notes

=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (c) 2021 Intel Corporation.

=============================================================================
                      ABOUT THIS RELEASE PACKAGE
=============================================================================

SDR file version:                   2.03

SDR data based on system/thermal team SDR spreadsheet:
    WFP FSC SDR config sheet - rev36 110819.xlsm

FRUSDR Tools: FRUSDR_V14_1_Build18_AllOS.zip

=============================================================================
	     SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- S2600WF baseboard.

- BMC FW 2.42 or later

- Front Panel, Hot-swap backplane, and Baseboard FRU data must be available
  for chassis auto-detection to succeed.

=============================================================================
                      IMPORTANT INSTALLATION NOTES
=============================================================================

NOTE: If you updated BIOS and did not clear CMOS Ram, you should do that before
      installing this package.

  

=============================================================================
			INSTALLATION PROCEDURE
=============================================================================

1. Ensure BMC FW release 2.42 or later is
   pre-installed before attempting this FRU/SDR update.

2. Copy all of the files and directories of this zip file
   to a USB key, hard disk drive or floppy drive.

3. Execute the following script to bring up the main FRU/SDR load menu:

     updS2600WF.nsh

4. Select Option 1 to do the SDR update.

5. Answer the prompts, and the SDRs will be loaded

=============================================================================
                           KNOWN ISSUES/WORKAROUNDS
=============================================================================

BMC behavior might be inconsistent up to 2 minutes after loading the
firmware update.  Initially, the BMCs were manufactured with an older style,
SHA1 private key.  This release causes the BMC to update its keys at first power
on, and correct some known issues.  This process takes about 2 minutes the first
time it is run, and will lead to inconsistent behavior immediately following a
firmware update.  Waiting for 2 minutes will allow the BMC procedure to complete
successfully.  Once this is successful, you will not see this issue again.

S2600WF power on boards came with no FRU programmed, which causes fru
loading to fail.  You must load an intial FRU manually before the FRUSDR package
can successfully load a fru.  This is done with the /fru flag on frusdr.efi

Processor DTS sensors appear to wrap around, so a clamp of -15 is imposed to
work around issue

=============================================================================
                           ISSUES FIXED
=============================================================================
Version will change to match BMC firmware.  Other changes noted below:
2.03
- HSD 15010443289 [Purley][BMC]wrong chassis information in frusdr
- update BIOS sensor according to BIOS EPS v1.19
- add support for WCP HSBP G97166-XXX FXX8X25S3DPBP 
- Remove the redundant character '2' of sensor string.

2.02
- update BIOS sensor number according to BIOS EPS v1.18
- remove "LAN NIC Temp" sensor from S2600WF0 and S2600WFQ
- HSD 1509288822 -(S2600WF) uses the wrong entity ID for the sensor "NVMe 1 Therm Mgn"

2.01
- CCB3059: Add 900W DC Power Supply support

2.00
- update FRUSDR utility to FRUSDR_V14_1_Build18_AllOS
- HSD 1508017146 -[S2600WF]NVMe 1 Therm Mgn reports the sensor is high, critical, and going higher state during stress testing

1.99
- HSD 2103631992 The BMC EWS WebUI copyright date still shows the 2019 year.

1.98
- HSD 2103626698 Change "Exit Air Temp" sensor clamp temperature from 4B to 46
- HSD 1507429379 Sync BIOS sensor definition as BIOS EPS v1.13 "table41. BIOS sensors and SEL data"

1.97
- Add sensor "eSPI Reg Access" for "BMC eSPI register access restriction"

1.96
- update FRUSDR utility to FRUSDR_V14_1_Build17

1.95
- Add new sensor "KCS Policy" for feature "KCS policy control mode"

1.94
- Changed the fans PWM for fan profile #3,4,5 and 6 and the Riser 1 shift profile number for 1U configurations.

1.90
- HSD 1408265820 - [WFP] R2000WF FANs increased speed to double at stand-by after upgrading to Q2 SUP BMC 1.60.56383bef.

1.73
- HSD 1506731770 - SDR record failure

1.60
- Enable "PS[x] Fan Fail" for 1600W PSU
- Enable median filter for hidden voltage sensors.

1.55
- Add support for 1600W psu.

1.52
- Updates to version 30 of FSC spreadsheet

1.51
- Adds remote PECI support to the Remote Debug sensor
- HSD 2103619689 - Includes NVMe sensors for 12*3.5 HSBP
- HSD 2202506519 - Updates CPU name in master.cfg display

1.48
- Adds processor absolute temp sensor
- Removes unused UPI Fatal sensors

1.38
- Updates to version 29 of FSC spreadsheet

1.37
- CCB1904 Adds support for Riser 3 temp sensor detection

1.35
- Adds FW Security sensor

1.22
- HSD 2103617663 - Updates Storage FP Temp to 78C to match Grantley

1.00:
- First release

=============================================================================
                           FEATURES ADDED
=============================================================================

1.00:
- First release

[END OF RELEASE NOTES]